(module "ESP32WROOM32EN8" (layer F.Cu)
  (descr "ESP32-WROOM-32E-N8-3")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference IC** (at 0.000 0.25) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0.000 0.25) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "ESP32WROOM32EN8" (at 0.000 0.25) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -9 12.75) (end 9 12.75) (layer F.Fab) (width 0.1))
  (fp_line (start 9 12.75) (end 9 -12.75) (layer F.Fab) (width 0.1))
  (fp_line (start 9 -12.75) (end -9 -12.75) (layer F.Fab) (width 0.1))
  (fp_line (start -9 -12.75) (end -9 12.75) (layer F.Fab) (width 0.1))
  (fp_line (start -10.5 -13.75) (end 10.5 -13.75) (layer F.CrtYd) (width 0.1))
  (fp_line (start 10.5 -13.75) (end 10.5 14.25) (layer F.CrtYd) (width 0.1))
  (fp_line (start 10.5 14.25) (end -10.5 14.25) (layer F.CrtYd) (width 0.1))
  (fp_line (start -10.5 14.25) (end -10.5 -13.75) (layer F.CrtYd) (width 0.1))
  (fp_line (start -9 -6) (end -9 -12.75) (layer F.SilkS) (width 0.2))
  (fp_line (start -9 -12.75) (end 9 -12.75) (layer F.SilkS) (width 0.2))
  (fp_line (start 9 -12.75) (end 9 -6) (layer F.SilkS) (width 0.2))
  (fp_line (start 9 12) (end 9 12.75) (layer F.SilkS) (width 0.2))
  (fp_line (start 9 12.75) (end 6.5 12.75) (layer F.SilkS) (width 0.2))
  (fp_line (start -6.5 12.75) (end -9 12.75) (layer F.SilkS) (width 0.2))
  (fp_line (start -9 12.75) (end -9 12) (layer F.SilkS) (width 0.2))
  (fp_line (start -10.1 -5.26) (end -10.1 -5.26) (layer F.SilkS) (width 0.1))
  (fp_line (start -10 -5.26) (end -10 -5.26) (layer F.SilkS) (width 0.1))
  (fp_arc (start -10.05 -5.26) (end -10.100 -5.26) (angle -180) (layer F.SilkS) (width 0.1))
  (fp_arc (start -10.05 -5.26) (end -10.000 -5.26) (angle -180) (layer F.SilkS) (width 0.1))
  (pad 1 smd rect (at -8.750 -5.26 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -8.750 -3.99 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -8.750 -2.72 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -8.750 -1.45 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -8.750 -0.18 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -8.750 1.09 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -8.750 2.36 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -8.750 3.63 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -8.750 4.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -8.750 6.17 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -8.750 7.44 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -8.750 8.71 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -8.750 9.98 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -8.750 11.25 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -5.715 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -4.445 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -3.175 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.905 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -0.635 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 0.635 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 1.905 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 3.175 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 4.445 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 5.715 12.5 0) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 8.750 11.25 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 8.750 9.98 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 8.750 8.71 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 8.750 7.44 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 8.750 6.17 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 8.750 4.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 8.750 3.63 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 8.750 2.36 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 8.750 1.09 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 8.750 -0.18 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 8.750 -1.45 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 8.750 -2.72 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 8.750 -3.99 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 8.750 -5.26 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at -2.900 1.06 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at -2.900 2.46 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at -2.900 3.86 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at -1.500 3.86 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 43 smd rect (at -0.100 3.86 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 44 smd rect (at -0.100 2.46 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 45 smd rect (at -0.100 1.06 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 46 smd rect (at -1.500 1.06 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (pad 47 smd rect (at -1.500 2.46 90) (size 0.900 0.900) (layers F.Cu F.Paste F.Mask))
  (model ESP32-WROOM-32E-N8.stp
    (at (xyz 0 0 0.001181102335805))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
