(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "5V")
	(net 2 "GND")
	(net 3 "3.3V")
	(net 4 "EN")
	(net 5 "24V GND")
	(net 6 "Net-(C_I1-Pad1)")
	(net 7 "Net-(D_I1-K)")
	(net 8 "Net-(D_I2-K)")
	(net 9 "Net-(C_I4-Pad1)")
	(net 10 "Net-(D_I3-K)")
	(net 11 "Net-(C_I6-Pad1)")
	(net 12 "Net-(D_I4-K)")
	(net 13 "Net-(C_I8-Pad1)")
	(net 14 "Net-(D_I5-K)")
	(net 15 "Net-(C_I10-Pad1)")
	(net 16 "Net-(D_I6-K)")
	(net 17 "Net-(C_I12-Pad1)")
	(net 18 "Net-(D_I7-K)")
	(net 19 "Net-(C_I14-Pad1)")
	(net 20 "Net-(D_I8-K)")
	(net 21 "Net-(C_I16-Pad1)")
	(net 22 "Net-(D_I9-K)")
	(net 23 "Net-(D_I10-K)")
	(net 24 "Net-(D_I11-K)")
	(net 25 "Net-(D_I12-K)")
	(net 26 "Net-(C_I21-Pad1)")
	(net 27 "Net-(C_I22-Pad1)")
	(net 28 "Net-(C_I23-Pad1)")
	(net 29 "Net-(C_I24-Pad1)")
	(net 30 "Net-(D_I13-K)")
	(net 31 "Net-(D_I14-K)")
	(net 32 "Net-(D_I15-K)")
	(net 33 "Net-(D_I16-K)")
	(net 34 "Net-(C_I29-Pad1)")
	(net 35 "Net-(C_I30-Pad1)")
	(net 36 "Net-(C_I31-Pad1)")
	(net 37 "Net-(C_I32-Pad1)")
	(net 38 "Net-(D2-A)")
	(net 39 "Net-(D3-A)")
	(net 40 "Net-(D4-A)")
	(net 41 "Net-(D5-A)")
	(net 42 "Net-(D10-A)")
	(net 43 "Net-(D11-A)")
	(net 44 "Net-(D12-A)")
	(net 45 "Net-(D13-A)")
	(net 46 "Net-(D14-A)")
	(net 47 "Net-(D15-A)")
	(net 48 "Net-(D16-A)")
	(net 49 "Net-(D17-A)")
	(net 50 "Net-(D18-A)")
	(net 51 "Net-(D19-A)")
	(net 52 "Net-(D20-A)")
	(net 53 "Net-(D21-A)")
	(net 54 "OUT1")
	(net 55 "OUT8")
	(net 56 "/PLC2 GPO/Relays/Relay8_A2")
	(net 57 "OUT3")
	(net 58 "/PLC2 GPO/Relays/Relay6_A2")
	(net 59 "OUT2")
	(net 60 "OUT5")
	(net 61 "/PLC2 GPO/Relays/Relay7_A2")
	(net 62 "/PLC2 GPO/Relays/Relay5_A2")
	(net 63 "/PLC2 GPO/Relays/Relay2_A2")
	(net 64 "OUT6")
	(net 65 "/PLC2 GPO/Relays/Relay1_A2")
	(net 66 "OUT7")
	(net 67 "/PLC2 GPO/Relays/Relay4_A2")
	(net 68 "/PLC2 GPO/Relays/Relay3_A2")
	(net 69 "24 IN")
	(net 70 "OUT4")
	(net 71 "TCK")
	(net 72 "IN4")
	(net 73 "unconnected-(IC3-IO35-Pad28)")
	(net 74 "TDO")
	(net 75 "TXD0")
	(net 76 "D-")
	(net 77 "IN10")
	(net 78 "RXD0")
	(net 79 "CAN Rx")
	(net 80 "CAN Tx")
	(net 81 "IN16")
	(net 82 "IN13")
	(net 83 "IN5")
	(net 84 "IN11")
	(net 85 "unconnected-(IC3-IO36-Pad29)")
	(net 86 "IN6")
	(net 87 "/PSRAM")
	(net 88 "IN3")
	(net 89 "IN9")
	(net 90 "IN12")
	(net 91 "GPIO0")
	(net 92 "TDI")
	(net 93 "IN2")
	(net 94 "IN1")
	(net 95 "TMS")
	(net 96 "D+")
	(net 97 "IN14")
	(net 98 "IN15")
	(net 99 "Net-(J1-CC1)")
	(net 100 "Net-(J1-D--PadA7)")
	(net 101 "unconnected-(J1-SBU1-PadA8)")
	(net 102 "Net-(J1-CC2)")
	(net 103 "Net-(J1-D+-PadA6)")
	(net 104 "unconnected-(J1-SBU2-PadB8)")
	(net 105 "Net-(J3-Pin_2)")
	(net 106 "Net-(J3-Pin_1)")
	(net 107 "unconnected-(J4-Pad9)")
	(net 108 "unconnected-(J4-Pad1)")
	(net 109 "unconnected-(J4-Pad5)")
	(net 110 "CANH")
	(net 111 "unconnected-(J4-Pad4)")
	(net 112 "unconnected-(J4-Pad6)")
	(net 113 "unconnected-(J4-Pad8)")
	(net 114 "CANL")
	(net 115 "Net-(J6-Pin_1)")
	(net 116 "Net-(J6-Pin_2)")
	(net 117 "unconnected-(J7-Pin_10-Pad10)")
	(net 118 "Net-(J8-Pin_2)")
	(net 119 "Net-(J8-Pin_1)")
	(net 120 "Net-(J9-Pin_2)")
	(net 121 "Net-(J9-Pin_1)")
	(net 122 "Net-(J10-Pin_2)")
	(net 123 "Net-(J10-Pin_1)")
	(net 124 "Net-(J11-Pin_1)")
	(net 125 "Net-(J11-Pin_2)")
	(net 126 "Net-(J12-Pin_2)")
	(net 127 "Net-(J12-Pin_1)")
	(net 128 "Net-(J13-Pin_1)")
	(net 129 "Net-(J13-Pin_2)")
	(net 130 "Net-(JP2-A)")
	(net 131 "unconnected-(K2-Pad12)")
	(net 132 "unconnected-(K3-Pad12)")
	(net 133 "unconnected-(K4-Pad12)")
	(net 134 "unconnected-(K5-Pad12)")
	(net 135 "unconnected-(K6-Pad12)")
	(net 136 "unconnected-(K7-Pad12)")
	(net 137 "unconnected-(K8-Pad12)")
	(net 138 "unconnected-(K9-Pad12)")
	(net 139 "/PLC2 GPI/O7")
	(net 140 "/PLC2 GPI/O8")
	(net 141 "unconnected-(U1-VBUS-Pad5)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0062dc06-f7b4-4f62-8b4d-f9b35ff319a2")
		(at 157.33 114.595)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I73"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b75e3053-efbc-48aa-8c2d-87dcd82ac286")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "47a03974-dd95-4007-a96f-03673cf68b79")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "93c90c5e-fb0c-4d8f-b767-0ff7267ee728")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd902f7a-6d84-45e3-a492-fa50569cd4b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/37276a6e-de04-4dcc-8d23-c00616bff3ee")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7abee44-aec6-46bb-87d4-d61c4979871a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d5a4ea1-4437-4d50-8289-4ed4ce58fab3")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "996929f1-0567-471e-addf-6d2dff89cde9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d93f711-1888-4c9d-90ae-28994fd2eaaa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "863e8ce7-1562-4d11-83f5-347cf21bb227")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5098edfc-63e1-432f-b873-7fe72eccd22e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "202e0b85-a433-4ea5-9005-65d72f756420")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ba6a8b9-b4c1-4373-9499-2a32fd447366")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf17232-501f-4be7-bc2d-d77740499171")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f586d4c-6362-4e12-b851-0509601c3616")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3bd8a817-ce83-4da5-94c8-cea110b0a23b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(D_I15-K)")
			(pintype "passive")
			(uuid "fd3eaab2-69fd-4935-be8a-a4b7ea6d1776")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 52 "Net-(D20-A)")
			(pintype "passive")
			(uuid "e984e2f0-352c-4942-aecc-856618ee755b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0466d866-81cf-4e76-8f30-1e0dc4b71e8e")
		(at 148.765 44.96)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "469cf0e0-5393-4f2e-9c0f-34e1485a1bf0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "8df7feca-9871-49f9-af42-d2a65a848359")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "66f27293-1f32-4421-8808-3d4dc0ff96c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2183c46-870d-44bd-82aa-13976e253f59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4fa642e-830c-44ad-ae3a-8bdd020465ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/cda83219-581f-4e07-8c48-c6f5e7e47983")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73ebfcf8-ad9f-4578-97c0-ac926c361f95")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "153e2127-fa9d-47e2-b22c-19d70e32fd34")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5fdbf8a-be7b-4ede-9dd1-0ccb96fecd0a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bb8e44f-8c42-4c69-9e29-7f028b5047dc")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2250f7cd-1534-4fae-9f56-01d6cd911e00")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec9f9e0c-7ee3-45e9-9b46-1245e15bd13f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b1d3f650-604d-4795-8cf3-56638e11047c")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "376144cd-c81e-46c5-9680-c3749fcda9c7")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b80c0d28-3192-4f86-8597-2f94da81220a")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4baf3088-f45b-4652-b34b-bd1c8f7023e0")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2a76e25-5787-4323-a7e1-a98ce4e2eac9")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96ff522e-a67e-4f79-ac75-2dbb5c1a8b89")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "25b539de-e7a9-4a9a-81d1-b6dd3a9fe1ca")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "cf6626a9-ef88-41f7-88ba-3a30bb2bbb17")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 42 "Net-(D10-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "cccb1f0b-0d19-449c-a87e-1e29bdb2b30b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "051c1286-4613-4523-8fed-b77af537d965")
		(at 143.08 129.345)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I54"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "da89fe3f-6df5-4abd-add4-1130f981b6f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f6a0ffbe-cc74-4e58-a2b5-a3a2c9fa7aaf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7b6436d-8187-4669-831f-7f34fda6b25f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f56c09b-25b1-40bf-a19c-349b4f275f89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/995f682f-c12a-42d8-a116-989e75feb021")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e93d1cdf-5248-4747-ba88-9530543bb79e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87acc34a-d2f8-43bf-83f9-d03434a7fbad")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d36a763a-1bc2-4cfd-8649-e4c396a51bf5")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7a779b3-ce00-4b21-b25e-d8d5d06e0fdf")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2a5f239-fa75-4ab2-9f98-4ea5222add23")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b96b5e14-4ea0-4d4a-9b4b-8b08c6382267")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52f90938-c7e7-4ac8-826b-cd03228368a4")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3690ba40-6c7d-4735-9d09-71cf878b082e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2f7413a-91f5-4336-adf8-d310fb66ef8a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a5f2549-aeff-41e8-8d0b-65138cdb8b0f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bed67851-677c-4f93-9f18-56b1da1e0ac1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(D_I10-K)")
			(pintype "passive")
			(uuid "f68ea242-ffee-44ec-b23c-36c86f3dd66e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(C_I22-Pad1)")
			(pintype "passive")
			(uuid "85e3e941-bb9a-4a22-9712-f8ea7568eaf4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "06a3768b-3edf-4c2e-990e-e4849bd57559")
		(at 141.175 39.63)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "cd5d588c-0723-42d7-9e00-28260cc4a3e0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "9a476fd0-7da1-4019-8d25-99e56403f669")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bcb0cd17-4fe3-496f-83e2-3652adef8783")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "87f35861-9e8c-4fd7-b494-9c1b98fc29ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/4cf7fd6d-a876-4525-ba9b-421ef5dde938")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3eceefc-f4b9-4a54-b02e-61a53881443b")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f854f53b-297c-4816-8bdc-06f4df61bfe7")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4aba9805-b5ff-4d3d-a9dd-5e5a838c4840")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71212f28-2057-4c87-b869-a2643c7b53a2")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91770845-b3ae-4d8e-a09f-eccd6b94d6dc")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f61fa80d-e215-4a5f-b92f-8d0fae1e1a3a")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de501a5d-4f9a-43c6-9c13-561988ff7f06")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47fc6e58-1d3a-4881-93bc-df1d48623f27")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8a2ee1a-ef49-4530-8492-8c3e170eb652")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "109dff27-cabd-4402-9921-8b72f9f64311")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5e3f5f3-dc77-4eb4-9949-d9ac9ae4fdea")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "243d5a82-e446-4825-80d0-e540343c9526")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b630e0f-ddf3-482d-bc36-fd25e0e1844b")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdc4067d-5800-42e4-acd3-8ade1cba0c96")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9712cf0e-61f5-48db-a330-ccdd3452c042")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "163822a8-f4ff-431e-85d7-ffc42eb92a00")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd766c3e-ad5f-439a-a43a-f0d3566303f0")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b889a6ba-ee45-49ad-9c87-535890cc3045")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "fc5e43b4-4af1-4a8f-aa17-b0a83655478d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 10 "Net-(D_I3-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "1c0914f7-310f-4565-8f2e-18a21f598f5d")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "cd40bd2a-e760-44d0-be98-e69c493dd732")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "07ba1ab0-422d-478a-98ea-f57b63a541b9")
		(at 158.35 38.805)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I9"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "591c8242-b289-441a-8118-32595c775d27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c94d09d3-c0bf-4796-8faf-bafd7cdee493")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3dcc645-845a-4729-9386-16d18def2ad5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "acaf23fe-1470-4da9-96c8-d54344940634")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/ca5ea6cc-59ed-4793-966f-a02947bbf9af")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cec57782-2fbe-4e57-b358-99e56c284f9b")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9a19e91-d412-4895-bea8-f5be09316675")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2007ee73-35f7-44d6-98d4-2d7878e2a8ef")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b6096c8-159b-43ea-98ed-0643d9d8333b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf6f1cdb-ef37-4a04-a3ea-e62a8b53290f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fc86800-aec2-4b60-99c7-b90fae242919")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "541248a8-ee12-46c0-b991-ca47c54bd7a3")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63ffbde4-862b-4767-9d90-3def04e42850")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "121e79f8-4923-44a6-add4-1b98ec910104")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99ebd3ee-3f65-4e7e-842b-5c70f4c46d20")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c27eaaaa-7366-4da8-b508-9711c134a3b5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "Net-(D_I5-K)")
			(pintype "passive")
			(uuid "86737c3b-d71a-4a84-a215-e40fca0e3e75")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "2b842ec5-56eb-46b2-a74e-0a5542954fdf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "085ba8af-51d9-4d8f-a687-da2145d046f6")
		(at 157.33 77.175)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I39"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "02bd0baf-2b88-4cac-9ca6-a7f57a429e26")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b90ec56b-f153-4052-aeb0-6d1995c9b315")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bb3bf10-b336-4714-88e1-1622498dd79a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c9991ac-e885-4b9e-ac10-02b43f110eea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/6e75ab72-ca51-48bf-9c2c-d91718bc9e9d")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b6944e4-f300-4b27-b22a-522f65f9ba62")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2be852ae-2be2-4e67-ada6-b692ce989459")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23160d63-f702-4904-a1a8-d48df62c8424")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2fb1dd44-b377-4b3d-b9b1-e2b834ff2f01")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a449df54-5cc2-44c6-8b7c-0ffc46e9deee")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f329fe8e-9039-4481-b8cc-c69ac2ea9980")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5397d444-9b22-486e-a32a-7f9a7309652d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68108c81-b04b-4ab8-9f31-78264fc8a053")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ef7d6d8-2f91-4b5c-bc49-a73bd02672ea")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d56409c6-97f8-4d47-b276-a99bf18d0342")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e79bd01f-a0a0-4085-bd63-be8143e7e674")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(D_I8-K)")
			(pintype "passive")
			(uuid "62de548d-7296-428d-b17c-22568184c85b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 21 "Net-(C_I16-Pad1)")
			(pintype "passive")
			(uuid "521bc64e-5c6d-40ca-9432-67e04965055d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "0bc1d964-cdde-4c97-b4d0-386b1cfc9320")
		(at 126.76 59.885)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U8"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "53f7c6a8-212a-4600-b7e5-e97c5717e921")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "6a785910-4f95-4256-bfce-738529a6b761")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d19c5f5-3a0e-4eef-abf2-820634a30328")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ed3bd9c-1802-454b-86bf-2b1612fed3cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/501e3c64-132e-4122-b9e7-463971556b1b")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd2fb963-b335-4052-81c4-8f43aa92aae6")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aff4dfae-3763-481d-97a5-85308ee08edb")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1cbc87d7-7b96-4757-a9ee-8c01179de90d")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "735b413e-65f0-4938-978a-6c0b68fb63ac")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b08467c-add6-43e8-a75a-fa22f0619cc0")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b41cdbda-1576-4ac6-9631-e2177b8ecb83")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "9529e8fa-f02f-4e80-8c43-f709bbac4419")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f5e1d14-35fd-4a96-87b7-768178aba193")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7be69dc2-595f-462c-a5a1-44c19673b5f7")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9253f4b-97b9-417e-b01b-87e936018aaa")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08c8befb-5a25-44bb-bb80-ff13114cb3b2")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd7239f3-c074-449b-afb1-ffed07e8ecec")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "3912ed4c-ce78-4342-b983-2f6c0cf44ee0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 6 "Net-(C_I1-Pad1)")
			(pintype "passive")
			(uuid "9b49eda4-6050-452d-a397-d8ca7a5e4301")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "23df71e5-e01a-44a5-b1d6-deeb67f36737")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "6b2aa05e-bee3-41a9-a33b-2b6464d85c6c")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "IN1")
			(pintype "passive")
			(uuid "b60467e5-e64e-49d5-bedb-11066323666c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0d051df2-80aa-4447-af17-282a3340ed0b")
		(at 138.33 114.595)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I41"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "508c893d-6961-459a-abfe-59079bd61315")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "bb856b67-905d-4c47-aa69-d117416eccac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "186a95bd-f4d9-4ef7-b924-ea847efd90d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f6e35de4-b537-45f7-b7a0-0ff9d8d2c1fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/c83a2dd7-0412-4860-baca-aed95a700ba8")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c1c8eb3-6b45-4265-98d7-131e8cb03614")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "319d58c8-cb11-4f6f-a66d-7b62db68db61")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c60aaca-15ac-45f2-8151-8bed3ff8c821")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ad966533-f96b-4a3a-8ce4-5a972020ebb9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56b91d50-3166-49f5-bc48-bcaaf2c581b0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "082c215c-5418-4c20-8fb7-e3d658d338f4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9da73a2-2df2-4296-8c07-0a69b067a3ee")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8048dca5-d9b6-45fa-bbee-85e8e8ceaea3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae721e1b-17ac-4b2d-aa08-01824fe8a352")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6dd38db7-5380-4f3d-8feb-fe6a6d783930")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "28030d13-bd44-4575-b04d-d793897b3127")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "43ddec67-8e20-4880-9320-2511eba23abb")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(D_I9-K)")
			(pintype "passive")
			(uuid "cc1d67e3-75a6-4d47-b2aa-8d415040869b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "100cfbb9-a495-4fa4-ab2c-0b3378d069ef")
		(at 147.83 126.395)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I61"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f132994c-fa31-4c26-9da6-fe2535e6f4f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "00379323-97d1-41fa-9291-e4a5b0f4550b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3446e3e-dfd2-462b-a0e4-bb966d6484ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2ab748e-4300-4800-8e0d-c666cf25d16a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/2de4869f-1d70-4754-9aea-70fdc0f084e3")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e10a2d9-ca80-426f-b77f-ac81815b2113")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16b99d33-5a3e-4618-a636-c499ae7c360e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6ea0de9-6913-49e8-bdf5-53f2407aa529")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87a52a9d-f8af-4779-902e-13b11b87f39a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28c02660-b710-4cb8-8006-ca3e444f075b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a46fbc4-e3ca-4d78-b401-7f05b6d96e53")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85e182d4-8a33-4a40-ae34-bcb78d3735fd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc472426-8d7f-4d26-883a-a616df25aa92")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4b313f7-f296-4a80-b076-ea8412860f29")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3da9dc47-5156-415d-a3f4-d6966fe9321d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b6c1471c-1dd4-4492-ba64-3747287314f8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "514aa1d7-e371-49fc-8d91-823c190f5af6")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(D_I13-K)")
			(pintype "passive")
			(uuid "4454296e-eb0c-4401-b5dc-8e952dafd391")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "10231c4d-3f75-43df-a070-3f94c0fd0343")
		(at 153.54 32.785)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "1ac7f0d2-fd86-4363-89d4-089dda7cec76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c4277d64-482f-4041-a123-e03e2a1cea75")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "26838496-e2b2-416d-9977-b01ec04c5826")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac164ca5-7a84-45ad-a959-95ed3d5b935c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/aa5c8b2e-cd3f-453c-a41d-5da334bd5c9a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd47e91e-a5f8-4ffa-bc6f-86b5dcf4ad23")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "458695ec-b0e2-4a63-bca0-b3419bd3c89b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12c8ef83-ba3e-4056-9dcf-14197d1666ee")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "75c97940-3fa6-4f43-ac68-1474aec59347")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "75be2da8-f4f1-4953-83bc-e145c4312cb1")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6ab1dd8-4846-4e58-a1df-bfc2d8a4925a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9afc831-9d7b-4f81-a8bb-348fb140170f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f206d28-7859-44fd-b5d2-59ea58827656")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "774f432c-a379-45e0-bc9c-07f5a86d2684")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2d7b852-6d7b-4071-a29f-caa06c20c730")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "92b2623d-687f-4864-939f-fe29d9dec99b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(C_I1-Pad1)")
			(pintype "passive")
			(uuid "e6716fb3-3663-4b38-a815-a58383755f72")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "227d77c7-0819-46da-abd0-fd686072435f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "107248be-5e42-4c62-b0fc-cb97fb76135f")
		(at 218.5 140 180)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J6"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "945ff9df-dbdb-42b0-a470-d9e558baf8b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "aaa9ba43-1722-4771-92ce-f568a4782e4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0454b223-b69e-46cd-baad-9286b03a9ad7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e27a6425-47ea-4fec-b0d9-14208cb2d468")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/bbf7bd76-e0af-4ff4-ad1f-e9ac86ac676d")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8539ac10-0358-47d0-9c54-97158953d260")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29bbb823-db01-4a61-aada-a79eb2c094ff")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3cc0c4a-2e23-454e-b7b8-af334765a179")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cce5120-6c38-4701-a3de-fa3b7ad8b73e")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2db74141-37a7-4083-8c9b-700458042a91")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f5d18a0-ebf0-43db-8938-5c616a3828db")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc11859e-d6b6-493b-aefc-d4d6fdfb4cc9")
		)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cac67c81-7dc8-48b2-96de-20d2e0c9cbe0")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "a1e449c5-d7bd-4a47-97f8-fe83327c92ac")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ae31610-1f7e-41e9-920a-878ec1964368")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ff2354b-2a4e-4011-9306-9384a9f0276c")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4249b565-0ca3-456b-99cf-7d27d60f9193")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25ced88c-bf6a-4745-b964-07dd63fc77e8")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e7e1fc2-cc65-4a21-aaf2-26ca94b695e3")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a551462-a446-4473-946b-5324fcad8f4b")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06af870f-0627-4516-8c28-034573d44173")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "214b930c-ba5a-4163-aaab-a62478785672")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37e6a3d5-9e95-4561-bea7-985c296ffdd4")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efb3a008-d8dd-4156-80be-6deabb47e502")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48c036de-a1be-41f1-9daf-cc5ddda44c47")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c719b88b-bb78-4353-8dda-5bded21a79a7")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d01ef67-430b-4cbc-87c1-e3ea58c5db13")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c8ddffa-f874-4c09-8b08-7f423178a654")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e7986f3-806f-43b4-aead-5986bf9bafde")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0be239bf-7c7c-4b6e-ac54-22e9ea71e8c6")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "66031c1a-6729-4c89-8d60-7e2d7bb04353")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d25b30d2-aca2-4afd-812f-4dcb415c6c28")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "609e89a3-ef76-47ec-bbaf-89bbbb6b1e94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 115 "Net-(J6-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c066495e-238f-4cee-a5c7-c01f4636cf8f")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(J6-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "e9a3af25-4ff0-47d5-9386-2f624bfd4fc6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "11b6d654-9a17-4ba9-9573-2c0ca1132e2e")
		(at 95.16 44.22)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J12"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "7c3f8acf-aa88-4e8b-bb1c-1187f8045764")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "03bf952a-86da-4609-a460-9b0e755df990")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "81a12f84-1b55-44af-96a2-50616445e0ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f2e8e08-bfb8-4a0e-acc3-edc9871f7b72")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/48894b03-3e75-4fe1-b768-4cabc214ff28")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "899409be-5da7-4290-ac0f-096631b44d53")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f08daacf-d03f-4f27-bd00-d7895959fe1b")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d00aee32-19d9-4945-9ff8-19d4845fa33c")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c613feaf-2d03-4aa7-9752-71da2400e686")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be9eec65-cc95-4256-8d61-7008213cdc93")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a1534e1-1f9b-4278-8b2b-3ffe13eab492")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1957c59f-7e06-478a-8ea1-efb60c76008d")
		)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68de208d-7709-4841-80d6-52895977fd81")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "1f6af25c-daea-4383-9700-ac8a0f302f0e")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ae94e4e-e3ca-4f9c-89f2-cb920d176a6b")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d459e59-956f-4bd7-988f-b4cb47e7f50a")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b90fe6d-4f1a-4c61-912d-2f61ff1f75c7")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c03b636-af32-4680-b9ae-4e0f4dbd35d6")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1832f740-3627-42bb-b802-2ce1e1bed903")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fc16168-3ef8-4416-ba1f-6c7633611baa")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0bfb193-ba9e-4fdd-8630-d78beb0b2460")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbf1b1af-affc-4048-a265-434826cbb943")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5467309e-7e2e-4cfe-83db-419142e3ac8f")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1511a5b-8eec-409f-87c1-77805ecb5f24")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21e811ec-a39c-4cf8-aefa-28effb75735f")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36e1cb38-ea9f-4bc3-9791-7527e69bbaef")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8701ab9-0281-4211-b77a-cf1de22f4adb")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b64e8afe-d92e-4407-a0f7-8969f47e868e")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91a4c858-a0f4-4ce9-9a0c-f0bfbd5cf78c")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8330c537-9165-49e5-922c-c7d4ea9c6198")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f9a4e642-9cc0-43c6-b8b3-b4c66885398f")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "49f00588-56fb-4cf7-bfef-c76e119138e2")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "8e388d70-6ea4-4627-8626-ccfaae21f8ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 127 "Net-(J12-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7d62c935-d79f-4d16-a1b9-fddf1baf8443")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(J12-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "21b96c32-772f-4a36-b885-715ae64d3b59")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "12635dd8-61c7-438b-b6de-2987cf9e4d88")
		(at 126.76 66.525)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U9"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "e7d3416a-ac77-4874-8ec0-46bf9f96170e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "09d2a1dd-9651-41a1-8022-3229d465fa8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f626a01-4f0c-4200-956c-8b1c66f2d5be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8fd308e8-bf19-426d-a050-3b243b77179a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/34778059-2c34-4f73-a87b-5f4e9da762dd")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8fd7ae3-5405-4764-9e99-93df1e8ba45f")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1bdc810a-db27-4154-85c3-10a1de4e45df")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "323f7fd7-c750-4872-bc16-b799b09d0c3a")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad47f94e-d91e-47cc-aa1f-4ccddec1f5c7")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7017ab6-78a6-45a6-b8f9-021d41130b75")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8933edce-a64d-422c-b805-0e9333dbac1b")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c9131b5f-b21a-4207-89ba-5df6a68ea46b")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ac992bf-98f4-41d6-9711-aeb8ff7af26d")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba3bedd0-57e9-4932-9b96-96b933443cd6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d87d83b-275b-4ffa-ab30-ede912593cb7")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a23250f-c751-47e8-afb0-db6ea52a1d4e")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f96e9ad-9624-4cf3-b50e-a9802c291ed5")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "e5fabdf1-431e-49b0-8088-f2c6fe676593")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 17 "Net-(C_I12-Pad1)")
			(pintype "passive")
			(uuid "d427ceca-e11b-4175-9e9b-854874cd07c2")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "566d42a9-79da-48eb-8fc5-1897510ff567")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "dd2bcd6a-f8ba-49fd-bc52-4c0a244930d8")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "IN6")
			(pintype "passive")
			(uuid "aaf5f142-5d49-4c1e-9f27-1db6260b16b3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "1309e823-b208-42d2-94f8-28e94bc75173")
		(at 118.08 35.405)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J10"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "c91446f1-f44e-474f-8091-3d0add97e7ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "e6456bbe-ec2c-442c-ae74-9758bef940bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8bc3b0e3-443a-429c-81bc-95360bba6412")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f73fee3e-0219-4a25-9e59-edf5b62acd18")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/ac92d996-a832-41f5-8632-881612454455")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdffc9f1-4099-477d-903b-9877456266bf")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "744ce9c5-7215-4221-9c2b-78d8efe1bd81")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7c58d17-2755-4976-b2f2-df247e9f144b")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6407e91f-2c03-4575-84f8-007228b08c46")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04641ea6-1a7b-48c9-b3a2-693e44e32f88")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cee56d7-d324-4ba2-adb9-2585bfa1d66a")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a39f946-9190-414f-92d7-840ba293f5b5")
		)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe15103c-20e6-43b5-9417-3c464d91f7a2")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "e4133418-2ee1-4e65-a2af-ffac1113c2bc")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7946def6-ff97-4294-a4af-5df28339bf8d")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c23078d-bf1d-401f-996b-87b38d408f95")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3154c2fe-94a5-49f0-b7f8-346e13d00b6a")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30fe2b04-4c0c-4e60-99f4-286faac9b539")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45abdf18-fb7d-4b56-bc48-fd50b7dc70a2")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "38725c68-f17b-478a-9b2c-159a50bff7df")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53d80538-7044-4267-ae01-cd01a10e23be")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "503b40e8-0f98-46e6-9e81-f41e12506328")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb0c9375-dee0-4254-b864-d4417ef9520f")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0348bbd-7d21-4e93-b6e8-8c029bafc6b6")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e194b2a-00c1-4f75-a5c1-1204032c9aca")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4cdab75d-8467-4c84-8c9a-1a2ad3a29ac9")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51458ebb-f156-4c4f-b90c-2580b354cc34")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8285f742-3892-4e14-88bc-5f85dc992ae7")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9fa6d9c-b284-4970-8cde-c53f68a0bfce")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfd479a9-68fe-4aa6-88bd-fabc927ff025")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d22ae5a4-103a-4eae-91c8-37e60c190fc3")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6c2e1abe-24b5-4515-b6de-9079b490ef78")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "62cc366c-a116-4111-baed-848b732806d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 123 "Net-(J10-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f4c3abb4-c173-4b8c-a113-cf7aeb839272")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "Net-(J10-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "af45ed6f-642b-4631-a102-61870c135aa1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "13bd3064-9c61-43e4-adb8-3d6e84e247cb")
		(at 102.8 44.22)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J13"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "890207f5-aad0-489d-b21f-2ebc4f179515")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "f42c2783-2cbf-4c0b-9bd4-75173c4e9536")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "848f4ab7-0643-4390-8972-fccaca3fe4d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8232ab91-98d3-46f0-8314-d06717b758dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/15539969-4c09-4168-85ec-468750a07e7d")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c33dfd26-c432-43c1-8f3d-7c388b69b0d1")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04d4a8f1-284a-4836-8152-5294d04a9c3c")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ab5a09b-49b1-43ae-bc8a-f32896699954")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c541a01f-7a23-4815-bcac-01dbe303209d")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3649d038-a29a-4d5f-8bcc-b76083b90fdd")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a01a0a42-8a60-4e16-8c5e-ee6aab4891b1")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "afeff57e-200d-4348-ab4e-9bd806885b94")
		)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3195d5bd-4ea5-454c-a936-1cd5a0ef3a6e")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "6575ae4c-27dc-4056-83e7-d9213f571fd5")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fdff4aa7-7d44-4a81-b7e1-2ea34b215e35")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6dc33c2-6f7b-4db1-90bb-c1a18650b9fd")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "219da7fa-b460-45fa-93c3-b0e24cd5b975")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f631a5ac-c69d-4048-9b38-2376dd020ca8")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c72e3d6b-d5f6-49c8-9c79-f6b94ef5205e")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02df1399-54f8-4502-8f09-cd46b243ea4a")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29082a78-5741-482f-88d3-04f0a76f4581")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aed82b78-b6f6-4736-82e8-ed459336140c")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c402471e-f689-4d74-83d5-9689e83465ae")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff989e8c-bc62-42cc-afdc-91ce1d83d454")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e9297a1-9f65-4920-b8bc-58c07887b9e1")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "880629c0-5601-4939-8066-f1ff76ee855c")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e5b6247-04bc-4828-833b-50d70cafcebc")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7498fa38-1cae-4fcc-88f6-32158d7b6481")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1b05001-ce17-4671-acf4-cbed98c5ecac")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0b891ee-ee95-4dc2-9457-2ae06310b130")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "9ac86d38-ae36-4bef-8444-fe9ec8c4ef69")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "53f1b944-47a2-4c26-8067-16b3d81be066")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "1e24c9ca-5b73-4cdd-8e43-98d22828ec3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 128 "Net-(J13-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "256b0f27-8318-43bd-8029-d7b1c358abaf")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "Net-(J13-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "4c670915-764f-4e87-8d43-2f822c238430")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "13c89b0a-316a-4ac6-a9ea-1c8b3c6f4239")
		(at 152.58 135.245)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I72"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "80bd130c-893c-4dad-a9e0-9118414242a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "568fec2f-89b1-4063-a3eb-799b64c697d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "61f7318a-dca7-4609-8e31-5e6d9b7e0e96")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca599cb7-d07e-41fa-b9de-b31d69e2be0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/19875c6b-2e5b-4b25-82dc-3fae977c5af5")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3630a3c-6d64-4f4f-883c-39ba0059c176")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c41c51d-33f1-464d-ab43-f4637e372f08")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e1de2eb-0475-4e7f-9bf3-544bdd538d0d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3d4340eb-d129-49ac-91cb-dfb26995b6bb")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9239a72f-2e36-4ba0-851c-959ac1a6d0e2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "596093a7-773f-4e83-bdd3-4cbfff9d1c16")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48a09621-9a46-4837-8e1c-e06cc72107d6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b354a18a-885d-4789-90b3-5fd3a8651c2c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fffc4ea2-075e-4cc8-be7d-c7047d7db571")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "876f4ee6-c1e6-4550-b791-cc7344aba8ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3a38262b-f927-400e-a6ed-b1232e0307f0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(D_I14-K)")
			(pintype "passive")
			(uuid "333207b4-253b-44ce-9193-6e1e6275efc8")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "Net-(C_I30-Pad1)")
			(pintype "passive")
			(uuid "bc076524-f70f-43d3-8c2d-d7e72c126bb8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "14ffead4-ee21-4cb2-a37b-4637427c9708")
		(at 74.7 56.555)
		(property "Reference" "K8"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "aafbc471-bb5a-4229-a33c-ddd444794cee")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "fcef6e1b-c6fc-4dca-a5e6-a92e42e5d63c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd1b73e5-2630-4ab4-b095-991385af437b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54571fc9-092d-4726-b80b-64cefbe91378")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c83ceb4a-7c7f-4e3e-bed6-c70a21ab2a42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/10917fdd-7a3d-4c48-b9cf-58219585d06c")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68d61e3f-28c9-43f3-9c40-9b2d91698bd9")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d99da59-4c7b-40ce-9193-193eef24fd39")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17ff298b-5e4d-4209-a21e-2543820ea40a")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "773586a8-dd44-42a5-90cc-1b899e3f98e4")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "887f134d-6d0d-4c56-a6cd-a0bd04289092")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c52dc573-cd7f-4672-b166-b0c4acb8a727")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(J12-Pin_2)")
			(pintype "passive")
			(uuid "5f7d3a71-259e-46e6-8a69-84847823b34b")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "unconnected-(K8-Pad12)")
			(pintype "passive+no_connect")
			(uuid "83000d43-0112-4f08-9d3d-cd79d81b2362")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(J12-Pin_1)")
			(pintype "passive")
			(uuid "6871c57c-d89f-476f-a0ec-bbd3df969be0")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "cda9dd71-d4ca-4904-88e1-3c1766f10f6f")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/PLC2 GPO/Relays/Relay7_A2")
			(pintype "passive")
			(uuid "a188a58b-a5be-4d3b-b9e5-069ef269df88")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "1529dab2-ef48-49de-9b66-0c8ff789e0f1")
		(at 158.35 41.815)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I10"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "2f424cfa-a8d3-41d7-9a2e-87d19a267893")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "40c73919-c361-40f8-9c20-d7c3eb25617d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5db5bae0-0261-44c7-b7a4-4033d8b7890a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "00a592e6-6454-4bf9-9a97-5b8f541d9bc2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/a1d0678b-1b4d-46a7-9f9b-51c48ff5a912")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3933640-395e-4fe7-ae1c-7e5259fcdc79")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ed773d3-4b15-4902-b869-420b9e8d79ca")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50855c0b-8634-4cfa-b936-20f9e21ce27e")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93bdeb2f-fc9c-42ae-b82d-7e0d43bbbe94")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fe392ec-4b57-4f9a-9aec-f6e84e64c791")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6cc937c-86c5-481a-b5d7-3c606e834d3e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f70f9bc-2ed6-479a-b07b-32c163755a25")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ac32a7a-bed5-461b-bbc1-0d73971a1236")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1779225d-af5a-4230-aa2d-e9d417144e23")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6be18eec-5f30-4906-a72c-fa52188de3fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5bc51293-8557-4ace-a437-5a278db609a2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 15 "Net-(C_I10-Pad1)")
			(pintype "passive")
			(uuid "48d8f76b-a2ee-4aec-a04a-33e873a804c4")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "2c5545bf-5172-4fda-99ee-c1790d12bb7e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "15a79aee-a2d2-4de6-a300-64c46a81009c")
		(at 126.76 88.445)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U17"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "7edf920d-d96d-4793-8eec-024ce8385f1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "36e3d337-7ccd-4c28-a078-0d94980e0ede")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "12121109-99d8-43d2-a314-586d642c0815")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3aa75e52-71b5-4a76-8506-132e1b864c89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/99c45d8a-b186-473d-9b1c-1449a0603741")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc3ebd65-1199-4a77-a907-0e4e568053d1")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2fc9c5d1-2d12-40a0-8929-145a49f56460")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abc5360f-6ec6-4c07-a27c-23df134def02")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56f17ad6-1461-498f-ac81-4b1ae5ddb584")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7ae102a-ae9d-4f10-ae05-c7319fe032a2")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1598d607-f2c9-47e4-b1b3-faaa2ff392a9")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "20ee848a-e8a0-42a5-9706-564e14c58920")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b1bdcbb-d9cc-40b3-b93f-84e181a674e1")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e40089c8-68b2-493a-b1d0-894e4dec6e5b")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79dcc3be-3fdf-40ad-9b5d-1ab24a40dfa3")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f8973fb-6b68-4e65-bcb3-276da263698e")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d27eb754-7b8a-4651-9912-b6a406b4ceec")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "06f68dad-4684-475a-a078-fdee84c8fb9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 26 "Net-(C_I21-Pad1)")
			(pintype "passive")
			(uuid "d1debe55-87ff-4ad0-9ecb-5a27c11e5df7")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "e76d3a40-a5cb-45f2-ad92-33265f5e5844")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "748495dc-8b08-4c49-a3af-441ee2b87b2c")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "IN9")
			(pintype "passive")
			(uuid "9b6c132e-c951-4893-84c4-a60167c83754")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "16db5f91-584e-4072-86ae-104c6f3bb5be")
		(at 153.54 35.795)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "c3fe4daf-bdba-4036-abfa-c794d12c03fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "785b98aa-d8c2-4667-8a03-9f7465fc03b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c6ffe567-8ba4-4d28-bdb0-22eebf0816fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b362c0f4-47df-4d28-b36a-49f116ca32b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/81be6362-6081-479d-8063-66b282ead670")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "639162ad-20fe-4603-b159-cc8a9b2ffa57")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43b1c498-25d5-426b-aed7-46fe78cdf53e")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "527aea1e-7439-40aa-90bc-02fb31d26257")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5df8151-f3fd-468b-a920-0dc7bab6b52c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a89c331f-a80f-4cda-af0a-fbe9cd8c1b05")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99fdc577-b50c-4261-ac71-0569bd8acf68")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b7b1553-5d76-4ae0-912e-c6eeb147d8a7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab66edda-c7ef-4227-8abc-c07c048af885")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87cb2212-2135-4b41-8d20-63d83919ae7d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6742499-764b-4e34-90ea-9e3d123e3601")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "087e59e1-e8d7-4836-98a5-a592b053e89e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(D_I1-K)")
			(pintype "passive")
			(uuid "259ab513-7b9d-42ac-88fd-656c73acb43a")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "0e9fbaf3-4d0b-46d3-af91-c93b6069f295")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "177cc2c0-1487-4511-9019-2580f3e80109")
		(at 163.16 87.905)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I29"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "123a8895-c077-4a5b-a712-3cbe716e0918")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "cd435ffc-a2ea-4559-b26e-6ab6835d3c3a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fcb31626-418c-4a90-8ca2-c3797ffe4519")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "864ebb9a-186b-4e71-8a9f-9ea864db80be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/d3489d77-ee07-452a-babc-940f2786eb91")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78aa5cab-d5e0-4cbf-8b20-4f79f4cc29cb")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c32465b-e8a7-47bd-bfef-a932362c9b3f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03221ee2-277d-4504-835f-937cb7d0e954")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6727f652-5053-4d2a-94c4-ff27723dcfcf")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43efc23b-4137-4625-bd02-825989eae5df")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b6f8d94-c154-418d-a413-40289fffd937")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc37d9dd-7ebe-4ffe-986b-be8d23c04a13")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb127b8a-020d-4739-a511-b425270ed0bd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1535569e-3e32-44ce-ae02-a30dc9c69287")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de2e32f5-6736-4025-817c-3116920b4705")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "463b95cf-ea9f-446c-aa90-5a59787412e6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 34 "Net-(C_I29-Pad1)")
			(pintype "passive")
			(uuid "dff79bbe-7d65-4359-8de1-b8ea7474aa08")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "a38a285e-239a-4c6e-9864-39c4708b1e6e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "180bff33-eca5-44ea-94b0-d746f3275076")
		(at 158.35 102.955)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I28"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "1125f11a-aaa7-46f2-992d-c425761a0cc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ff09b7ce-1176-40da-a35c-f47a740efcc2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b6f9082-7c1a-45a9-8cd4-3ebaee6a6f5f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "81d97ed6-6f92-405c-8d0d-6a9c587da8e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/42fcb9b3-b7e5-448b-9b88-de9e263705c3")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c863e2fe-1419-46db-a843-e643ffb4eac8")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d40000a-ef3c-4c3f-a483-b478d96c59d3")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20bbf90c-71d8-4149-8069-d6a08b57851e")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29152d44-ae30-434a-a430-bdcd4a89c2c7")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4784986-56ab-4c6a-b162-ecea57c454b2")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3846f411-696d-4209-a024-b2a5373b33fe")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4538aa43-2639-4c91-9e61-d22de9c48ef3")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c857882-8b89-42da-917f-b5e6ca287788")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6eb5d5f-85cb-4ab5-820e-1111338ebae4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f97f5cd-e6bf-4459-9bbb-5a40ebc1c79a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d6881501-e26c-4acb-a625-7e21830fce5f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 33 "Net-(D_I16-K)")
			(pintype "passive")
			(uuid "8b5b16c4-f626-45a3-bb86-374b59c76197")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "1c466869-7e3e-4991-997c-9cc4d800506d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "1a7ac19f-4255-40b1-839b-45fb484e2939")
		(at 138.33 129.345)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I46"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "fe34cfd6-f369-4813-9555-671a692149c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e68d2c01-0dc9-4292-aedd-51774d3a13bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "120ceb69-ede6-4d84-ae73-d45a78e79483")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb172ea4-2170-496c-9a9c-32b8d19c1239")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/8afca869-85fc-43b1-bc81-2be442bacd37")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "996fb252-1d09-4577-b356-9a27f809379b")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b16e679-27f2-4892-9d2e-bebf5a44a5ea")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b132339-2107-4b64-90b9-aec501170c71")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca411477-de63-456e-9425-785f74d830c2")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29e15f49-1451-4dfc-9622-f1ee00316ba1")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "530a13f3-1d5d-4098-bfd7-1da816e27e51")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6170edb-b49d-4f70-b073-073b209ac250")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d7ae0cd-f24a-46e7-946e-eb17a43dab21")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb885caa-bbae-4b78-b2ca-c40d37a1e457")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7dca1e68-8425-4aa8-abae-707323ae293e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2f81528d-ca3d-4d8b-9f97-8c9e2034053b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "8dbba9b2-82a6-4bb7-ad19-360eca333f8d")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(D_I11-K)")
			(pintype "passive")
			(uuid "d43e8b4e-c914-4dca-b179-1180e0192a7c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "2026452c-c8e6-4348-90c9-160fc98ccf22")
		(at 147.83 65.375)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I19"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "eed74bfb-87d8-4a5c-ae10-2c8aa1e64fa4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "50a7ef74-739d-4824-b6fb-167883ec68ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d84dee03-6330-47ab-8276-b315af895a61")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0026c974-c867-4997-800e-2dfd79248944")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/406ba2e6-a024-4693-a9bc-c6881ea77d56")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a7bb76f-22a2-4aaf-9aaf-93d45c0ef6b8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad2acd69-645d-42a8-9758-ecf5516a6d9c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a3c0331-878c-453a-aa7c-07d0021bade8")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7c206a8-751b-4690-b2b8-a794540b8a10")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc85b625-baf3-4c79-b5ee-59c76eba8fbd")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43acd527-da02-4c40-803e-ec9ca1c47918")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55e45ec9-4ed5-47a6-a610-a22ae6858012")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb1baf12-81b6-4586-9179-a57708e9ab58")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0964a7c-5c80-400c-9380-c8aa619948d9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "141e5ae7-273f-4785-a0ba-2659c5a125f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "56db115d-bb7f-40a9-ab5d-5a393bcaa830")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D_I4-K)")
			(pintype "passive")
			(uuid "13391585-61f2-483b-a76a-bcfed59329ac")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "Net-(C_I8-Pad1)")
			(pintype "passive")
			(uuid "511df104-d97c-493f-9f63-24882a65b14d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "241cae3f-3cf6-4528-a02f-9dd8bc7a322d")
		(at 110.44 35.405)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J9"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "c3222c38-8317-49cd-a0e2-c9ddf66a1d86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "a141c939-d7a2-4dc0-8b6d-15e3273e2dbe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7f82a96-b3cd-4fa4-b15b-3eac919f0fbe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c97092ca-45b5-4f65-b3cb-6e4c9a952d94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/21820eb9-3420-4c24-97dc-0fc82da88055")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab17455c-e6a2-40ae-8f72-844c9b7d2a19")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36eb51fc-701e-490b-8152-f9d980d02ccb")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6779871-819f-427c-8333-ddccd46941df")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f00f2b9-f9d3-4c6a-9e89-521d8389699d")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06d59415-6bfb-4a01-aca0-9c6364ac6a87")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58c41d4c-9913-4a62-b8c8-57b5808ba638")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4120c8c0-d371-4bce-b1a2-4a6b7095ec0d")
		)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6da2833d-a95c-4057-baf1-83fa06b1b337")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "f47c56f3-24ac-4479-a77a-d086f60d0706")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95a95ba2-afc9-49d8-9c92-a727a1708cec")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86d5ffdd-7883-4ea6-9517-a49d6258236e")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd8f6314-9f07-4adc-922d-97c986529d98")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60bc2047-d865-4066-adf6-f1b29a50eef3")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff0214c3-5844-4cf9-9461-e0735b9a557a")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b21509cf-0413-48a5-85ba-af334a38361f")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdad4464-f44b-4e47-bd19-0d3ecfbea983")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13606c6c-279c-4b42-a020-a8cb4b6dec33")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce5cd0ff-ba54-4cef-a887-ea4e4a98c4ec")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5424074e-e50d-4766-985f-59929bfa0b3b")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89be5788-cac6-4596-999b-7dc443879256")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8c38873-7255-4cdf-8fe5-69d071394db7")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d61fb36f-c951-483a-b9cc-70c30b7545e6")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24e386a7-eb5e-45d8-9a12-4ad5a86e8415")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5af40bd-237a-4cbd-a669-566ad23116a5")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de9905f0-13be-49b2-b88c-9e411a8b29e3")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2707432c-d95d-48c7-9895-10794a486b1f")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2637dd15-71db-4cd3-9942-3f69d2ddd1fe")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "5d01d930-f329-42a1-bf8d-02cefae932b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 121 "Net-(J9-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "bccdd18d-0da9-4380-9335-c901a9e5317c")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(J9-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b1a1fbdf-f214-4faf-be57-d6f18763013e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "2596fedd-3b1e-449d-91bb-7f906f07fd4a")
		(at 141.175 91.41)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I10"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "d4b01fa4-15e4-4870-9405-4bef2e60d6e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "78ae1a0c-e767-4786-b8f9-d1a34bac9670")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01aff9c6-7838-4612-8189-caecef789468")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f1d8c33-52b0-4b23-95a7-871adacb0acd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/0e6b02a5-1750-4662-a0d9-771202511790")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6cd7c0ee-35eb-4303-878b-b4f6caa0e024")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53451cd4-4b5a-4f1f-8a47-75bab4dd3287")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8885cad4-896f-4248-8ec8-98b7c5b9385b")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1415790-16f9-425b-b56d-3b8600a58d61")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "251a2a21-597a-4947-9ccb-c6a5015e07bd")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b708913-5b3c-431e-813a-a56ea01a2e62")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3077642c-dc38-4288-b6fc-c44ccd36ea81")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab066d17-d2e5-48fb-8a94-3473e2efbbde")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "351c877c-5d91-4753-923d-fa8572b42c15")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99105a65-d69a-4255-ba14-10cd9f8ba2dd")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ea87fbc-475b-4bb8-b30b-1154547f1388")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "879e58e1-8982-4ca3-80b7-e70cf122a94c")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1960c1e-a1a8-4c36-abc7-42992165555f")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbb00e54-e7aa-4a13-91c9-9009ffea32f6")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "547243a5-5e50-41dc-b952-69b2fb1c265b")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5ed552c-59e1-4548-a3be-aa5fe1f0ab26")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85a22321-b01f-494b-ad7b-48d951550688")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f3e0f44-f9fc-4917-ad31-94c2ea596e65")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "5e3c8357-3391-4594-8707-ae17a2d8a768")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 23 "Net-(D_I10-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "df3a014b-9a0d-4e04-b51d-828afdff4809")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "06ec93b1-8aea-494b-846c-ee65b4acd9de")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "25d5a2ff-1def-40af-b399-d8520e9aa513")
		(at 54.15 107.105)
		(property "Reference" "K6"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "963f4d0a-6a44-4623-bb0d-1ecdda6e4dff")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e8b85f47-b8c1-4497-8d4d-89a9178cec45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "aa20d9d7-7832-48c4-906b-39cf485bc956")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "588eeb45-b07b-4568-885f-5d38618d6868")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8e003bf-327b-4b66-9419-41f4d3a4f967")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/4c344eff-d976-4da9-ba59-6ba67ebef54a")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "331d2f35-d72b-4372-b2dc-ea2cff5f0fe2")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f356aefc-8321-41e9-8dd6-2bda11d602a0")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e34e0a9c-b8b6-49c5-853d-06a99a18d93d")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "98ae2cc4-d8fb-4ffb-ab02-d462de180e69")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e24946ea-379b-4e62-9e27-ac78acc575e7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "b793f75d-ad01-4ee9-b229-b5ac6de68bf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "Net-(J10-Pin_2)")
			(pintype "passive")
			(uuid "db0d5bcc-8d20-4c90-884c-f0ba29cf67af")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "unconnected-(K6-Pad12)")
			(pintype "passive+no_connect")
			(uuid "f09cc215-aba0-4139-8788-26d3d381050a")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "Net-(J10-Pin_1)")
			(pintype "passive")
			(uuid "f258e5be-9096-4019-87f1-69aa113dedb1")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "7bd71bb7-d108-443c-bf05-957e02bea8be")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/PLC2 GPO/Relays/Relay5_A2")
			(pintype "passive")
			(uuid "617b5aa6-c5ba-45e6-b453-a5f5272ecd38")
		)
		(embedded_fonts no)
	)
	(footprint "TBD62083AFWG:SOIC127P1032X285-18N"
		(layer "F.Cu")
		(uuid "25f62a03-9bb1-4b70-9531-1116bcd9440c")
		(at 21.0075 68.6)
		(descr "P-SOP18-0812-1.27-001")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "a22beff3-a6e0-4e1d-918b-080a396863d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "TBD62083AFWG,EL"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0b15658b-7709-4fb5-a547-389a0004a2b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7293683-fd77-4e96-b23d-9f2658d1d24a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Gate Drivers DMOS Transistor Array 8-CH, 50V/0.5A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "48217486-8d5d-4c31-b2fa-41a302740653")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "2.85"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8662b733-fced-4660-9394-009d372d8f88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "757-TBD62083AFWGEL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1085c5eb-75f8-4dfe-bdfd-6cf820300694")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TBD62083AFWGEL?qs=fSnNYG2PaKJPpDBB6xK1QA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e82596d-e185-4c57-9f8a-b0d1b4277387")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Toshiba"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e357966-150e-4de9-a39f-968b8d06759f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "TBD62083AFWG,EL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f27694e-7dc0-4e75-91a6-cc13f54d3c39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/4b39e818-bbd6-4ffe-bb8f-187ecf4c0338")
		(sheetname "/PLC2 GPO/")
		(sheetfile "PLC2.kicad_sch")
		(attr smd)
		(fp_line
			(start -5.7 -5.78)
			(end -3.75 -5.78)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef522c0b-055e-47eb-af96-a35bf2a772d6")
		)
		(fp_line
			(start -3.4 -5.758)
			(end 3.4 -5.758)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4955efd4-10d3-493f-8d27-4d1138eb9be4")
		)
		(fp_line
			(start -3.4 5.758)
			(end -3.4 -5.758)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "173bf22f-e9c3-40df-9904-a0f9f03abc85")
		)
		(fp_line
			(start 3.4 -5.758)
			(end 3.4 5.758)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0d9b837-83b1-4909-8ea5-7a64f20368a6")
		)
		(fp_line
			(start 3.4 5.758)
			(end -3.4 5.758)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2fa671d-42e0-4bc9-9e6c-5538ece86293")
		)
		(fp_line
			(start -5.95 -6.09)
			(end 5.95 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aafcd788-913d-48d5-ab72-bb5e6249f3fd")
		)
		(fp_line
			(start -5.95 6.09)
			(end -5.95 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4a49241-6736-4a2e-8d8e-809cad897f23")
		)
		(fp_line
			(start 5.95 -6.09)
			(end 5.95 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e52420f-18a4-42d2-91c2-32ab8527dab4")
		)
		(fp_line
			(start 5.95 6.09)
			(end -5.95 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd000859-a638-4393-99f3-b86b8ea5fc76")
		)
		(fp_line
			(start -3.748 -5.758)
			(end 3.748 -5.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5890fc73-f9d0-4167-a578-bb9f54b2acef")
		)
		(fp_line
			(start -3.748 -4.488)
			(end -2.478 -5.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2366e982-e119-4b4e-b098-bcb89757b74c")
		)
		(fp_line
			(start -3.748 5.758)
			(end -3.748 -5.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf0ac11d-681d-4eb4-887e-f65629d0ac44")
		)
		(fp_line
			(start 3.748 -5.758)
			(end 3.748 5.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87ba7445-13b0-42e0-89fb-83056ef700e4")
		)
		(fp_line
			(start 3.748 5.758)
			(end -3.748 5.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39369faf-4e85-40ea-b976-9228e8d83c34")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "15bda35a-59a5-4551-8ba8-45de6dbd376e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -4.725 -5.08 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "OUT1")
			(pinfunction "I1")
			(pintype "passive")
			(uuid "0179879e-0ecb-45fb-9156-ea265ce0b58e")
		)
		(pad "2" smd rect
			(at -4.725 -3.81 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "OUT2")
			(pinfunction "I2")
			(pintype "passive")
			(uuid "6ac71279-e3bb-4f97-a007-c7eba2a61533")
		)
		(pad "3" smd rect
			(at -4.725 -2.54 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "OUT3")
			(pinfunction "I3")
			(pintype "passive")
			(uuid "38ca738a-0698-4bfd-a8e7-1b64b81a3689")
		)
		(pad "4" smd rect
			(at -4.725 -1.27 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "OUT4")
			(pinfunction "I4")
			(pintype "passive")
			(uuid "f2671088-3397-4d9f-a9a9-c45325e801e3")
		)
		(pad "5" smd rect
			(at -4.725 0 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "OUT5")
			(pinfunction "I5")
			(pintype "passive")
			(uuid "6c87b0ad-8fef-4aa0-82c7-173a84de26df")
		)
		(pad "6" smd rect
			(at -4.725 1.27 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "OUT6")
			(pinfunction "I6")
			(pintype "passive")
			(uuid "7f0e5638-4a0a-42c9-893d-47e133585d60")
		)
		(pad "7" smd rect
			(at -4.725 2.54 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "OUT7")
			(pinfunction "I7")
			(pintype "passive")
			(uuid "c368be8a-3e10-4020-89f1-7e70feea3f66")
		)
		(pad "8" smd rect
			(at -4.725 3.81 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "OUT8")
			(pinfunction "I8")
			(pintype "passive")
			(uuid "0cec224f-4319-4826-b7d0-64b186b4e103")
		)
		(pad "9" smd rect
			(at -4.725 5.08 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "08d30441-088e-4ddc-8773-3126495c34ec")
		)
		(pad "10" smd rect
			(at 4.725 5.08 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "24 IN")
			(pinfunction "COMMON")
			(pintype "passive")
			(uuid "e848b42a-4a9b-46e3-8e8d-054ca617091a")
		)
		(pad "11" smd rect
			(at 4.725 3.81 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/PLC2 GPO/Relays/Relay8_A2")
			(pinfunction "O8")
			(pintype "passive")
			(uuid "17ee1238-7c0f-4db6-89c4-d4aa160805f5")
		)
		(pad "12" smd rect
			(at 4.725 2.54 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/PLC2 GPO/Relays/Relay7_A2")
			(pinfunction "O7")
			(pintype "passive")
			(uuid "749ba512-463e-4bef-85e6-8afcfbb6b3e3")
		)
		(pad "13" smd rect
			(at 4.725 1.27 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "/PLC2 GPO/Relays/Relay6_A2")
			(pinfunction "O6")
			(pintype "passive")
			(uuid "5135dd9d-2301-4392-bedc-8972433bb40e")
		)
		(pad "14" smd rect
			(at 4.725 0 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/PLC2 GPO/Relays/Relay5_A2")
			(pinfunction "O5")
			(pintype "passive")
			(uuid "7aafc915-beda-4991-a2a5-be12bfc09577")
		)
		(pad "15" smd rect
			(at 4.725 -1.27 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "/PLC2 GPO/Relays/Relay4_A2")
			(pinfunction "O4")
			(pintype "passive")
			(uuid "dce2fa19-de5a-492d-8205-7757b8193884")
		)
		(pad "16" smd rect
			(at 4.725 -2.54 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "/PLC2 GPO/Relays/Relay3_A2")
			(pinfunction "O3")
			(pintype "passive")
			(uuid "e455f8e4-81de-4904-a62d-cdb004bb5fee")
		)
		(pad "17" smd rect
			(at 4.725 -3.81 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/PLC2 GPO/Relays/Relay2_A2")
			(pinfunction "O2")
			(pintype "passive")
			(uuid "7edf0e72-fed4-4268-be54-3aa704552a34")
		)
		(pad "18" smd rect
			(at 4.725 -5.08 90)
			(size 0.7 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/PLC2 GPO/Relays/Relay1_A2")
			(pinfunction "O1")
			(pintype "passive")
			(uuid "c21d3bdb-cd2b-4179-a226-84b5968721f3")
		)
		(embedded_fonts no)
		(model "TBD62083AFWG,EL.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "2d8785eb-2936-4dc7-8d89-3167134a415f")
		(at 141.175 111.45)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I16"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "16d8064a-602a-4034-9162-92b9a81b867b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "b5e8e58b-6aa8-486c-8cf6-488fa6b93522")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c3d17a5-6576-4b30-9021-e00d5b6cab5a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32bf80fd-b938-4d90-85d2-519a08d24ab8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/d2d46ea4-20a7-4207-ba9d-baa863bc8096")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c577e84-7d54-4ad6-bbaf-bc7b6396a3c5")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcfdd3a8-554d-4e86-b81d-94121beb08f9")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8eaf2a1-3218-49d4-9766-6fd98d5cb1b1")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc20f3e5-f974-4eed-b9db-03f37a0c964b")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f178831e-9513-4d57-98a9-90ec621d4d5f")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba216b97-5fb2-4967-acfa-d0e74fabfd3e")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ed8556b-bcea-46cd-9092-46f3d47a58d1")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9445974-4b2f-4fef-80d4-7e4d1c9646fb")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c35fdcd8-23f7-4c43-829e-e982c68634f6")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2434ec05-4c51-498b-95af-6f279fb4af91")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0507bd14-3794-4fa7-8900-9693a44f9f8c")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03211a62-cdd2-44b6-b5ce-cff5477729e0")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4803487-529c-4505-83c1-3a1115dea8ae")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "126d6fce-ca94-476c-b599-bfadd26041d9")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f263bfa-e506-4dd3-a6ba-605500853fa7")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea329171-e682-491c-adeb-d51cf6c967f3")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8241696-0e11-4078-b057-95676141f25c")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcde373b-f1b8-4013-8e57-62ca5bb38bb1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "e6e22b38-bfbc-4feb-a0e7-0cc09b05ab8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 33 "Net-(D_I16-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "a8dca176-d23f-47e3-a159-423ea889f957")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "a7023d86-cf85-4ce7-a2d8-ef13938a5c34")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
		(layer "F.Cu")
		(uuid "2df1d36d-cccc-4063-892d-893cddd12fc5")
		(at -5.7025 97.82)
		(descr "Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)")
		(tags "push horizontal SPST 1P1T")
		(property "Reference" "SW1"
			(at 0 -2.7 180)
			(layer "F.SilkS")
			(uuid "6b609e19-a969-4a3c-be51-9c0ab7bac354")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "07c4cda5-7f74-4f2f-b4ee-b11527f30560")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "20447cde-fcc6-438a-b62e-404a9b110cde")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0b8c925-3113-48ba-a323-8573d0f2c477")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/2a6e2dd9-ea11-4da1-8863-b29804df0cb8")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.4 -1.5)
			(end -2.4 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a633a42a-2ee9-421b-81fb-058f803b662c")
		)
		(fp_line
			(start -1.8 -1.5)
			(end -2.4 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cae7c84-9fd4-4fe7-a218-f6e7fdda59bd")
		)
		(fp_line
			(start -1 1.3)
			(end 1 1.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9bfda3b-2fb6-443e-ac31-7b792c82068a")
		)
		(fp_line
			(start 1.8 -1.5)
			(end 2.4 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e11bc794-cc5c-4453-a2be-386ede2609de")
		)
		(fp_line
			(start 2.4 -1.5)
			(end 2.4 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adc4537d-75ef-48b2-8258-234e92f208bf")
		)
		(fp_line
			(start -1 0.3)
			(end -1 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "019f6867-0f85-41dc-8d96-1800af3ac197")
		)
		(fp_line
			(start -1 1.5)
			(end -0.5 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a9387a6a-62cf-490d-bd90-2ab042522c84")
		)
		(fp_line
			(start -1 1.5)
			(end 1 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "7a1f6025-a13d-4ca6-87f1-8bc0b7925a43")
		)
		(fp_line
			(start -0.5 1.5)
			(end 0 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a2369a88-72d3-48f6-8ebc-16cf0bf2d740")
		)
		(fp_line
			(start 0 1.5)
			(end 0.5 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a3f40846-0f64-429e-9430-72b239e19219")
		)
		(fp_line
			(start 0.5 1.5)
			(end 1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "ec23493d-27dc-4f86-ae01-67c87c394399")
		)
		(fp_line
			(start 1 0.3)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "bda3c555-eb7e-48f4-8f11-c7fc8bb598ff")
		)
		(fp_line
			(start 1 1.5)
			(end 1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "0dfbb057-1af4-4c04-b4b4-902fc6ad8f83")
		)
		(fp_line
			(start -2.83 -2.05)
			(end -2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52fe9eba-ce12-4c1f-bf48-f7124df415e8")
		)
		(fp_line
			(start -2.83 -2.05)
			(end 2.83 -2.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "055157bf-dd39-411d-9dd2-9df9e7ee27dd")
		)
		(fp_line
			(start -2.83 2.3)
			(end 2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8721d4e0-398e-4428-bf19-b9cbe0f56c0f")
		)
		(fp_line
			(start 2.83 -2.05)
			(end 2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "665f6dfd-9ad9-4aec-8b64-f25fc2e5c52a")
		)
		(fp_line
			(start -2.25 -1.35)
			(end -2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99ca2b05-2332-473f-9e5b-7c6caefa25e3")
		)
		(fp_line
			(start -2.25 -1.35)
			(end 2.25 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f50eaa64-457d-432a-b40c-c57fc08f12ab")
		)
		(fp_line
			(start -2.25 1.21)
			(end 2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07e11e6a-1bec-4f26-9673-4633bda82cb3")
		)
		(fp_line
			(start -1 2.04)
			(end -1 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cee08284-3939-4f6a-bb59-2a9d681ea1cf")
		)
		(fp_line
			(start -1 2.04)
			(end 1 2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "089ef512-45de-449c-8917-2b6eeaac3b72")
		)
		(fp_line
			(start 1 2.04)
			(end 1 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01f9c256-80fb-4441-9e25-539301db3c0d")
		)
		(fp_line
			(start 2.25 -1.35)
			(end 2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5dca3b61-31da-4fc5-a6c6-1e67ce2aec16")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ee353b1e-b30e-43c1-bf2f-23a1d428092a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.125 0)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(uuid "8e9ae593-4f64-4fb1-8c04-2eca54422915")
		)
		(pad "" np_thru_hole circle
			(at 2.125 0)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(uuid "fcf21473-2508-4b43-81ec-16878c057454")
		)
		(pad "1" smd roundrect
			(at -1.225 -0.9)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "6611142f-3e20-4b46-9ac5-d1a834a6ad9e")
		)
		(pad "1" smd roundrect
			(at 1.225 -0.9)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "c3856b9c-d212-418e-af67-912921223935")
		)
		(pad "2" smd roundrect
			(at 0 -0.9)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "EN")
			(pinfunction "2")
			(pintype "passive")
			(uuid "5f19c451-3bf1-4269-9d8a-fb16ebf7c151")
		)
		(pad "MP" smd roundrect
			(at -1.85 1.05)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "f7521d33-2560-4514-8dcc-8af803b17e34")
		)
		(pad "MP" smd roundrect
			(at 1.85 1.05)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "86536076-166c-45d4-9dab-4e050cecc2e2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "2ff1396e-f0ae-48b5-bd15-a3c57fe741cc")
		(at 153.54 99.945)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I21"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "2435e3e6-1045-4f5f-b0f2-95c4026349f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ee81324b-d568-45bd-93f7-203174296926")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9176756-58c7-480d-b616-8f4af6032750")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1af9fc36-11bd-4199-bcd9-b536c83af256")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/7371191c-5341-48b2-99f1-5bd2a61f50bc")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01d723f3-23c6-47f4-816f-61044db8a5f8")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "552a1e47-5245-40ac-be3e-fe757d94d3a4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c4abad5-657b-4f1c-abf1-618eadfca6bd")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80df3490-ffcf-4c5c-97e1-d6795d0c9e2d")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f60b1de8-8437-4d09-bba4-a07e800cab06")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51cafef2-8c03-4475-adb9-854e663a444c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71b3203d-0e6c-4c7f-9471-01f6defbc85b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "823fec07-7436-47e0-8c1b-41c6b2d0d9d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c8d63a5-00e1-47ac-a2b1-69dd7dc7b2bc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b488d003-bd89-400e-9691-0586a4894612")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5c35d163-5b13-41d6-aa85-a1858f8bfc79")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 26 "Net-(C_I21-Pad1)")
			(pintype "passive")
			(uuid "f52cacd7-6551-4d61-a360-915c0bf28d4f")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "2198e634-bade-4b34-a4c6-8b78614184ae")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "325177e4-a8e2-4a63-86d9-46baf269e0ca")
		(at 158.35 93.925)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I25"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "3f95e3fa-3b81-4357-a710-091dd1955a12")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "0af1d8c9-406d-4105-b0a0-12407dfbc055")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c928d92e-13d0-4b0f-a724-3b8934ba04d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6190951b-e33f-4846-a01d-802f9fbbd179")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/e3c6ed0d-d2f4-4b65-b981-d926b39bbd8c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d11e500e-2c0f-47c3-8bd2-934ac4b355e2")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b644c31c-9a01-4c3f-abd5-8e2a5ff859a2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa286ab4-bf02-4449-b464-a4622df6ce15")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff6ec0fb-8346-4bc3-a349-93c19eb99d54")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b339dc3-530e-4a71-8602-23c0c485b551")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a54aa509-fecb-43e6-a18e-0a68eaaea328")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a17b161e-6319-4dfe-9f92-d63869b127ca")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2316806e-57eb-45f8-a462-9079fb74c9d9")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc7e99e9-3614-45a3-a71b-c8299e216a9a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1fb156db-4245-4085-bbf0-57d70100b73a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "285ba218-7d09-464d-ad30-5dec5cb2d4ab")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 30 "Net-(D_I13-K)")
			(pintype "passive")
			(uuid "f39287b0-7cc5-4129-8c81-6eb340a6e915")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "a3745e11-c87f-4647-9d55-277c2eaec580")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "349067bf-a0a8-4b75-8154-0cb9769e6a90")
		(at 87.52 44.22)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J11"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "d9d9acbf-da90-4b34-89c4-9adf765f31d1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "c05181d2-1057-47a9-ac36-2f973e884ec8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7fa5fc2-8102-46fa-adbb-7e60c3dfe8cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b9985dc-69b8-4317-873e-aa99e809c1a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/f4fa594a-336b-42e7-a959-586272aee921")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0753bc13-3b4f-4305-8150-6f982312583b")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4eb2eb7-97bc-4ea2-9a7d-45f3770fd312")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "163eca5b-d5d2-4d91-ab77-f6fff4d965ac")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65380c59-1fca-40ef-b92f-1ee90c5c3da0")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cd97264-d76d-4508-a3b8-c71c5484ce2a")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5db8cf2d-99ff-478e-a7d5-364b614fd7c3")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a51fcd7-7734-4ad6-8784-2c83473e956d")
		)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d44dc498-a51d-4e29-b416-2e2d189686f3")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "a36efea4-5323-40e1-9f9e-be3c617b9963")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57363847-68ae-4921-ab42-c82adee8d8ab")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0490000f-50fa-4063-8534-0a932d6b6318")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50ff23ee-ab84-44f2-a41a-d5d1df7ebd81")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8628edf8-65ba-4673-91b0-6d5eacc547fd")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44bcce1d-cc31-4ab8-b787-a9544272f24b")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea6d0ecf-1b85-4258-9324-a66bb0eb0b7f")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3da914f0-fa22-4ebc-91f4-364d72f0ae9b")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c567b260-4a54-488f-ab2c-fe4161612f7b")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4fa32e3-23bf-4594-851d-b463ce3cb2b5")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29e19127-850a-4590-affb-f5ce4a723ed1")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76f9cb58-c34e-47b7-97d0-0fae47ca40db")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23182391-e78d-49c7-ab54-b793b793b12a")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ce5b682-8521-4709-8d50-a7be6eac641d")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d44b4f2-0197-4e61-a3d2-5a7b8da29d08")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d99db1dd-9c17-42d8-acac-90df26e481a7")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "100b4477-7d80-4221-befc-0a82e14281fe")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2561ac40-2eed-4fdd-a1e8-64d858c475be")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cee3e3a2-bcfa-48e0-b659-d8248b780a10")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "39140be3-04d4-4dbc-8c11-f40387656b2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 124 "Net-(J11-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "761d04f0-b7b3-4fe4-865c-817d03682453")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "Net-(J11-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "e1224bcd-a6b9-42e2-926a-ea943baa9f39")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "35c465e4-8d74-499d-a843-5b5547404db2")
		(at 152.58 74.225)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I30"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "645b99a2-226d-4219-a3cd-e51b70ae6c32")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "46101660-a424-4637-9969-286919b8dfa3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d5bd142-b626-432b-850c-0ec049e330db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6e2616ea-dc8a-4a1f-949d-c18d91f36536")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/ac964d8f-c8bb-4320-9eef-471ba52e0880")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ea8dadb-31a2-40a2-8d1b-9056cf9e916e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4e31bc4-2cda-434a-ba7f-bd2fa778b56d")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5baf381b-a696-49f7-bccd-efd416a31855")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f590b22-13e8-44e1-996b-b755a5f7d340")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce788a16-74e1-4e18-bca2-51c8dcd01341")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a820417-5df2-4a05-b7c5-94727ea13173")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e34f1d2-b424-449a-ae04-acccf81e01af")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25092f49-7765-46d0-acef-928683903afd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90633797-46ec-4824-8f73-c796ab8d8dba")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "112d0605-b210-48f7-85be-421ddb944652")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "035abc80-994f-42c1-b9bf-37b25c9eff56")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 86 "IN6")
			(pintype "passive")
			(uuid "d4a866d1-6224-4050-a3a2-3dd5b7ed12d1")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "8fc712ba-c76f-45fb-a48f-01875855dd62")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3646a88f-29dd-4e32-b507-112681d37659")
		(at 147.83 123.445)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I60"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "af907b55-d5f3-4169-97d9-e2dfbc352002")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "50b14deb-7270-48f1-9d54-18fb5b27ca57")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8cecd2cf-532c-40f9-8ca4-48958f6dd930")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "962e762a-9b95-4227-8369-21f09043e018")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/9a4adb22-1d4f-4385-a057-ba21e66ab418")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "639259c3-befc-4ec1-b944-70c0a5be922c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b976e33-1582-4a75-9171-834d5ad996e5")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c91e81b-461f-4027-8505-e839b69c6fae")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c6637ca-84cf-4fa3-a53f-4724cce687ed")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcd2c6eb-38ab-4870-b6d0-5c0b3a9a4371")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e99631e7-a645-42ff-9c84-6cafad80f32d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d58445d6-7b08-4ea2-87ca-fb41b458e363")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca496140-b809-403a-a3ce-e6f7e92c4448")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80152998-e279-4834-9d0e-b2117afca479")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a77c5c6-83ff-4564-bb10-3d59be61e52c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b4cb039c-f1af-499a-a30a-09482c6c65a0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 90 "IN12")
			(pintype "passive")
			(uuid "10c42d95-e3f8-463f-8f4a-ba73cc5a02fd")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "c0463790-1f4d-48a6-94dd-003ab857cfda")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "37a5397c-bfef-4902-b99d-853473e5d1b0")
		(at -6.7625 82.79)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J7"
			(at 1.27 -2.38 0)
			(layer "F.SilkS")
			(uuid "80f2f43b-1e5f-46d8-9921-0091ac6a2ff0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_02x05_Odd_Even"
			(at 1.27 12.54 0)
			(layer "F.Fab")
			(uuid "ad8e7613-0f67-4069-a7d8-1fb1427f0a1e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d02b4d46-8d78-4457-bb7e-f55c5db7ae7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7923846-b463-4495-8849-564bd22758f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/64bc3050-92ae-496a-bb8a-b727b8690d64")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.38 -1.38)
			(end 0 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58b19ab1-a2bf-4d04-8e31-559a2da0287a")
		)
		(fp_line
			(start -1.38 0)
			(end -1.38 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "794284ba-8c25-4cee-9118-f6b021edf11c")
		)
		(fp_line
			(start -1.38 1.27)
			(end -1.38 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9161d3b7-d81a-4865-8b81-31a39708d574")
		)
		(fp_line
			(start -1.38 1.27)
			(end 1.27 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bec8f138-a4aa-43dc-ae54-6597cab7ebe7")
		)
		(fp_line
			(start -1.38 11.54)
			(end 3.92 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3eb79255-7f7c-455b-9108-05776db4520a")
		)
		(fp_line
			(start 1.27 -1.38)
			(end 3.92 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56e07389-2345-4591-a5d7-c956132d6ab9")
		)
		(fp_line
			(start 1.27 1.27)
			(end 1.27 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49a7f0fb-ee84-43cc-bf50-c296c388706f")
		)
		(fp_line
			(start 3.92 -1.38)
			(end 3.92 11.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8437cd1d-dc19-47bd-9754-e9a6c620af74")
		)
		(fp_line
			(start -1.77 -1.77)
			(end -1.77 11.93)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8eaf5cc9-cecf-457f-b8c1-174536920d4c")
		)
		(fp_line
			(start -1.77 11.93)
			(end 4.32 11.93)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d491b45-d547-4478-8feb-3d23b2adf52c")
		)
		(fp_line
			(start 4.32 -1.77)
			(end -1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fb1deef-0c7f-4e59-a91d-4375bb7d03ff")
		)
		(fp_line
			(start 4.32 11.93)
			(end 4.32 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8511390f-889d-4db6-856c-6f2dea2f7531")
		)
		(fp_line
			(start -1.27 0)
			(end 0 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b8ee3ce-b678-4a76-8095-df7b7cd28c52")
		)
		(fp_line
			(start -1.27 11.43)
			(end -1.27 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd44bbd4-c645-4ecc-a61e-b23d4b8f0c19")
		)
		(fp_line
			(start 0 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a6ba0e4-3004-421d-9fbe-15af56694c72")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4441ad67-98e4-411f-a563-2bd3ec0305d6")
		)
		(fp_line
			(start 3.81 11.43)
			(end -1.27 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53747035-1cb9-406b-996e-f0fbb54e6c5a")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 90)
			(layer "F.Fab")
			(uuid "49f68c0e-1097-4b35-948e-a7a73960828e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2af73281-d423-4942-80b0-20a3f406e3df")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "TMS")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "9fff25d7-c896-4b25-b5e0-5af01c29903d")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "31e1bf18-0174-47f0-b3dc-1bafe628df8e")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "TCK")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "b962e104-cd88-4035-a19a-c2a75cc31a5d")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "de1062ac-582c-44fe-90d2-358ac4d2803f")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "TDO")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "25f23437-e8ee-4eb3-976b-cc08c2753ce7")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "9d5eda13-af24-4d7f-8ee9-78e48d09f7f8")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "TDI")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "86d713bb-b3f1-482a-b055-ef5944c77dca")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "942e5969-5d3c-4862-9ebc-b47ad8df2e35")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "unconnected-(J7-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
			(uuid "20b77f00-84ae-46e2-b189-1d64c7d75dbc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3845943e-60c0-4d16-b074-2b43b40e55a5")
		(at 148.765 38.88)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "21c22402-26ab-40a3-8ffe-10ae2ea1f1f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5b316f2f-d79c-4dd1-b5cc-7b2f7f82d31c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "53be2c07-ae11-499a-ae2c-67adcda5033d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "29d0eba3-deda-49f4-a6e8-e37feca4381d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffc832c0-67fc-4cc8-bb8e-0dcc62ab8d88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/514a0196-ff03-4d2d-b1c4-88ec83caf6cd")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8d340ae-40d5-49fc-84d6-085fb71eac1c")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48540f8a-be2e-4677-8d71-a41ebdebcba5")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "388d9c5d-a0c3-4767-94df-99935ec8dcdd")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd3392a3-285f-4238-942f-df92059a3675")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2d67652-a3e8-47f1-82dd-04f5cb66aef4")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "538f30c6-2455-4238-a65a-42de81b31212")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "08445a71-fa6e-4679-98b0-6bf0e2c476be")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7198b1e-8bdc-4403-bfe6-f996cd1eef63")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ee552f1-d55c-4798-9e9f-45fce088e6a8")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abb3511c-91ef-4de7-ad89-fb8f0eff2842")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42fb5237-c771-42f5-9b65-85e10ca896c8")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcea9264-58d3-4a21-8131-4fd9fab4e03f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cc5e9a33-8298-4cdd-a169-26dcff50ac3a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "1b1d5644-7127-457c-8e29-4f0460526809")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 40 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "e7f58f83-5d91-4c9e-96bb-ae9c77fa24c6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "3997d4e9-b125-4737-92d9-f7aac9fbd1f4")
		(at 126.76 115.005)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U21"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "d5ec9692-d860-43a3-a430-b63955f3d8a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "9ca8e9a0-ffac-4ab7-8f20-d94254da8629")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b6e5089-a5fb-448f-896b-0d88faede529")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "042fc6df-7198-4bc8-906c-86961c6503aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/21276137-376a-4d7f-ab72-7de6acc0e07a")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d09207a-c6e6-492e-b194-0ab4bc851d80")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1c13e46-ab68-40a3-ab2e-5a1d7f352b31")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "892a6285-c8cd-4365-b1e1-9ea1c6dd1dea")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e21c7cf0-5f45-465d-8dcd-45fd5838680c")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edd6bca5-7284-44b2-9636-f7bc69d604b2")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7eb8de87-8d58-4cef-b926-44f20fdd403f")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ecfcba2d-c488-4757-8f59-26ee79ea03ae")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f09817c5-485c-4dc4-bbb3-e9d97b8b3a94")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4cf92633-3cee-4374-930a-85aa2c62c06b")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c952c5d-eaf8-4c84-ac61-918225eb2eac")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80006a4e-ccbd-41c1-b3a0-2d6b2712d106")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5179dac8-2f01-456a-a530-9c1ea2b788f8")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "ee35431f-562d-4c7b-9060-66dd0a69c5dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 34 "Net-(C_I29-Pad1)")
			(pintype "passive")
			(uuid "49a678a7-ae4d-4123-b3d9-6608ed43531c")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "217c5707-15a7-4030-a061-23c61ac6dc9b")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "da80a013-a26c-433b-ae26-e92c8eb7eb94")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "IN13")
			(pintype "passive")
			(uuid "500746e0-7c06-4b97-9b85-59eb39f225a3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3a0e21db-2498-4800-bf53-d266b3fb86e1")
		(at 163.16 96.935)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I32"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "495e11a5-4b9c-4a88-8110-3bc50487a5b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ea7a8491-0511-4c6d-a4b4-c75034cf3f44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f8fa5bc-5fcf-4550-8bea-058668c397a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b17e0b5-8936-42ef-b975-1ecbb8f64aaa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/dbe99fa5-6b5f-4c92-b562-18a97c14a69c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97ad32d4-9672-4163-8760-408a7c299792")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cb63d96-2fd0-418f-9e68-904b9a38566b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbfb9899-a656-4b5b-8e33-ecfc45dcc5be")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d9943da-7af9-4546-816c-9a796767df95")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ddc55775-6def-4f42-91e5-f2d5897bc43b")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63027cfd-78fc-4d0b-854b-d16e8f455db4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "365d1fa9-3097-4678-8fbd-49587b6fd4b7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea6ba31c-a5ae-4958-970c-c84222a8c48b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1053e80c-fed2-4b6d-bd10-b3398aa5fae1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebf5153e-46fa-4482-921d-359b844e8d2f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "009b2f1a-cd1e-459e-b2f7-9b1c314a39b3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 37 "Net-(C_I32-Pad1)")
			(pintype "passive")
			(uuid "ecba5e10-7c8f-4170-9091-42be0f1312fa")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "66f6d107-1c1d-4b5c-b890-a5a210d7afbd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-3P_1x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "3a23bc52-1771-423e-a840-f46afeb653ed")
		(at 0.6275 84.62)
		(descr "Terminal Block Xinya XY308-2.54-3P, 3 pins, pitch 2.54mm, size 8.12x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-3P pitch 2.54mm size 8.12x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J5"
			(at 2.54 -4.22 0)
			(layer "F.SilkS")
			(uuid "673a8236-2bca-4ee6-939c-bc8e06060bd8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 4.52 0)
			(layer "F.Fab")
			(uuid "aa2aee8e-4d73-46cc-9545-cee9c3606204")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0d1393d-130f-4439-b55f-78447759055b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c787d58c-0728-4470-b1cf-2cb2bfe4a27e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/6ad5211a-d3c1-4577-832d-b40040ebc866")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.64 -3.22)
			(end 6.72 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7db0b5c-38e5-4b36-a9ce-e45bd2e3cf12")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 6.72 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44b32b21-3276-435b-b4e7-ab67adf3758c")
		)
		(fp_line
			(start -1.64 1.6)
			(end 6.72 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcb1b2b9-0b09-498d-bb5b-7d7eee8876ca")
		)
		(fp_line
			(start -1.64 2.6)
			(end 6.72 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e068ca7-5886-4147-b857-12464b901731")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d4ad2e3-7073-4a52-80b0-9f2eb4bdbae6")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28659240-34a4-4232-915d-462758083162")
		)
		(fp_line
			(start 6.72 -3.22)
			(end 6.72 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9caa9083-7124-44d1-9265-efda9fb56ef8")
		)
		(fp_line
			(start 6.72 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "227cc596-8c33-4cd5-b91c-59eb3acbd055")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "c5ff5a88-5227-458f-a510-3a6634e649c4")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12313f29-5760-43de-997f-9ed3eb894a84")
		)
		(fp_line
			(start -2.02 3.9)
			(end 7.11 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "862e723b-b25d-4893-a91d-0ea7e583527e")
		)
		(fp_line
			(start 7.11 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c59603f-de1d-414d-afe3-7e830338fac9")
		)
		(fp_line
			(start 7.11 3.9)
			(end 7.11 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "007b0241-1c3f-4f95-a15d-333853c3c664")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 6.6 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d331125c-27f1-4ac9-89cd-8b837718aaa4")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 6.6 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a45725aa-f195-416b-abd9-c9199abe4179")
		)
		(fp_line
			(start -1.52 1.6)
			(end 6.6 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53a0ec03-0a6e-4f18-bfca-e6695fd3dfb8")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a49f597d-8ad7-4795-b15a-e8f2ab8d235a")
		)
		(fp_line
			(start -1.52 2.6)
			(end 6.6 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4fa3267-936b-442e-814e-ee50b18ed1a2")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "444b0d89-73d5-45b9-9d17-d1473985c275")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83d57196-590a-43e2-a5e0-8e4a878493eb")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61d88f27-12ef-4cb4-b821-662cbc321d23")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df588806-476e-44b9-81ce-32e939427d78")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92f5cb3e-41a6-4da5-a0ed-1829ae53493a")
		)
		(fp_line
			(start 5.716 -0.758)
			(end 4.322 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2cc3a99-c8e7-4ab9-a67b-b68114552163")
		)
		(fp_line
			(start 5.838 -0.636)
			(end 4.444 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c65a363-9528-4093-bd97-63f3a244b086")
		)
		(fp_line
			(start 6.6 -3.1)
			(end 6.6 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a7f5b6c-9d11-455a-9842-3d50f881d05d")
		)
		(fp_line
			(start 6.6 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e9ee859-6700-4500-88c3-55ea1e04e634")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "4ffccfa7-82d5-451d-abfb-e7749046ab8e")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d718cf9b-6bb8-4585-b9ee-678a6395922b")
		)
		(fp_circle
			(center 5.08 0)
			(end 6.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f4c8382b-6c44-4bb8-9ac4-5eaae21dcf32")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 2.15 0)
			(layer "F.Fab")
			(uuid "dbccda7c-414b-425b-b678-b096850a4515")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 114 "CANL")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "91ee9470-9d13-47af-b6b0-987777f1625e")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "CANH")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ae2b0beb-4b57-443e-9f78-35ca18225045")
		)
		(pad "3" thru_hole circle
			(at 5.08 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "f2a233f0-f546-4218-8772-1d5cf1a873eb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-3P_1x03_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3a5ab838-ffed-4d5e-92a4-dcdaaf09dd21")
		(at 143.08 74.225)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "012524a6-1510-4d8f-8049-cbe3ce5458ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a6c22ded-c198-4518-959d-be83959fcca4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0ed1cb7-4a19-434d-adef-b736699d00ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6f9c2e9-fad4-4bcd-91c4-31b1ebcedf63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/4324414d-fdfd-4189-9d80-042a7ba04eda")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "deeff45b-5c54-492d-b380-efe58a3631a7")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75cf46af-694c-41d5-859c-5cec6b7560b1")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b23eb17c-f82e-49d6-9166-784eda527e3d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05cc7c43-2764-44c0-acff-32b91b7c9cc9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7add53b4-504b-4427-bfdd-7162c3cc43ec")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94156dc7-cb6d-4a74-a185-01775972c81c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce5bcb31-0969-421b-bbbe-6dc0cfd85ee7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f04af4c-2f83-4dc7-bd6d-e4e373d5ac28")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6aeb8d9a-4eea-4bc0-8362-a846c43e1d7c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6545418a-5f79-481a-9506-393499562f07")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ae731190-b0ca-49f6-b7de-46d399cbb134")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(D_I3-K)")
			(pintype "passive")
			(uuid "e7fd6aed-bd80-4c5d-ac97-a15058be1f23")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "Net-(C_I6-Pad1)")
			(pintype "passive")
			(uuid "1c2f8a4e-464c-4ad8-8474-2d80063daf97")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(uuid "3c73f07b-0ac3-4577-84e9-a88f032f100c")
		(at 3.0075 100.955)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U3"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(uuid "3ef5af72-bc50-40a5-a629-638ad4921b8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LD1117S33CTR-ST"
			(at 0 4.5 0)
			(layer "F.Fab")
			(uuid "e69ede76-85f9-4540-b1cc-039cd39dcd78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1da02394-7e50-432d-89ca-fc5a246140ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d803228-20bb-4841-9c4c-1f4a61eb6d30")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(path "/fd70f0bc-86fa-4550-9b9b-d941623ef582")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.85 -3.41)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c8d73de-faa3-40d7-846f-f572fe359922")
		)
		(fp_line
			(start -1.85 3.41)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21c56278-c388-4aa2-935d-54c1d8fa0dd6")
		)
		(fp_line
			(start 1.91 -3.41)
			(end 1.91 -2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4547df9f-6f75-49c5-98b1-4f1cbf4a752a")
		)
		(fp_line
			(start 1.91 3.41)
			(end 1.91 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd4575e2-1150-49ef-8020-288b7d102369")
		)
		(fp_poly
			(pts
				(xy -3.13 -3.31) (xy -3.37 -3.64) (xy -2.89 -3.64) (xy -3.13 -3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "b79a3978-ebd8-4890-9d68-c93a9a69d1ab")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9aa50a20-9a72-459c-b7cc-7cb08247c019")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "939c7a67-4cf4-4d4f-acb7-21f9969d8a06")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b1e0aba0-fe1e-45a0-9a85-91eed3210faf")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25c21381-80c3-41c1-85c5-5666dc2cdb88")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1fa67d8-00d8-42d3-8d63-e78296731b4a")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -0.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9e5e747-11bf-4ead-892b-1f011bb4953a")
		)
		(fp_line
			(start -1.85 3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f48cdc85-2df4-4e2c-b3d4-3cdc60442188")
		)
		(fp_line
			(start -0.85 -3.35)
			(end 1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47cdce40-896e-46da-80b8-105ad5c90fb2")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "661f0e4f-34b9-4eab-96f7-1ae73ed0c7b4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "5bf84ee4-af94-4e10-b360-e9f63f1d7069")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "6e25ccd4-d179-4cae-9549-1ff8e06e1d77")
		)
		(pad "2" smd roundrect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "3.3V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "27d0f4fa-7cae-4605-aec8-fb92affc9418")
		)
		(pad "2" smd roundrect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "3.3V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "dca755cd-18b8-446e-9619-4c5981acdced")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "a943d88b-5d61-4095-88b5-869c8f0e4408")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3d83478e-808a-4084-8819-5551a9cda3d8")
		(at -11.4625 88.02)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "0bb46bf8-4727-45e7-93e2-1f865bcada08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ec71bf05-f64a-440e-8731-8a7bbf080739")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d36a75cc-30f9-4cc1-a753-3da1ada6f3d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b6c96a6-77f5-44ac-9ad8-db7c5f9e7a78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4be1ef54-6569-48af-b253-fc66b3551d29")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cb7de57-d555-49a0-ab69-d76c97ff26c0")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbf814ef-7045-4b6e-aa9a-43d749003e9f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8310e73-e74c-4a57-9184-d7e19f556e44")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aec8b0e1-0829-4bbb-9d1c-b9decc5aa65d")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7aeef17-0766-4145-b9f9-3bf59d487a0f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "234a4d70-6b10-4826-87fb-cbb5d8faa4f3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54494688-3548-4588-b200-3762992dc107")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04a06719-717f-42bb-a06d-ab0fd3104228")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6a79e94-02a7-4448-a7d8-933d00ffeca7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60524526-7fd9-40b8-bee4-ed416658e400")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "419c9ebd-16e3-4e6f-b5e3-320907f59cee")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "af52074a-626e-4b96-b3cf-fddd64a078e4")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "5V")
			(pintype "passive")
			(uuid "0b31d786-2933-48bd-a9c6-88be206a2427")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3efea083-9043-4a82-9843-8e0e4ade9a44")
		(at -11.4625 91.03)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "5cf6ceb4-8c70-4ba4-bc7b-5c3288bc21ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "bc9e1891-99b0-4046-8eec-d0fbd5c97bbc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0d1299e-93bf-461a-9182-da3af308dbcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7ec15c6e-fdbb-40dc-99ac-31b9d536e5c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/14c971c2-c9d5-44d7-944f-1fc1ad0707e2")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ba52135-cef5-4a15-b6bc-59ee5877e144")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a258691-bbb6-4a24-ba92-53039faa3428")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f2e6d03-a308-43e3-9f14-a125d362118c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4325149-582b-453b-87bd-ecde8759703b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fb0c614-a520-49ed-bd6e-f709b1d21c2c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a049b6a-809f-417d-afee-ce6de4db1f25")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3f23e56-b880-4c6b-9aee-88f2dfaf78cf")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18179692-8435-420a-a43b-9a993a11fd64")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43d6eb3a-e305-48cd-b163-4bd467bac9d7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c93d2591-2145-4a4d-9aea-888734b19a2a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "64c2e9bf-b53c-4b10-b22c-a6d2042e5bb2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "489a51d1-3133-472c-b559-fefe70374e01")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "62c43f8b-0243-4e14-96ba-b5fa3b5d0d02")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "40a2ca4d-18c4-4574-9294-de660f545981")
		(at 148.765 103.12)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D19"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b920af60-072b-4680-8416-e24c9dbe72b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c9acf0bf-b330-4aa2-833d-1a060c4e1699")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a92cd06e-c8d1-4ff1-a73f-ffb628c22b9d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e33fb12-6e15-4131-94b2-1559d4d1b58e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "31d2e199-efa0-43fb-bafd-8f4e6b4539ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/a5dd06e8-c38a-44e2-be7a-b3e1d68cc13c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ef67861-8e7f-4644-9aaa-5fdfffe682cc")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "802ee3b4-5584-4c13-82ea-f7e057824482")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34468d2e-905e-471c-a38d-6590e18f99f2")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5c77c70-a527-4353-ada8-361379c82c59")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bcf71cca-1612-496b-bca1-eda59e2e22f7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bae9e21f-c589-4657-9fb8-d909c01fe067")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c15bc494-6158-4a66-a44c-2b22245c9a75")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae1d6999-9547-4c9c-9794-44ed1306abbb")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bee3250-1f94-45c8-a4c5-65f9e25fcdbd")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdbd1f78-6277-465d-9c37-1dcf2799be73")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf05b957-b4c0-406e-8152-48981b353d87")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "602795d5-e7f5-4a99-9771-8a668b63a1e8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "92bd52c3-35a8-45ad-ae85-89d59e10dbaf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "041a05fd-6f00-46f7-adb7-dc7f4fdd4b40")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 51 "Net-(D19-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1febef46-3521-4eaf-a766-533e8cb2d0dc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "415078aa-5f37-4eff-b038-c5369cc6b162")
		(at 148.765 106.16)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D20"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "6d8d3a6e-a207-41d2-b5cc-e90c1120c418")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "cac63e6d-927b-4093-8eb5-d9bf60cbbb5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "93fdb03a-8b76-4f62-9027-1a6d72cf15b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3511b2f4-b281-4562-830b-80d77b2838b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e8f139c-31df-467a-8f9e-f0527b2aba54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/e1807c8e-7a7f-442c-8fa0-682b56224d17")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebc0a12c-b7f0-4084-ac67-c31f69033a0f")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7641f75-d936-4ffc-8f24-72e75e4926b6")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bde23896-aaa9-40f0-a03f-f306c1bbe51e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b15a4c1-1b76-430f-87e8-208b110b8f1f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa98f3a5-769f-415f-97a5-1ea20d60319e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eaf2289b-064d-4b4a-9255-f4c3f77cd021")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b620b0d-370c-411a-ab91-a517f5ddec8e")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b133498b-ea52-4ebf-bd9c-179c1a90ce61")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70e067b4-9c09-4a97-afbc-47f8c3b5ff0c")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8dfd910c-d58f-48af-b4c5-b84e4b5e84a3")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "744fe840-6bf4-4ca9-9b4b-0345f230d3ac")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12560b4a-8f7d-436e-a052-36082f0c19e7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "95993a50-2903-4e7a-81b5-0354c4bdf97e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "1f1f13d0-178f-4113-ab63-94542625788b")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 52 "Net-(D20-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "ddb964ba-5e8b-43ee-88b0-8c141ee2a6f4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "42a62eba-e86c-4e7c-a130-1aee51900fd0")
		(at 143.08 126.395)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I53"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "28e244ff-62ce-4a51-92b3-9f080756808b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "711d2efa-7ad8-4aa4-83fa-6d560a61b0fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c7186ac-164c-4d6a-9971-c2738cd3a161")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "88104283-8d72-4b5f-a7fc-a3ce02b10894")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/1cdc88eb-f790-47fb-aec8-eecaa6929c3e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67cf1a1e-de97-477e-b35c-f10aad023e0a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "145a6487-42da-4d52-994d-f7567f2b63e8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e595f1e7-17b9-4f6d-9613-6c7fae34aa69")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "659694fa-732b-48b0-b5a9-3d8b55431b1f")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0cc991c3-31ef-44be-8474-9f4d308d6ec4")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db948825-0283-4c31-b644-e0e3eda4ac7c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe21250a-4ed3-467e-8f13-ae0498d1b1f6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be357cb4-a485-4aa7-a750-252398aba547")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ebe0980-4747-4d0c-8d82-c1d218fbaab5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80d7914c-67a7-4428-a7f0-98751513b316")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c13e20a0-4a38-4dff-b08b-96ccf2b54005")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(D_I9-K)")
			(pintype "passive")
			(uuid "a346167d-91ae-46b3-8535-feff73401da3")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(C_I21-Pad1)")
			(pintype "passive")
			(uuid "8e725299-5338-4ea8-b789-28f7050cb388")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "4521834d-ccc4-4a12-b916-a60d73311487")
		(at 126.76 101.725)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U19"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "47905d66-b748-4511-9816-354763fd02b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "da01e129-fb44-43bf-af89-6e0649b9890f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0274fed8-5dcc-4b3e-b968-683ac65843bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2faee8f0-30b3-4002-a98d-a6d6f5b5005f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/2de99f44-d739-45da-8106-ef6d9e3a575f")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27a6511c-48a9-432d-baca-3ff54b941e5f")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "caa8913b-7745-449c-9b05-bd56cb62cf3b")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edae25f6-51d3-498a-bf5b-a376f1e9e721")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c44bc3d7-f82d-4e23-a2db-a97d1fa4cbef")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "758243b0-d2c9-4254-ae7d-80b4545cec67")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4de9028e-7c48-4d9f-b1b7-3b2ef6dedb3d")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "84e1772b-c748-42bc-b459-eacf4682b75b")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3609f00-72c0-4bb1-a25f-5f4fffeec618")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c5564c8-e8d8-4dd6-97a1-0e67927d6d56")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6a615c3-8b4a-409a-94f2-27d8937b26ee")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "477528b7-04d7-4bea-8f59-b666f60c3500")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b229e3d1-97fd-4fe5-813d-42b7f205e4f7")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "c6ada2e9-41e7-4951-8640-715afbfdab19")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 28 "Net-(C_I23-Pad1)")
			(pintype "passive")
			(uuid "9a85b4cb-e6c3-46f1-b304-5e78995bdeb0")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "f33ccd5c-0088-4a9d-9305-1237400226ee")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "6fbeb6f7-751e-4278-bed9-7702f9561923")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "IN11")
			(pintype "passive")
			(uuid "9d7a2939-c924-4dc3-9eeb-327c393d1f8a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4532655c-8cbc-44a8-a0c0-4e13ae1dbf44")
		(at 138.33 80.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "ef6ce704-b999-47e3-9d59-8658c5d3616f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "9c91a96a-6994-4792-990a-a3e4e1ed6eac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5dc3254e-68bb-4e49-86ca-c8752112b26e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0bb51f2-dc6d-4a45-88db-b086f27de32b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/cbb4ec4d-859d-41ee-9704-1f4f7cb67932")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "665c3831-3830-4ecd-a18c-98848157cbad")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4f1fa52-0887-4e63-9424-f60739885816")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae75ace8-7755-4777-82c2-14d76bb852f4")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23eade2f-a751-466d-9649-ad1568d038ad")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d10c2cd-2de1-4fea-9d83-a5bb33a5fdc8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c002c6d-921e-46ee-bad5-c57e37134897")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "547908db-3b0a-45b2-b951-32a574c31328")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7565d244-5bca-4add-a041-2d2b9a51eeec")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "613e7a43-75ec-4fad-8e96-e94920d4f169")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ef3d927-631c-47c9-9e0e-a1211cee3294")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4ad82edd-af4c-4784-8f10-a1d2e25e81af")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D_I2-K)")
			(pintype "passive")
			(uuid "325450db-5f61-4bb5-b593-ecb4cbd4f6ca")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(D3-A)")
			(pintype "passive")
			(uuid "1962a02d-367a-4716-9d51-ec8a20ee0c8d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "46739585-07c4-4d99-a6a1-7e72496e6078")
		(at 157.33 132.295)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I79"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "744da80d-b4b8-43aa-959d-ff7fcfaef5d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "6d12c727-c2fe-41d2-8f16-d83e0a291fd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5b84b25-9557-47a2-a1f5-bcbbedf971ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c1e3cfd-597e-48d4-8552-bd3f284644ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/4c09ee73-d5c2-4fd3-b341-2fe8fb1f0a5e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d9785b3-d7a3-42ea-9119-5aa39392ae01")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baacec10-38f0-4ee7-9c20-8f060e3d0959")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aabf0565-855f-4fb0-8b23-af1ff06549fe")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c10b1e6d-0672-4640-82dd-0ae3ee752785")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a9fe25d7-b88d-42e2-a416-ae3375239a2e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "73bc5db1-a0d9-43ac-8644-5b31e5146ddd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c27c0f3-bd48-47f2-ac08-bba76f1664e2")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21473ea8-f2cd-4c0e-8673-17d7993fda4c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf42300f-de04-44d2-96d7-c8546ce911a8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6846de6-3676-41d8-b250-8887e52f1bf4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6bce6c38-f0a6-4918-8160-03ccc2f3865b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 98 "IN15")
			(pintype "passive")
			(uuid "b9d81cba-e825-4fc0-a33e-d00a05cc9756")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "f6de1dd0-8cc2-4177-bf1e-f5b109cac133")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "46d6fb6b-1a9e-49eb-aa69-f076a8580ce6")
		(at 232 125 90)
		(property "Reference" "K2"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "526228a4-4258-4f88-869b-fd8c17b7459b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c8c9c1ae-11a6-40b0-b995-1dc11d3e8421")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "434e469e-103e-44a6-bf3b-a01459125649")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4e12811-bae9-4d78-900d-baab7b97c1f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "69f896f3-3f90-45c2-9a17-70198fca7f35")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/be527b41-7db3-478c-ac4e-ab8ee8ff6198")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a86f3ce-3e13-42d6-8ebb-2c161a51617a")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e50cc4a2-48fa-411f-bb9d-3e49a1c07774")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c0772e7-a381-4833-8118-18e1ce1326a5")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "40985c0a-f5fe-480c-9505-30900398933d")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "61face56-0b09-486d-b49e-75596b48689b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "52b3ffda-1d39-42ff-a250-baf0a0af4e91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "Net-(J3-Pin_2)")
			(pintype "passive")
			(uuid "20aa30e8-7947-42d5-8152-7dc859be9cfc")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "unconnected-(K2-Pad12)")
			(pintype "passive+no_connect")
			(uuid "280dd1e3-77c4-43e5-9cfd-22db8790b74b")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "Net-(J3-Pin_1)")
			(pintype "passive")
			(uuid "0c9d6b8d-e355-414f-b47a-2acd1be2087f")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16 90)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "42dee497-15b5-4fa8-9d9c-4e88f095ad5c")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/PLC2 GPO/Relays/Relay1_A2")
			(pintype "passive")
			(uuid "82cfb183-6f63-403e-ae35-dc973f80ed54")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "486d368f-01e1-4263-98fd-5fb57b823d4c")
		(at 138.33 74.225)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "812bc5f3-fa6f-4e95-92cb-aabb8af1eb60")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ad8455e4-ab93-49be-acba-b008c49815bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "350a1931-475b-4045-9fb7-6a8dfaebdab7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5105806-1646-4911-9514-1d0e702c5177")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/04a1769f-d4cc-4ffe-be31-030578f894ba")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e831e25d-db10-4ab6-8573-aaf41d3b822a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ffb7cdf-8165-4ce7-9614-b12af2729428")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3bde3b56-8d1e-4970-8e63-537376dade88")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ab86f63-6124-4087-b022-44316d53bfea")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f7f7ce9-f80b-45ac-80a3-906ecee252be")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c528ee7-0be7-4c0d-a5fd-54831d110d22")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e64b0c6d-9cf0-429f-9720-479ec8f4fbf0")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "056790da-862f-4ac2-a1f9-0d052955d2fa")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cba06f46-89b2-4fb6-abd9-5578388ae8ca")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48c08787-ff3d-4428-bf4e-7c97ea5fced7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fd72c9d2-adfd-4f31-b97b-769357eddd47")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "d62e6c72-3e60-4a1f-b2b8-2d8375d14508")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D_I2-K)")
			(pintype "passive")
			(uuid "86c4ae52-d820-45a2-9ca8-f7bb501642d3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4a3e7a18-6dc0-4b9d-81c0-5be69e1dfef8")
		(at 147.83 135.245)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I64"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c0b13a0a-ec5f-4336-bc91-16f36dc1ece8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "3c4fb1c1-4b0f-4f4d-be00-192e40a47216")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "174cd315-f2e0-49f3-a679-d44720a429dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "69b45b64-8ede-4f4f-aaa9-94f7e7872006")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/2160d79d-dec7-4625-b871-6446b2e4dd18")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d4c40f5-24f4-4e4a-99d1-17a30f7cc310")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6516f292-9648-4e0d-b139-c3d4d1d52d82")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "402c2402-a57b-43ea-b2b7-cd2c43590409")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ff99916-108a-4ceb-b31b-aded1ee80952")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58de8bfa-b25d-4dee-ad0f-f75a305ba486")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3011e3a-1269-4103-8ae3-4046449d5d81")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12bb6dd0-e522-45a4-8a95-edc4d1fb7e0a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a908f55b-665a-4919-9021-d968583aaa75")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b01e6b4-b3c6-47ce-addf-8e3940b1852b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9869aae3-30ba-491b-9c4a-6eef02e083f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "145f042b-8d1d-4bf9-9d3c-018f206577df")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "4130b773-0c0c-47b0-8e2e-c49da304badf")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(D_I14-K)")
			(pintype "passive")
			(uuid "12c85730-4ee8-463d-8206-38ec4993a4ee")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4aa2e786-a5fc-4565-888c-3f34188ba08d")
		(at 138.33 132.295)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I47"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "317c768c-1c8b-49b9-b5ba-b1cf1ffc3c05")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "78dbcfcd-2253-4f44-a8e8-bc209c62bfdd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1fb04ef-703e-4cae-8eb8-345b445222d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fe72f2c-c57a-4ca0-9d0f-7b6ba33e49aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/42e58810-863f-4832-9a1b-8bb84b2df59e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebb3bbc6-bb38-452f-83dc-eef8f28e08df")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "552fc709-7a25-4cd4-98a8-d417e4769da4")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6e96d5c-6780-4d2a-be62-14d263fe06c5")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4bb18de2-5b8d-46fb-96f9-988387b07f00")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc85c22c-121d-4cfe-94ae-11599a214b37")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac58b93b-d08c-4ada-98b9-3872520d879c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "439bc49e-f7ea-442d-a4a0-516af65dd23e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03afcd43-f0cc-49f6-b545-a08584eef3d6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54aa9d64-62ac-4222-b145-c5e176867bfc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce2ee0e1-5ebb-4326-8d16-f3faa38ddfee")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "42b1ff9d-1e41-488e-bc4c-168fb89776ab")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "b7c62066-9e2c-4416-bb8e-b19f3f244df1")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(D_I12-K)")
			(pintype "passive")
			(uuid "22808202-8dba-41d5-b85c-77f2a42c7951")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4abd1e12-2c24-422f-8887-f833d40d521e")
		(at 157.33 62.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I34"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e8ed7ffe-02b6-41c7-9325-592951b06eca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "85603391-c6e4-46ff-869a-a64fa25e07c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e26c5b63-4026-4a77-82fa-ef2d97254ecc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d92e7a67-e5da-4ee0-9d53-17c058ec0220")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3ed7e8cd-3ae3-4848-9893-c736812ff720")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0d9db66-6d96-4488-afd9-9adb4cea0fc3")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42e25f8f-121b-4a3c-b4f0-1b6ba6ce6b67")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b98dd451-123c-45d1-bf14-7f75da61224f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "631d782e-35ff-47d4-ad5e-703655fa9d1a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97777af7-d096-454f-a15d-dbeb5f156cb7")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5306f29-6d80-4e53-8b22-4001711de5a7")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8012ffce-a5c5-41d8-be8e-8516a3f4ad39")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7037afbe-edd7-4c74-8b70-62c03e073dc5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c91156eb-b414-4757-9b40-ea7c1c100f43")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce28b8e5-9a0b-4f13-81c4-034027ff7b7c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3f44cde9-a87c-4a49-b2fc-6ca646f114e0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(D_I7-K)")
			(pintype "passive")
			(uuid "3982313b-3899-4650-b18e-d1edaa1cce06")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 19 "Net-(C_I14-Pad1)")
			(pintype "passive")
			(uuid "0011bdb2-e2f7-41aa-a96f-1d01f61d4e6a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "4c132a88-4934-4c1c-bdf9-f3329e9ae9a5")
		(at -0.7625 64.28)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "JP1"
			(at 1.27 -2.38 0)
			(layer "F.SilkS")
			(uuid "13a224ed-783b-4d13-8571-9b1a274b3f75")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_02x03_Odd_Even"
			(at 1.27 7.46 0)
			(layer "F.Fab")
			(uuid "812ec18d-c8e7-41aa-aa5b-a95b34ab8943")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f7c04e1-7ab2-4e73-8f60-6ff0e0fa4c3e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f93103f-66d9-4c00-a7c3-69efc5379340")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/e75ede96-df16-48a2-b3d1-cde9ff312c5f")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.38 -1.38)
			(end 0 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ec4d34a-b637-4e04-8e1a-2dfad86f50c9")
		)
		(fp_line
			(start -1.38 0)
			(end -1.38 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0838893-41b8-4173-aeef-b53c7174c263")
		)
		(fp_line
			(start -1.38 1.27)
			(end -1.38 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "809692ca-5f0c-487c-8e14-37277fdd7974")
		)
		(fp_line
			(start -1.38 1.27)
			(end 1.27 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bb76f09-821b-42ae-9509-8bdbb0859031")
		)
		(fp_line
			(start -1.38 6.46)
			(end 3.92 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3376b0bb-4a64-40ed-81c6-76a042416eb8")
		)
		(fp_line
			(start 1.27 -1.38)
			(end 3.92 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b6e5b09-3763-4fe0-a987-183017f9983a")
		)
		(fp_line
			(start 1.27 1.27)
			(end 1.27 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7761aaf7-5353-493e-8e07-4c6efdb0979b")
		)
		(fp_line
			(start 3.92 -1.38)
			(end 3.92 6.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bbff2f5e-d4af-41df-84a9-da2780fe7849")
		)
		(fp_line
			(start -1.77 -1.77)
			(end -1.77 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa5dc842-11c1-4d7c-a67b-c4445068d415")
		)
		(fp_line
			(start -1.77 6.85)
			(end 4.32 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9795851-9cb0-40e4-b6c5-6305ba672ea2")
		)
		(fp_line
			(start 4.32 -1.77)
			(end -1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a79424a4-163c-4597-8720-ecc383f14797")
		)
		(fp_line
			(start 4.32 6.85)
			(end 4.32 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "174b09c6-9301-4411-92d6-07ca1e870e98")
		)
		(fp_line
			(start -1.27 0)
			(end 0 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2d4a3d7-cdce-49c1-b201-b99eeb7555fa")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51c7f638-cc51-41a3-91a3-fcf5849168da")
		)
		(fp_line
			(start 0 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f859aa23-eafd-45e2-83a0-2d0a8834900e")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b890a35a-4f8c-4848-8295-2e6bd204b9b8")
		)
		(fp_line
			(start 3.81 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bde01563-3881-4771-b061-1a5d3d578647")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
			(uuid "afbefc3d-6be6-47bf-9ced-90d82d717116")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "EN")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "9a479b1d-649f-42ac-aa49-8c94abd17bc8")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "44a51928-2ee5-4559-bcd6-4a2b3657bf84")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "TXD0")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "11e94207-58f3-4e70-acfd-9413d32a3cae")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "05b80ad9-4f16-42f9-83ea-bf423aee80ee")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "RXD0")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "d05aa214-dc4d-45f0-bbb3-5bc21c281760")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GPIO0")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "cbbd0200-bc57-4bdb-a7b1-98a07d00e135")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4f7337fa-871d-4d91-87fc-ea6a1e40f36c")
		(at 148.765 90.96)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D15"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c51ab16b-cf81-4c5f-877d-b34e533ddfd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c9d59514-894f-4a11-a71d-0cc7d923a9d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b8845283-55ec-419f-9b05-181c1504b337")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4c639bf-91f6-4470-bb8f-f4fc84f56b63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "316bddcf-9de7-44a0-851d-d9058e76eac8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/a7f0e543-0bb5-4d7b-950e-b400e8186bfd")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0571a449-919d-43f0-a447-9b1bc58d4c6e")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2053fb92-79b9-4afb-84c4-45ba336463ff")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e743e3f1-7332-43c1-b084-14aee48b2f92")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a0d61c3-421c-4b39-95f4-e739470beb96")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11e5cd47-bc5f-4fc9-bf76-863421f1ed26")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7d06aa1-9a92-4e51-ba17-0c5a76cf8076")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94ad7f41-85c6-4f37-8157-d0fd4197c09b")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb5287d4-72d9-4f8d-a965-4ca1d75b95f5")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47d61696-969d-4e26-abe3-170c7c11b7a3")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b26629d-452a-4a17-9085-8ceae01da584")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54a0f14b-7e5e-47d8-a4d8-8c158dbdbe92")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47affffc-be52-4e26-816f-55bcfb4ab639")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1ec7e934-6f1b-4702-84bc-c5607ae63838")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "20eda70d-f651-42fe-9d28-693e6769ff8a")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 47 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "78e2fb7e-e2d5-41f7-b8fb-56706d01075b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "4fafbae0-040a-459c-94a8-654f6aaffa00")
		(at 126.76 33.325)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "f924bef4-155b-4300-aceb-bd551d417a00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "d165336c-0335-496c-a046-c85abbc2ac43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f050a3c3-7d9a-49b6-90ce-838d6d3df627")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6303545a-d61a-4202-9189-90bcd6c63b6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9762e82f-daf6-4416-82a0-8abf980ed190")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23c7fc9e-8c49-4b9e-a7b0-442e6bdfacd0")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10f49cf3-4ef0-4bea-b6eb-79e140371b2d")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c9bfd84-7384-4dc9-9d2c-21a735e67831")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d020da8f-2fa1-4354-aa14-13ec267796bc")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea568ba0-84f5-46ea-9749-5cfb320f3bdb")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a8984fa-768a-4c2b-9d98-005e86c91187")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1f5f62dc-ed25-4207-bf00-66ca17d9f719")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81b5995f-1bbe-4043-b6a5-e3b899f4b4a0")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be1ba9e6-ad0f-49b5-8b62-7fd7d7f9222a")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f845801-69fd-4d49-b2a0-590fa011f012")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d0b9264-0d83-4cc1-ab00-c477468fbfc5")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "361396a3-96bc-4824-ad54-07e90ce96363")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "0446e997-a7cf-4fbd-8fda-e3de7c8f2033")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 9 "Net-(C_I4-Pad1)")
			(pintype "passive")
			(uuid "abeff5ca-ccb9-4d7e-9716-0eeed37af2e9")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "df5bf778-2aff-4d9c-9f8f-ea59f1ea24bf")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "6e0ce4bc-ed3a-41ff-b4e9-005fac709dbd")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "IN2")
			(pintype "passive")
			(uuid "35c7ece5-f1b4-4f75-9e86-32da46e3cb11")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "52a59ddf-d605-4e2c-8d0f-82bdf481dcee")
		(at 153.54 41.815)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "46cdd50f-8c39-439e-9d61-f0f6f2af6691")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "6966bb2f-a2d8-4ebc-9ed0-da2e6cfaac1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "112b2042-7eef-466e-b29b-9ae2882eddb5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a90cae5-d343-4940-8ae2-94f1cbc903e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/2f1ab314-f2c4-4aae-9082-f9c5ffdb6a86")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1668337-5fd9-433e-a1c8-ae714c6e8529")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "493850c1-ef75-44aa-a702-02494a18d83c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a05256ed-2fa8-4853-a2a6-cfa728827087")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1effa75f-ae2e-459f-aaf8-397d2979ad75")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6531a566-fa4b-4f37-9fa4-87d0b68ef8d2")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8155cb86-d224-458f-85ed-078b7dd840c2")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9643a65-aa6d-43fd-83e8-d17437df7343")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52a2805e-8daf-4bf9-bf25-1e0cc4f9ca27")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa1660a6-adc1-410f-9e23-d0df534f64df")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f23cf322-5392-47ff-928c-786c81155fc9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b43e0a70-5f7b-4c5c-9869-454d8e10805c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "Net-(C_I4-Pad1)")
			(pintype "passive")
			(uuid "059ef242-2375-45b6-948a-d763e554c8c9")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "a6d51d15-24d0-4364-9020-2be0bffbec5d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "52f540ca-e2cc-4291-b68f-0a4739e1b17a")
		(at 147.83 77.175)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I23"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e10f238e-0fe8-4a62-8c2c-f3ebdefda812")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "fb3e5210-048f-405a-b6a0-c7c8bf545dc4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "36117e94-e2f1-4bf4-9a46-33161d0bd089")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "abffe14d-339b-43bb-849b-51c42640e0ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/ac501c0d-5686-4685-af6b-cbcdec1a3829")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6eb39e0e-c04f-484f-a49b-57e4aef78e68")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34c1f4e7-4d21-4240-86c1-477241883d50")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6042476-f954-42e6-b059-7875e21499cf")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74c44fa3-4204-4a4c-ae0a-30504dc6273e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae3146c0-5221-4ca6-8e22-3054cebcefc6")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26bcf882-f0d3-4bb2-ad35-ec64ce7dc32c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63a81318-1ca6-4498-825e-d46e46f8070b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "462c9d3e-ab7d-4099-80fb-75612e01e5e8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f1b6a22-20eb-4e39-b1e4-a5bd8f6a21d7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73a59179-2b60-4614-8597-a0263047edcb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "959cd384-8452-445f-9021-2cabe13a5900")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(D_I5-K)")
			(pintype "passive")
			(uuid "9cda4d53-283a-4f7d-9a9e-4930933dfc73")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 42 "Net-(D10-A)")
			(pintype "passive")
			(uuid "38cb77b2-bd34-4f82-a258-f11635845546")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "52f81a4c-9e03-4a98-ae68-b911b1f76f4f")
		(at 158.35 35.795)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "c4f1b8fc-293f-4cd2-924f-46df8770cd08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4c40a194-a248-4929-ac97-298575c1d2cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f35dd984-83c5-487d-bde5-fbd0295e52e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "15aa1df7-6150-4cf6-8d89-5e6d87203d54")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/316faabe-2e21-4fe2-af31-ace2b5379f42")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c46f044-6d4b-4134-a90e-685073f56fc7")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7bbc211-d6c3-4e9d-8e97-e298ee1db9d8")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8f23680-bfe0-4cf5-80b3-c8272c36ed16")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "567de8ec-a8d9-4416-ada6-68db076de33c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b3e1822-f5c3-43e8-8711-828302fe7313")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "417973ee-4852-4b72-a1f1-aa76773280f6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1cef7f7-57cc-45ee-98c1-aa9f6e8be88b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8dd762d-b2fb-4720-b2e2-7253cc025ed8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "261577bc-16ec-4647-a110-2bae4a844de8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b19aeedc-3084-49d9-b930-d96d1d3307ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "26217b00-a00d-4864-93d8-17fff02f1741")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 13 "Net-(C_I8-Pad1)")
			(pintype "passive")
			(uuid "bb4c7421-47d7-43d1-9de1-4aaf60a9c092")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "d28a6557-f78c-443f-b6e8-212acb007768")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "537345dc-7664-49fe-88d2-5ba84059fbe1")
		(at 6.4575 69.36)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c1f0ded7-cdd0-48f3-8693-fbf4bbad217c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "120"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "bbe894d2-54cf-4f4e-a4f0-f6854efd1528")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a842eacb-ad81-42b0-82c8-ec1c0c36464b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "237b2716-6eda-420c-bd60-28d253b25e04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/8a68a1f6-391d-431c-83f3-1beb5da5c9af")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c32f6cf-b263-454e-a518-4ce9c3849a21")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f22605c4-00c7-486f-9e86-d624a9e7211e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c9db692-4cc0-4423-9cf7-14911bdafc58")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df1ce0b9-c561-410e-8945-7c4790ec53a0")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77e78507-3cf0-4243-bbcb-b67ee612bd6a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07f03ede-6853-426e-a276-25e328c59221")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ccd659a-be2e-40f2-9aae-f7ccc9c37dba")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74c3d0f3-ae6f-43a0-8f4c-f5b975457154")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3de74924-f8de-423d-93c2-0516b108ce5d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b177ee86-70e9-45f1-b7c8-3eb584dabb7a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0ede8ba7-b87f-4f52-a2ab-e8b52254d15c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 130 "Net-(JP2-A)")
			(pintype "passive")
			(uuid "23396177-4d23-416d-bf91-020449a6a88b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 114 "CANL")
			(pintype "passive")
			(uuid "d22484dd-75db-47ae-a570-ed1b762633ef")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "55360159-e5dc-49ac-ba05-91dabbb2791f")
		(at 147.83 117.545)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I58"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "036ba481-b541-429f-a666-5efb1d08e219")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "38106458-d204-4269-b933-613daaf8e144")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff6f3c33-4f4b-417b-9796-36fa694edac1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0076c032-511a-4dfa-8a64-d11e7628aa47")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/fe62f70d-9065-4daa-8465-d9d490ae3f30")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fecfb975-2159-452d-9fed-f5c1729e0e7d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22f5e8a4-2945-40e1-9c43-50e651590800")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68cee9fd-890a-4a8e-9619-0bdd51929a90")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c15d5a35-776a-43c5-9825-168dedad3bfa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "250de9a5-feba-461f-b4dd-ca7ca2d07af2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b0a0387-f760-418d-9cb0-bd40b767fbef")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "442211c2-86cb-4704-81d9-5a42bd3edd9f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7065e6a0-a6c1-4399-81e0-936432246d73")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eae60248-73fd-4af6-b0b0-2ae09d4cd54b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8303e367-2428-46f9-a4a5-32d70936df79")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "20e3a980-b0c3-41c8-b095-07575f379acf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 77 "IN10")
			(pintype "passive")
			(uuid "c2cb00ad-30fc-4288-900e-95c78402621a")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "b855a56f-1f06-474e-ab4b-bbf589320ef9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "56fd4fec-3d77-43bb-83c0-edeb7ec14da6")
		(at -23.0025 105.695)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "261fcd01-6d05-44b2-95ea-558329b3d1a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "3465ca1f-13c3-45b2-a1b0-617bf856cb23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5b78cc0-4595-4582-9dae-4d4c3854a7a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "805ac7ea-840f-4069-87d2-786a1f38cca2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/a1e5f5f2-a6d4-4c83-8056-ca09e7c4d51c")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.91 -1.56)
			(end 0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f96cac9-ba39-4c2d-a557-bd7e2d6e51ae")
		)
		(fp_line
			(start -0.91 -1.51)
			(end -0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c69e952-a5b4-4ee3-af68-37fc037a0123")
		)
		(fp_line
			(start -0.91 1.56)
			(end -0.91 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49cd4269-42ff-47ba-932e-89e2db349b39")
		)
		(fp_line
			(start 0.91 -1.56)
			(end 0.91 -1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4eb03025-e250-45ba-aa9c-5c0c7d5eb0ca")
		)
		(fp_line
			(start 0.91 1.51)
			(end 0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5bd38e79-31c3-47bb-a4ad-6a5229e18d22")
		)
		(fp_line
			(start 0.91 1.56)
			(end -0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4fe78c9-02e9-4a67-9db2-8f506b590f49")
		)
		(fp_poly
			(pts
				(xy -1.45 -1.51) (xy -1.69 -1.84) (xy -1.21 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "08c13b75-9d6e-4693-a9df-744b0df4ee09")
		)
		(fp_line
			(start -2.05 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d238bf57-b4fa-4cf7-84ba-77e495ac93bf")
		)
		(fp_line
			(start -2.05 1.5)
			(end -2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27b2acc9-e166-481c-b1c3-666396ea64f1")
		)
		(fp_line
			(start -1.05 -1.7)
			(end 1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d007ad9-2478-44ba-83f3-ea762a5bb80a")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab1c44d0-40ae-46cf-bf56-736f38272518")
		)
		(fp_line
			(start -1.05 1.5)
			(end -2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f0bd8d5-bdb9-4849-b852-babbf00d7490")
		)
		(fp_line
			(start -1.05 1.7)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7b31711-5dc4-4ddf-a87c-f46cead64ae2")
		)
		(fp_line
			(start 1.05 -1.7)
			(end 1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d8b9ae8-f2e4-4340-9b1b-410decfb1371")
		)
		(fp_line
			(start 1.05 -1.5)
			(end 2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2634d5f-83c0-42be-99ff-1c5fab195762")
		)
		(fp_line
			(start 1.05 1.5)
			(end 1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6dbcec0c-5cca-4eea-b9c0-4632e7abca1c")
		)
		(fp_line
			(start 1.05 1.7)
			(end -1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bc07c8e-feee-48d9-a70e-e592a7173f4c")
		)
		(fp_line
			(start 2.05 -1.5)
			(end 2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38b275d1-e58d-4468-8c6e-d31f7e6abd54")
		)
		(fp_line
			(start 2.05 1.5)
			(end 1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a18c46f0-45c2-4056-8c09-4d34f5cf0563")
		)
		(fp_poly
			(pts
				(xy -0.8 -1.05) (xy -0.8 1.45) (xy 0.8 1.45) (xy 0.8 -1.45) (xy -0.4 -1.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "443d6498-b189-4e58-8d60-488780fa1b75")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c9277c55-4f70-4c25-8775-da3968a31ab7")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(J1-D--PadA7)")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "7221e908-6f24-4a33-a787-cefdaa46594a")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "2561135e-0b1f-415d-aa50-b9bd89cdfde0")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(J1-D+-PadA6)")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "9d5a9837-f025-486e-8cde-ffb2d8f54709")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "D+")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "2de1f8e3-23de-456d-acba-6cb02483e39f")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "unconnected-(U1-VBUS-Pad5)")
			(pinfunction "VBUS")
			(pintype "passive+no_connect")
			(uuid "a2acc8a4-5181-4e3a-8810-fcf3168d4dda")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "D-")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "8c3d811c-d8cd-41f1-9da5-f5312236d677")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "57d80761-3fc4-4c13-802c-4f8bd3c1f5d4")
		(at 152.58 68.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I28"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7ed04aed-a41e-4461-add5-77549844097c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c7d0a6f2-423a-4096-adf7-5e8c6f83d569")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0e2b240-8e6c-4eca-b4f8-1ed5a2565469")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bb4bf51d-be92-45bd-be61-0b08193c25e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/d9eca52d-f3bf-4d18-a290-168887b0489b")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "499afad0-344b-432e-b46a-293e58501ba9")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da302b28-1f68-4eed-8fcd-3f798e9575a5")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b359443-895d-4d2a-8a83-f4aabc1139bd")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7572644a-8ff2-4b48-b3b1-a178fa4fb395")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8fa44925-43a4-43b8-bc48-3478e267e5a5")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98c5a372-e365-493f-8702-60cf0737b495")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26745699-e2d7-4665-b062-30a32dbde2ec")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cc805b0-5231-4b5d-bee2-c4a11c0534f2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94b991b1-fb05-46b4-bbd1-5ce37d19ffa8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8029a756-926f-4f6d-9706-886ec15f6dd4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a6250271-74e8-4712-88c4-4a2b8fdd710b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D_I6-K)")
			(pintype "passive")
			(uuid "658699a4-7ff3-42b9-9d42-321e8c30ee2f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 43 "Net-(D11-A)")
			(pintype "passive")
			(uuid "95a6863b-4b50-4085-88f9-c5f47c5393b1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5a86d50e-5652-4d75-86a4-79d21a7f49f3")
		(at 147.83 59.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "23df756f-4bf8-4076-9d01-85eb2e28e717")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "df226adc-c682-4742-962f-573d2bd9e0e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7eb88fb9-4b0f-4c6f-9859-98b5bc621642")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "54352f52-f2a0-45f6-8696-7371c68a9c6f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/86205a9c-708f-44e9-8a8a-f8b7e4e8a411")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23df0b0f-e63d-4461-a18f-4cee4fa417cb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa50d781-f52e-4376-a474-6db5f60bc8cc")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "215d05e9-0077-4bb9-9955-58bc8e4ce8c0")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e50a4074-6021-4d4d-9441-29d2bcc7c4a9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41d77108-820e-4375-8de4-925c14dfa32f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e908966-37de-4ced-b902-2cf595da46fb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08ca37b5-0882-4282-8b60-499f332d153b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16917d7f-e1cb-438e-bb42-380f6b115aa6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b740157c-064a-40f3-8625-4a5fac31a46d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a350fc18-d676-471a-a4f2-3d80af59b2c5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b8517c31-470c-450f-8af0-acb1543aa4a0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "0db481c8-8dd6-4fa0-a61d-c0f95e4f1f17")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D_I4-K)")
			(pintype "passive")
			(uuid "7be8b195-87ce-4a50-a009-f958bf949143")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5ac4402e-6965-4a95-bf8b-dee91f8322c1")
		(at 143.08 114.595)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I49"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "82f2ef72-a9d4-4b05-a960-67c298a8e262")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "aecd025d-1fe8-401f-b8df-0d9e02ddb35c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c69d6f84-79ed-4bb0-be00-19e7aebb99e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9fc799c5-30ff-4cf1-bc93-f3b26537b97c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/dd299bc4-dab4-4597-a7c1-c69142eeffc4")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56c70be9-1d69-4db7-92a9-71c1a59d3bcc")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "223a9132-33ed-4c01-bda2-f6b696acca01")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "81508dac-a194-48f6-8dad-6ff0a7758993")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "306a7d59-d5fb-4015-b24b-bb7b36e53539")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "32f3b6e7-40d0-4325-a7c3-4199e82c7403")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95c6ab1e-9501-48e1-acca-7d3b596266f2")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00d57fa2-d977-4eb6-8fb4-1091a2a51b08")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "258bdb62-8b18-45ef-bec4-28e02e441406")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec9153a4-906a-4e01-8d51-10358d001d7f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d926b84-c1b1-4681-9591-9bd6a003d8d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ad84a530-1b80-4e54-9419-2c1681f19906")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(D_I9-K)")
			(pintype "passive")
			(uuid "03acd86f-a035-46b1-a852-655a84cc9e28")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 46 "Net-(D14-A)")
			(pintype "passive")
			(uuid "45c5ed22-90f3-4e8a-bc0f-b7f7c53f9ed8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5b177ce7-7caa-4e2c-a0c5-f387ad0b3ab9")
		(at 138.33 68.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d92d2832-437a-4d2c-b0f0-803910cbade8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "8aafa84a-02f0-4dc3-b2ed-e60cc97cd1b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "440297cc-cd18-4853-8b32-666f26975cb7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6576e79-f394-428e-8602-6ce2bab667af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3e7da175-e63f-42ea-a70b-221f2cf0d821")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65f2236d-db11-4cdf-bab8-9caa3588b8eb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d0d10b0-8591-4717-aa6a-06836ae7833d")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "677ec4d8-a0c8-49f2-b6b4-3c7657d7f60f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7116c8b6-a8d6-4d59-94ea-34330d70e34d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b16ddc4-edde-41e5-913d-f0c5e4a423b2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39f568c5-3992-4a5f-97d3-efda1813d49a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a463e458-b116-4a10-bd66-61f37318c25c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bb59371-6e34-4bac-93d0-2593f65ab117")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad34695e-2704-4185-9d77-5b19b7c91f4d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c276f93-37a7-4406-88ab-95fd3f938ed1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6101fa56-d261-45ed-ae4f-ffd5b5c67246")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 94 "IN1")
			(pintype "passive")
			(uuid "63c48d9c-c1a9-40d5-8a3c-d7036f4c2ca9")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "5d94beae-fb5d-4cff-8fa8-b81053a73344")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5b6362ae-cbba-413c-9988-e700df6fec3f")
		(at 138.33 59.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "4c3e140e-4a46-4f62-8747-e85b411b055d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2d92a1dc-203d-4a33-9e6e-3b05e7eb8e99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e802604-050e-4775-8282-dc02e2b2aa37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aa60ddcb-f2c0-4341-95bf-4603b985e232")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3392d5ad-c8d9-4249-ba01-561de6c50aba")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40b365a6-a7ef-4399-a7b7-094cf4ffe38f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8629113d-bcdb-49f9-95a1-250468aedc22")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "960ed065-620c-4724-a5c1-6513b733b2a9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33759011-1fa4-48be-9a2c-2d9e1187526b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46df48b7-caf3-47f0-aff2-d21f76953b99")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4db8cc77-f2ab-4a8a-9cc6-6d558594305d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7061e1b-3e95-47a8-8a0c-4c9ee91ebbd8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75a66171-0b61-4ec8-8e22-7e7dc124c51f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83db5408-cef4-41e7-8d8d-261541e6f459")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "292381e6-fadf-40e0-b121-c47eb910e1e1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0ace1561-9e1f-457d-b2bc-40bc8275eaa6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "a240827b-0401-480c-8d18-49b4ebc5a471")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(D_I1-K)")
			(pintype "passive")
			(uuid "b871c465-3b9b-40d3-9635-df02c44e5b1d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5d5f554c-6bb9-431e-9551-e4a18f19bdfa")
		(at 6.4575 66.41)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "8072adf4-4b02-4bae-9e7f-696493b7cb5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1k 10%"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "25747f0f-60c5-4887-9e47-5f14b9abfaef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd428e65-5ffb-41f8-aeff-9760e3ebecd9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b86b98b-c21c-4abe-9e35-4a9a0a8ea2f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/58e3b604-2e10-49c5-a726-dbb4db0ab34c")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bb10843-6fb4-471a-b341-aed8741b4b78")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16cfd570-b703-4128-9e83-24d732de9d37")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6642155-1a37-4fac-a6c3-3df47d6a87f8")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbd5b166-59f3-4ff5-8a4f-04fb9a973c97")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7cb931f-cb93-478c-b1bc-cad3b788456f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b31715fb-2a49-445b-b905-36bd6c3e29ef")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e62d44d-b5fd-4dc2-afb0-4e97e1fd799d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d818191a-e92b-43fd-88f1-c5aae3a068e7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81da6b4c-43fc-49ed-ac49-fc7d968da117")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bca63463-0b95-4e29-b288-3ede6103e269")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bb52a75a-dab6-436e-8088-fefe6733a903")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pintype "passive")
			(uuid "c10f475f-6f63-493f-a071-99dd7a8c80c7")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 102 "Net-(J1-CC2)")
			(pintype "passive")
			(uuid "630d7c6f-2cb2-42e5-aaaa-165b2aa10e7c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5df36641-64c1-4e5c-907a-2fa5004678a2")
		(at 152.58 129.345)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I70"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5110e13b-4e09-433b-8597-1c11e715f854")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "024e8545-f1c6-4547-8519-1cb635e08e39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ffa1a78-bee7-4cf9-bcdc-1fd2681a37db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "00cfaf91-a6a4-475a-a143-9e6abebba30f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/bf84a4df-65b0-491c-bd60-0d62a6f248b2")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b2b888c-d647-4e41-9964-7c83d4d3f4f4")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b19bbc3-4919-491f-b698-e50ed87d4d8b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97f07353-f374-46c3-82f1-8a8de92103d6")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e5496c9-ec81-4e4a-91b7-998f1a4afd93")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e4219ba-5498-4b42-a9d4-fcb06c24a3c8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fedee67b-b4a7-47a0-8a24-924013546781")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7bfc849-af20-48bd-ba99-55dafaa82261")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7673002-5817-4c46-be5c-673d0047b1e1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "526b0271-e739-480e-a6ad-c9525e422cfd")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05209bcd-3759-491b-9ea4-96393d36b00c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "355b9aaa-7ae8-42b9-84e4-62ba1774b083")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(D_I13-K)")
			(pintype "passive")
			(uuid "664fda68-1533-47ff-abfc-eff1859d6ac5")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 34 "Net-(C_I29-Pad1)")
			(pintype "passive")
			(uuid "a8df6293-4f39-4c1f-af10-2e4071d91414")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "5e515383-f6a6-4706-bde9-6013647a3cd7")
		(at 158.35 99.945)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I27"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "7c180b17-13e6-42c7-8284-430524de0030")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "9dc72f34-4b5a-4e11-b09a-f2715713e321")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "45048b4c-45ef-4c31-aaed-37f63e5f041b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d950b0eb-ab12-436b-809c-4cc2c2d06e63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/f7bf8446-edd1-4e78-b390-e54a2b781fb9")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b41b55c-91bf-473e-8dc1-54568faae96d")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac61b3fa-d6ec-49a9-8cb7-1e9f2f249e33")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72aa86ca-a84b-43cb-981a-b95ec3be9f40")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61ce6286-06ed-4e6f-bd95-a4e272a04ca1")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06110c47-8eb4-4185-b0e3-3e4c897a4445")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ebfe4c6-40dd-4a41-a394-879ffa3da9b7")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e42d8f48-a952-48b2-a70c-98bb177fabc6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e181b4bc-4aa9-4ad2-a967-328a904241d6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fb62cf2-f6f1-4ba7-bf8a-f7a6272a7e2f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75130d86-520f-4d0d-bd6e-0edabbad580e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "09686f78-ebc5-4fb8-b83b-fe5794aee95d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 32 "Net-(D_I15-K)")
			(pintype "passive")
			(uuid "acf19f73-1594-4f2e-9e9c-b365292b2cb0")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "b8fe2d1a-493c-4f4e-92c9-8750743f3d72")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "5fe4b921-c0f6-4189-bd9c-db9b64fff2f7")
		(at 153.54 44.825)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "886840fb-96b2-47a9-b0c4-af13789ec8ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "dc7b9ddc-5420-4ae0-a646-27bf5f79ba25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "69ef9444-558f-4c02-b61b-1ecd3d2bf75e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6a048a1-9262-4d80-a6a2-f8e79dc16cad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/dd5a0b0a-7b59-4941-952e-d6a06a1c263d")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2daa0fd0-3384-4f1f-9058-844d726ce664")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bddc039f-6d34-43f7-b7e1-a689cfeb0f46")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b34db2a0-4042-4d7c-9a6c-1398eee798eb")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2192b14-645c-4d9c-a738-fd943224e2fd")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9875fc5d-f245-444e-9068-454e41e95f5f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c76823c-39ca-44f0-b8c0-a660257b1dac")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a295177-1dff-4c17-a064-d1f3542ab068")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "487efc27-7423-4b36-b75d-d83b606d8d97")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c9e6f14-c09a-4988-ab87-61af503d91bb")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7b43b56-b10d-4c01-9759-a72a32f465c3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ff7652ce-7480-4e15-873c-3767bb675b15")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 10 "Net-(D_I3-K)")
			(pintype "passive")
			(uuid "3f6d128d-2313-44ac-8d80-eaef45f82356")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "0a5bc1ed-f7db-4b76-9220-879d7ebecf5b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "61ae57e8-bfc5-45c4-b42b-85b448e02f0a")
		(at 148.765 100.08)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5018c747-e643-40a0-8f11-ea5af283dcc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "803cbdfd-c74c-420e-9cb3-66ebf9a7695e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "750b20c6-b419-44d7-8af4-05f81d624f6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7076e011-9ba4-439e-a1d1-643e97921b05")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "71203ecb-1858-425e-8583-a6d2a10a36a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/5be7cf34-6288-47e4-b94a-5512f4120910")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "add22733-80e6-4ea2-9c56-449ebbaa69d5")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6cd89a52-0b22-4820-a4db-4370cc3a9b88")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3344ec38-cfd4-48ba-98ef-c715811c668c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ebc02de-854d-488a-9fbf-d610194681a6")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "846ce3ab-ce80-463b-80be-76e860e83d78")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "81fe4c52-efc7-4a18-810e-5f35ddf22845")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c032524-5511-4520-9903-faa5c0ce85ee")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fcc8171-3024-40c0-a9fe-0ceae4a6083f")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32107989-5445-4c45-b54d-96b2ba686529")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e831d46b-8ce4-481b-95c1-4fce894fd6a2")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f248b4e-ea04-4a23-8260-bc2abb77cc61")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cfaef41c-67e5-4077-a5ae-f5d13590267a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eb6f944f-bad6-46bc-b6e8-4eed8dfc8dad")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "16e2548e-cf67-4a83-a7fc-6ea4fabc06a7")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 50 "Net-(D18-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "fdbc6bfc-c356-4189-b4b7-59beaf9f8ae4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "61f84ea1-da8e-4c74-9c27-4c6ff6fe415f")
		(at 138.33 123.445)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I44"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "795e874f-0ae2-4afa-b8bb-3e4272346772")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "3c0b9557-df52-42b4-93de-57d1bdd9abbb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5004d0ff-663d-422f-895a-62d66e0c641f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "56e3af8c-da72-4284-a95f-824e02b7172e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/75138a52-3b8f-4d34-aa2f-f2e1148a2c0d")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "144aa13f-9327-4bab-b9a3-8f2bea1ca59d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8d6b78f-8202-4f33-b3ab-013ee0ec064f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b7169ba-4b94-4b87-aeb6-047c59288bd1")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4d42335-aae8-42c4-8cfe-48b38341f6d6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f10726a9-b39c-4678-9579-d3c4e771f45f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4c1de35-725e-4bf4-a183-ae252dd6be9b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5be0a2c2-6434-4177-8c81-6489d7fb5d77")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e68654f-9934-488b-96e5-f3b3b014b727")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b7c2350-57f6-42b3-b890-14e171733712")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c164a8a9-f04a-4c4b-8d52-c13e29361ee5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "413e5c7b-1c12-4047-a0f6-060433a28670")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "32652111-4c95-42ae-986a-4256731b0574")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(D_I10-K)")
			(pintype "passive")
			(uuid "9d3f1f0d-02d4-4c98-9770-257bcffe528e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "62849463-c9c8-44f6-977c-a2b5d9f8d525")
		(at 152.58 65.375)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I27"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7399d219-513e-4d94-949d-15fcb21ded9c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "439071ee-f505-441f-a60c-e7b0666bc1e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2032648e-db5c-4934-bc23-c7ef1a13cb25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "147a7853-789c-4f94-a8de-d70ac8d46974")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9593baad-bb02-4166-a600-34df186beff0")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3e2b443-d886-41c8-b05b-c572d9d3053f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c89ca64b-383b-43f9-bc6f-958e6ba20fa4")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52f8bef5-58e6-4563-987c-6386742edbd4")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d941841b-5a57-46ed-a4ba-3aeb67bc8a62")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3055895a-ddf5-4f84-9056-ec273b3121a2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7eb0b26-43f2-4722-8da1-148dde1a1bd4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ed96f99-4727-4553-be5d-714a2732bc15")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86377991-86b4-40c2-8361-35985eda9cc7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e6cd570-1ad3-4b99-ba34-646309a937fa")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "002d93d4-23d5-4db6-98bf-deb415bf4bd7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "22e0110c-8842-4948-b3ca-cbc1eb5e5f52")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "799fdbde-4a60-4035-895d-5ae872fe680c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D_I6-K)")
			(pintype "passive")
			(uuid "b54677b7-2b3c-41a1-8234-c2d68b92ba5f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "62b7fc63-dbd9-446d-aa8a-acebb239f030")
		(at 126.76 108.365)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U20"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "a9adcbbd-d5b3-49a9-8019-9688ec693836")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "1eb92f1d-5299-4ddd-af66-769c9a5b5e65")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0de86a45-ad49-4a6a-b58f-1d56b5b2fea5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4709285-9a78-4c41-b26e-532d45e4569d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/9c26c74c-fdf0-449c-93ad-95c67a86969c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07fe0caa-3a36-4f8f-b312-99a7c1612a13")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dabacc4e-c795-43f3-af77-3d225b926fad")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e839a1d0-f9bf-495a-ad94-b389a79248c7")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a7eaaff-9c2e-4bb6-8fab-67b216802452")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a66a3d99-c4fe-471b-a98f-52cbf1992c5f")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd048882-41d5-4055-8d52-f56c2508039f")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "edfafb8a-5261-4c8f-9b59-9799d7bc90f9")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa3c8e15-b9e0-48b7-8375-fef8d3605841")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89a4eccf-85fa-42a2-bb2c-b37383e87c70")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b93d18c3-66cc-4408-971e-4b969c96b779")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d98023d-dda3-4960-a2b0-20e226ce289d")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ea0587c-127c-49fe-9f85-93051504dd78")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "0bf6152b-bccc-4ab0-97a6-69326130b36f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 29 "Net-(C_I24-Pad1)")
			(pintype "passive")
			(uuid "6e6a66f8-ad5c-4097-8552-4b62def7f750")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "704b0788-e1d3-4ee7-94a9-88778c15e9cc")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "bdbe3611-499d-4a4e-ad39-47a75c85a489")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "IN12")
			(pintype "passive")
			(uuid "d78baf25-0523-4d11-9fe5-3b6d6b311053")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "6316f9bf-c0ae-428b-87ec-63a73c3e9789")
		(at 152.58 114.595)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I65"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9c7df332-8d7d-4987-bad0-14bf56260542")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0ca90023-7891-4742-8c3b-b4bea850fe3c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b304783f-c765-4c13-a9ce-4915232071b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "393ffdf2-9da8-4be9-9869-0f2cbbeaff81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/957c211a-ef6d-4829-af21-68a0baf2184d")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d84b786-be73-4365-abdb-572312a2a184")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4c13493-95df-4653-8d13-0ac671da2255")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6152942-050e-4155-8c99-711284e472b7")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94454018-a272-4691-8b7b-5246ae5e633f")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a3354b9-7053-4fdd-9d3b-4e8de306b5da")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd5b1747-782a-4aec-9041-4c4a36fd9894")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "984e63a4-85d4-4655-a484-2066c228648b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d7e5e09-6ad3-4497-8068-f0b1ba9dfeb3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccccd399-3c4e-4c8d-bcd5-b71fa464370a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef2155db-b08e-4ab6-90b7-5a11697b16cc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "63e35115-1a72-48f6-b5c3-fac8329a1a22")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "3f95ab78-ff8a-4172-bd96-2e509c45be27")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(D_I15-K)")
			(pintype "passive")
			(uuid "980d3ff5-7ce9-45b4-8586-cc8c0c2abe7a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "631d4a20-9732-42e7-9b26-b09aad40b8f9")
		(at 141.175 42.97)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I4"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "3851f9b2-6cd1-4ea0-90c4-6c104751c291")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "a1173ca1-ab04-4180-b39a-befee530200d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "73192845-af5c-44d4-9e7a-432a111d97bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ccb8d06c-e3d7-4633-8bbd-3bd720ac062f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/c674a2fa-8d55-4638-a52f-c095f6c7ec6c")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebbd2fa9-4db4-4208-b498-cf7e9c62bf89")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9bd6b6f-64e7-4dd1-bec3-f261b47985ce")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b332ec6-f57d-4199-baca-49c0ac4a1801")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d910fdac-0e34-40fc-a393-4bf9ba72cdf0")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a56c4f7-7b99-452e-ac58-4ef64948b1d9")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "026d821e-6958-42c2-936e-d00275d4d1bc")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d782698-72cb-4552-bac6-176267dd160b")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87225f99-e4cd-4a95-be4d-115fa4c004bf")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "676216b7-fc4d-443e-8f75-4ca04cf2c11e")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30220b7c-4d54-49b4-8358-322ec072ae69")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a1e436b-7593-456f-9426-48a7d8b35868")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "713c0a4e-7efd-4164-bf89-695d49759829")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10aebb69-0242-4106-818e-ae514c7833f8")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e582f3c-9f79-4c17-9a1e-de44946ed68a")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f56ee1db-4c91-4e6d-9ee4-6b45deb7d89a")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ddab044-0749-4f68-b543-450168ad45dd")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ed5393b-5055-44de-9785-fd09370f2cc5")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd368fab-b3ee-45dc-9da7-c13128ca706c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "5cf0efa7-78b7-424f-a655-4f7845901a4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 12 "Net-(D_I4-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "61e27dbb-1da2-49d4-bcf1-7357c4941e34")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "456f9e12-3edf-4eef-8b25-aa82064163b8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "63ce167e-08e5-41de-b724-138d0d742e60")
		(at 141.175 104.77)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I14"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "68172671-dd3c-4f43-86d6-729fec510136")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "a96a2fbd-730c-4a12-ae0e-2dd588e91d85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bccb8295-68af-4249-ab52-5073a63a22b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a580f17-db0f-4897-a71c-72d0b0d8229a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/a750fcb5-38af-43cd-947e-f645852c7279")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a80ee2e-8286-46f3-9929-31c05426730c")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "034662e3-7173-422e-9c7c-14155c72378b")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87fb3502-d397-4252-889c-692fa92c8403")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2314e7e5-a35b-47d3-9697-f98496404a73")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fa958d5-c9b2-4cf9-980e-9a39a2e8f232")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "00905c5c-2e38-4b19-a83f-7c2fc2f2dee4")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc23b921-3790-447c-8f6f-91b5cd8b20b5")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9293908-e9f8-4907-8bad-f6b723bfa8d1")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d26e487c-8b92-4bed-86a7-3f288e7fa97f")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4360a5d-f8fe-4b00-a41a-bfbea824f30f")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e6ce99e-fbbe-41e1-8d09-1c933de6c399")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e06ca79e-7447-4c63-8135-4d95f9e98fb4")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b640981c-df2b-45cb-b8e4-5e63e33e8904")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb178163-df23-4c39-a9e0-3a7db28c3473")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2145e173-d0cb-408a-9367-e86b05b23a19")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a57d9392-fbb5-48c0-b7e8-1646f22038ae")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bb9c742-7576-4afb-97d4-f001f5d063d6")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "331677ce-d29f-4af1-b98c-64adefcc6a16")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "77c5369d-a1ba-45ab-b58a-0218bdf51ac3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 31 "Net-(D_I14-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "618681df-d327-4f2c-840e-4ad98f46eef9")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "c6edcf02-cfef-4c86-bb8f-5b1bee2bdd4b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-9_Pins_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm"
		(layer "F.Cu")
		(uuid "65144718-e7a5-4595-8183-afb5d56fbc7f")
		(at 249.945331 86.96 -90)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, pins (male), pitch 2.77x2.84mm, pin-PCB-offset 4.94mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.94mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT pins pitch 2.77x2.84mm pin-PCB-offset 4.94mm mounting-holes-distance 25mm mounting-hole-offset 4.94mm")
		(property "Reference" "J4"
			(at 5.54 -2.8 90)
			(layer "F.SilkS")
			(uuid "6af9703e-211e-45ad-8288-681cd712e7a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "DE9_Socket"
			(at 5.54 15.68 90)
			(layer "F.Fab")
			(uuid "2bc478e5-ad26-4fe2-a3b8-a315f4573584")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c31f1f0b-fe93-46f4-9c1c-8ed31b6622d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "9-pin D-SUB connector, socket (female)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f3f0d9c-6610-4244-b284-8dca1ea9246d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DSUB*Socket*")
		(path "/fd8b193b-bcaf-4a83-8c09-cdb9237e4b01")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.945 7.72)
			(end -9.945 -1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae6a6445-b170-43cf-9570-85418e16cb60")
		)
		(fp_line
			(start -9.945 -1.86)
			(end 21.025 -1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90b40abe-9a7a-4a63-a4ac-92ccbd0cf11b")
		)
		(fp_line
			(start 21.025 -1.86)
			(end 21.025 7.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df85bc71-8b55-47fa-bae6-bfea66ab02dc")
		)
		(fp_line
			(start 0 -2.321325)
			(end -0.25 -2.754338)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f22f68f-8e47-4761-acc1-8d8011810f24")
		)
		(fp_line
			(start -0.25 -2.754338)
			(end 0.25 -2.754338)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cffa1f0b-bd71-4c8e-aa53-b94235cc8f18")
		)
		(fp_line
			(start 0.25 -2.754338)
			(end 0 -2.321325)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6875a216-7b03-42e1-9953-3d500bda6513")
		)
		(fp_line
			(start -10.39 14.68)
			(end 21.47 14.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0113967-1fc5-499e-bb6e-22ff5de88ec1")
		)
		(fp_line
			(start 21.47 14.68)
			(end 21.47 -2.31)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "765e7ca9-cddf-478a-b5fb-13111f865357")
		)
		(fp_line
			(start -10.39 -2.31)
			(end -10.39 14.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6e1c48a-30aa-490a-a3ae-fb9d0d927c18")
		)
		(fp_line
			(start 21.47 -2.31)
			(end -10.39 -2.31)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9074623-44da-4a45-bb28-7b16713affd5")
		)
		(fp_line
			(start -2.61 14.18)
			(end 13.69 14.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "821f7793-2946-4813-9a46-a9233a65a081")
		)
		(fp_line
			(start 13.69 14.18)
			(end 13.69 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75d42b2f-8d8c-4cba-b350-141ba1fadf8e")
		)
		(fp_line
			(start -9.46 13.18)
			(end -4.46 13.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "891ead92-7f57-4417-b825-07d7e11e1e05")
		)
		(fp_line
			(start -4.46 13.18)
			(end -4.46 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bf569d6-fb16-4f3b-9fd3-4cef16871d56")
		)
		(fp_line
			(start 15.54 13.18)
			(end 20.54 13.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e18a8e87-f57b-42fb-aab4-7addcc33ae80")
		)
		(fp_line
			(start 20.54 13.18)
			(end 20.54 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6ec85de-50cf-47bc-b60b-0a27cb5b4923")
		)
		(fp_line
			(start -9.885 8.18)
			(end 20.965 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c14d1d92-eba0-427d-8a3b-e3dc4e55e762")
		)
		(fp_line
			(start -9.46 8.18)
			(end -9.46 13.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0dfb398-51b3-4093-8fee-9408fb7b04e6")
		)
		(fp_line
			(start -4.46 8.18)
			(end -9.46 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca5598d1-3404-4f18-a7db-8fc39d3f8861")
		)
		(fp_line
			(start -2.61 8.18)
			(end -2.61 14.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6902aaa9-9416-49f3-a700-076ceabe7d88")
		)
		(fp_line
			(start 13.69 8.18)
			(end -2.61 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "400d90fe-9b54-4d8c-aa6a-524ce4d6bebd")
		)
		(fp_line
			(start 15.54 8.18)
			(end 15.54 13.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77e57473-2a11-46d7-955b-3d80d3387440")
		)
		(fp_line
			(start 20.54 8.18)
			(end 15.54 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a23ed739-19a4-4812-a8ff-53b3c23bca3f")
		)
		(fp_line
			(start 20.965 8.18)
			(end 20.965 7.78)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8985ba32-b79c-419e-9b6d-e960eb6c6c7f")
		)
		(fp_line
			(start -9.885 7.78)
			(end -9.885 8.18)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ed9f3e5-f1ca-4b29-9489-ef3879053997")
		)
		(fp_line
			(start -9.885 7.78)
			(end 20.965 7.78)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc9b55e1-185a-492c-b672-b8866cd9e1e7")
		)
		(fp_line
			(start -8.56 7.78)
			(end -8.56 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e07604dc-5c81-4c62-89de-48ffce499cf3")
		)
		(fp_line
			(start -5.36 7.78)
			(end -5.36 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1929dd3b-5328-4ec3-923e-bc58455b61a8")
		)
		(fp_line
			(start 16.44 7.78)
			(end 16.44 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76f742ea-fe5a-471a-9a30-be56c5f44ea0")
		)
		(fp_line
			(start 19.64 7.78)
			(end 19.64 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e46a2565-a2e2-4e24-ae4b-1c9e75e86dea")
		)
		(fp_line
			(start 20.965 7.78)
			(end -9.885 7.78)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd25889d-9059-4503-a96f-bdd69145a072")
		)
		(fp_line
			(start 20.965 7.78)
			(end 20.965 -1.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95e2b3fc-9da7-4535-bfa4-b20e80771fde")
		)
		(fp_line
			(start -9.885 -1.8)
			(end -9.885 7.78)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a424116-9de7-4f87-b8ef-1c463f00424c")
		)
		(fp_line
			(start 20.965 -1.8)
			(end -9.885 -1.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7425858d-3394-4868-b344-6cf300e9057c")
		)
		(fp_arc
			(start -8.56 2.84)
			(mid -6.96 1.24)
			(end -5.36 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3403088-acaa-4e83-84d4-91ce3dd525ce")
		)
		(fp_arc
			(start 16.44 2.84)
			(mid 18.04 1.24)
			(end 19.64 2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f939194c-dc42-46f8-ba92-33bad1692100")
		)
		(fp_text user "${REFERENCE}"
			(at 5.54 11.18 90)
			(layer "F.Fab")
			(uuid "689e3814-e2b0-4f54-8180-947105a6313e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "0" thru_hole circle
			(at -6.96 2.84 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(uuid "7e52fff2-2c33-4121-8cfd-beea1ee456b0")
		)
		(pad "0" thru_hole circle
			(at 18.04 2.84 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Shield")
			(pintype "passive")
			(uuid "82e4df80-f219-4c01-bcbc-ddcb8404fe87")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "unconnected-(J4-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
			(uuid "404acc2f-7318-4b72-ac10-b2e6038308d4")
		)
		(pad "2" thru_hole circle
			(at 2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "CANL")
			(pinfunction "2")
			(pintype "passive")
			(uuid "b0e24e2a-ee6f-42db-98d1-d6703846b897")
		)
		(pad "3" thru_hole circle
			(at 5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "3")
			(pintype "passive")
			(uuid "117d7ef8-8db2-4ec6-bde6-dfc552cc5fd3")
		)
		(pad "4" thru_hole circle
			(at 8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "unconnected-(J4-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
			(uuid "6f24f51f-c028-452b-ac8d-408a9137f461")
		)
		(pad "5" thru_hole circle
			(at 11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "unconnected-(J4-Pad5)")
			(pinfunction "5")
			(pintype "passive+no_connect")
			(uuid "5989a61f-afcf-4952-841c-c588cd5d95fd")
		)
		(pad "6" thru_hole circle
			(at 1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "unconnected-(J4-Pad6)")
			(pinfunction "6")
			(pintype "passive+no_connect")
			(uuid "8c713777-7f50-4be6-ba54-d458d95f798b")
		)
		(pad "7" thru_hole circle
			(at 4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "CANH")
			(pinfunction "7")
			(pintype "passive")
			(uuid "5c387ff9-9d40-435f-929d-48c5b134947e")
		)
		(pad "8" thru_hole circle
			(at 6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "unconnected-(J4-Pad8)")
			(pinfunction "8")
			(pintype "passive+no_connect")
			(uuid "9df6e600-689c-46d3-a562-53c4faddf7a7")
		)
		(pad "9" thru_hole circle
			(at 9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "unconnected-(J4-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
			(uuid "0fb1aacf-d7dc-4cf1-a598-b6edf09931a6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Pins_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6603c6c1-1443-4a84-bf9c-05f3875ff5f9")
		(at -11.4625 94.04)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "52f03a5b-ea4d-4d6d-8366-365aa676047f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "cdfb5edf-c539-4ec5-8e67-82996a01e697")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c59cd852-0d8c-49c1-b9b5-be59f0f86b7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e79e3edd-20f7-447b-b082-ca19fa8367f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b8b3a0e8-c372-4500-beee-5a57e92abe68")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "241f497b-ef6b-489e-a454-8b01111e8b20")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23f1a3d5-1830-4df4-ac4a-5543bf84fa6a")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13a388b5-98c4-46c8-9a34-fef839fa4bb1")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a04ab95a-1c27-4424-a8e7-1118a221eea5")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "947e41c4-dbb1-48be-a4f0-a1a38978a7fd")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f77ef92e-e02d-4a9b-b69c-3d8fd25b1c56")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d18feab0-bcec-47ec-8d57-243f2dbf8b6c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb7f4b77-ed47-460d-b156-82ad3593200e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f3f114b-62a1-470c-a938-b5b60b295a78")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5904e44-dcdb-4178-8678-744095e1d933")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "26fe8f22-e387-40fa-ab7e-68c6544122a4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "15cbb767-a571-4bc0-b814-66f248a97447")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "4aa6711f-ad1a-4616-a73b-24076cb559c5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "665e94b9-67f3-4774-937a-db97ba195e57")
		(at 147.83 120.495)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I59"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d87b5db9-8593-477c-bd91-2e1f8eb9b4bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "fdfe33dd-0f9e-489f-a549-be6cdab0204f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1bbd611b-efd7-4dbc-afcf-430f0dee676f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "279d520f-7966-45c6-859d-24b0d1b193d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/004cbe87-9f57-435d-ba09-24a70c121893")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff2604fa-4a37-4d69-9bfd-98c9803abf2a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc26a250-f427-41ee-8a8f-3e0c3a663899")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "475c680c-750a-4b08-ba30-0c02c1d3cd38")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7df4d572-f6c9-4d00-bbb4-eac3db5aadc4")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a54295b0-c916-405b-a0da-dfd5a25f09d3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4650d12-5a45-43c1-b593-d3ac1652ab36")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "761356f5-f1ad-49c3-9ca9-b8a119485921")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e72b46c-2c75-4992-807e-f3446b8958e2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3cff3427-b0f2-4ae2-936d-0dfdd73c33ba")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a26c2c0-62f8-42ec-b830-b9a526c6bc0a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1a149bb3-fac8-49a3-976a-6d347df9ff8e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 84 "IN11")
			(pintype "passive")
			(uuid "11ec22fe-1eb5-47ac-99b7-de88cdae9705")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "bd4c0794-f213-491b-b012-833c9899a70c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "668fd9d1-b649-4bc4-834c-82e02920a7e0")
		(at 141.175 94.75)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I11"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "20d71a18-a312-4677-9622-04c2c729bf65")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "d9be5f0e-5204-48cb-8e3b-2228d3c24389")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a6cb1cd-32a9-40a2-8fd4-9a729d6fe2e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9de3e0a7-cf5e-4227-bdec-094ad3532926")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/d5114d38-193d-4fe1-9627-2faa9ab5024b")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cffacea-8367-4075-9844-3aa1cd7b0b83")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "029af5ae-d43c-49f3-ba00-ce9598adbd59")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6415a5bc-6e0b-47b5-9712-66782a4669e6")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2179d51a-f719-44c2-b0cd-672f658c871f")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc9093a3-d258-42d6-8380-1083bbd50b57")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95d11648-e35f-4ee3-b493-07626bceab84")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bd798fe-da6b-44eb-bc0a-df044d4e5d98")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc21acc8-bd7d-4247-a62b-a21c69cabb5c")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f068e3b-2829-4d55-924e-d969d4f3a812")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5456c770-30e1-45ef-8de3-5a02bf450be9")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a4c0d20-610e-4724-9a71-a9f7194fbd76")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86fb28a2-46e8-4125-9841-ee732e0096b6")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5248985d-7093-4e40-a047-f3e56569bcb5")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9da2ca5c-fef8-4f5b-a747-74dab5ff7504")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a26f8712-47cb-4ed0-8c24-33dc7707a35e")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c94a76ba-45a4-41cd-8a1f-71c24a6d8a91")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40b502c8-0bf6-4d77-a776-287b6ea9484c")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9ecd785-f237-4aaa-a711-f64741c3c248")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "4689dd3c-6b87-4fe9-94ae-8e53ad68b5c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 24 "Net-(D_I11-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "efe9454f-71b2-4737-ab76-05c12c92ae70")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "f3e76a2a-908c-4a7b-8982-b880d619a626")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "67396613-93e2-426d-9180-e02d3dbb774c")
		(at 138.33 126.395)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I45"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "307430f6-8f55-4d6d-816e-8412c9bed50a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4879e9cf-9035-4d18-aa73-96295f8b3f23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6af5abc-e302-4072-93fa-8653ca9929c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "57f14159-a95b-4b6c-87e5-51f1f63fc3c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/4e5cf595-d5af-4c84-b108-f67305677525")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b4125bf-708f-414f-bfd4-97816d56a5b5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d570436-bb74-43fb-846d-04e03049aa8f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fdea3e2f-1257-4d98-8374-60001cf12828")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d416482c-dfb5-4e24-aecb-2f9d7f189c0d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b6cc8b2-d772-431c-85cd-432bddb884c0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8b01d87-9aef-4635-a315-5cf9692e380b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35f76706-1f53-4374-a71d-c6f608225705")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4ef82d0-d635-4dd0-a80f-1df60c242436")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d03004a2-d36e-4752-a11e-44e0df2f8557")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a6b82eb-e315-4823-88ae-c1912b0b5cf6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "79292356-9dc9-4979-b3f2-208207693aad")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "a697e68b-a525-4d1f-acf9-97eb150348cc")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(D_I11-K)")
			(pintype "passive")
			(uuid "7a56796c-1b29-41d7-b9f3-b476db3886e3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "67c42939-c767-4b30-aedf-5a0a5a0a7074")
		(at 157.33 120.495)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I75"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "4b560046-2e92-4ab6-aef8-961bf0cd422b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a48f2f14-8b4b-40c9-b8a0-40577b8679a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2af3946-b046-4446-a105-be00ec43d80e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bd2883e-da2a-49ed-9818-fdacd07494eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/a7428a7f-d25b-48cb-840d-f4f87e9ce991")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79c8709a-1862-4e74-b199-ee66f77b9c55")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1bdb97c-aa6a-4d61-9416-e57a915b9c26")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39fb8d0e-dfd0-477a-84ca-46dd8a443e7d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "019e678b-7c9f-4a51-ab89-6361e4f357aa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7a7788d-18f0-4575-8462-6c47b1a316a3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9303a61-6606-487f-8066-441475b75bae")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f1d4276-ef6f-4334-aa92-78ac6594e1b6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fd4a874-19ed-481e-ad1d-b1d0f75e6022")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6715d654-b89b-4309-b055-1317700c039b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f9ca09e-9a16-4be6-94b2-0a44717a92e3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "95757877-8537-4f50-a52e-4566981840a1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(D_I15-K)")
			(pintype "passive")
			(uuid "3b6aca26-6693-4a89-a089-6c6d4afc8419")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(C_I31-Pad1)")
			(pintype "passive")
			(uuid "2e61a667-5607-41f0-ba11-179914b00fcb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "6afc9fcd-0b66-47a5-9eaf-42c6628832a7")
		(at 138.33 71.275)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "27da9d5b-7a1c-4f2f-8746-af10e0b38a92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b030901e-28b3-45c6-a075-561facf2df48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e81e2f52-48a8-4f77-a7e3-85d2281e2e58")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "51a67455-7ebb-4818-a2f3-56280299cf80")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/5591eb71-aef2-4344-9d7b-740233fde812")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6877b72f-7262-42d1-a1bc-aac5ebbe95ef")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53c6d62c-fbe9-4115-97f5-0fc36242179e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12decc72-93bb-4de1-b718-1c74f9345e72")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efaea8bd-adc4-4755-ab83-6b41e2baf9cb")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2fb8a93d-9f10-4f8a-a525-f755ff82baee")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ca092af-6655-400c-acf9-b74d62da2a57")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "412574f7-6c56-45b1-ab46-bd30e54f9ce5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d08ff4b-498c-4ca8-94c3-28942f7aafcd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28bf9b18-f62f-4fec-b1af-ceed87156c3b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b11e53e-8480-442c-a7c9-78cf9a1eba05")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "de99ce11-d063-43b2-893a-8c890eafe115")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(D_I1-K)")
			(pintype "passive")
			(uuid "bf3d946c-aee6-44cd-96d0-c9e1146f7694")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 38 "Net-(D2-A)")
			(pintype "passive")
			(uuid "17638673-14e4-4d33-8a19-2c8a39e25d23")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "6c06e3a2-b84a-4aa1-97c3-1d997cc44006")
		(at 141.175 32.95)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I1"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "97643af5-95ea-44f4-b232-0319f9d1a079")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "0622ddd2-bdae-4689-9aed-02fac65c7374")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c06d459-2bf9-4eaf-820b-cbeb65979859")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15e51325-bae7-4d70-bddd-8b892f13d659")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/faa025f6-4703-4edc-ba61-9e7f4cb1c332")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b2608fa-4c43-42f5-b4cf-8014661b5142")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "940fb36d-f179-43d8-9ebf-b46f31b57370")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00979ae2-a805-4303-9c98-ae45e6d3e771")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16324405-fc31-4bf5-ba7e-3c716fffbe8e")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cc510a1-e001-434c-9f62-9916016f6bae")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dee95238-3ba8-4069-a5a5-2bd124f61935")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "335d4b2f-42ca-4f06-aa67-fc3ebfc5fd87")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b413013-246b-44b9-9039-5b4ef14103a0")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17761db6-3041-416e-a7dc-de7b1e36b69a")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcb9d773-8c80-4d9b-ac8b-e7de7f1fd743")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0bc60586-f6c5-4186-93b5-e7d1e440075e")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b41d4d17-b31c-4fbb-adbc-674fe33fc96a")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f31600e5-816c-44cf-ae56-7a6cf0b4fff1")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95883b39-bee3-4a1d-9223-3419c044b43e")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5792005e-b8bd-401e-84ca-2c8edffd1c0f")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eae61ef8-9b90-4d4a-96da-817a62535fe6")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf64f06a-d110-4d43-af9b-1cb209d33525")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5961b464-18c4-41f2-8455-6f8d62855814")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "37f0a25e-88ec-430a-83c7-b28c5e10fd34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 7 "Net-(D_I1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "cf99e46f-57a9-4281-bc68-7117c1ec50b2")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "0cf09651-247e-4134-9f80-31ea5288ae67")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "6d8ab8b9-8a1d-4625-9c66-cd196f4abb4b")
		(at 143.08 120.495)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I51"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "758f7427-6d83-4093-9f2b-59e6bc129c14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "312a86b0-b99d-4ec0-b578-268f2ece2d01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea500738-64cd-40eb-8d26-c1e5f8b34cae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4bf2c8b2-7477-4735-9b94-973730df15e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/2ab9805e-ced6-49e0-aa85-214a78472d08")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47915c5d-3136-45f0-b41e-5f5a1688de4f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3003de81-3dc7-4d60-907d-1719a09d10f9")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d95de656-5962-434b-8c70-91f10c4fdcd9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7cf941f3-8ee2-4d95-8dcd-3d9cb22c2839")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "657f025e-5558-47a3-99b8-67a3866001fb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd177402-c6cd-46c2-9a84-6e88430c40b0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bad39bb7-c624-4a8e-b60d-cec9859cf58a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e8378fa-083f-45d5-96ba-4002e97a397f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ccbdb3d-2f36-4317-ad58-7a902ffa857a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaebb356-2016-414c-9993-c5ac9ea2efdb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b87a9d88-b010-49d9-98fc-9a87ee6f6da2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(D_I11-K)")
			(pintype "passive")
			(uuid "7c4dd602-80e3-49dd-81a3-47af87179abd")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 48 "Net-(D16-A)")
			(pintype "passive")
			(uuid "cf99af38-a5a2-475e-ba71-3234acada856")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "6ea7fad5-6dfb-43c1-a7b1-62c5e8c72780")
		(at 6.4575 72.31)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "06fcfbf2-5110-4f9d-9d3b-eb805ff95e44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "47799cdb-ad89-4c89-affc-07101e8df87a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "da590533-41d7-4c3a-9445-e7068fbd8d8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e27d6b78-69d0-4d42-9ca2-cd4b8d105e4f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/01e360f8-3883-4641-93d9-4160961da1be")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd73c86e-072b-4bf0-8ce9-77d216cdc831")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "392c3fca-1d1f-4be6-b582-3a51be51523e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c116e25-bf29-4104-ae2b-d79d05048110")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a928159c-3d92-4dae-be39-98c52b02e381")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "747a9981-6298-4c32-9154-f5cc722d8af7")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3edd367-6af7-4c51-ad13-1ec8dcec9ea5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81d120c4-4bd8-41d2-b1e9-572656f782ca")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "358a4363-cea2-4fde-899d-afb032a47e6a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01e4dede-35f6-4b6d-8394-13bc0a82b016")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3171ce2a-5a33-4839-ad9e-c204206c0949")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "59581b4d-dd7e-4057-9fe4-10d248c291d3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "EN")
			(pintype "passive")
			(uuid "48cb4ede-0cc9-4d2d-9817-3aac81c7a460")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "31d0c633-d12a-46b5-a02d-1679092dc28a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6f44e4d2-25dc-4588-90bf-9755f810725a")
		(at 153.54 38.805)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "6602ba91-674f-47ac-a22f-79cd4233d420")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "f39e546e-5505-4a53-82d6-ffbe9be89617")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9d7ecefe-b9ad-4369-9c28-6e54c7cb7966")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "26c8ddb9-a2a2-4b66-bdc8-d28814ed76b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/bb5e668f-5fea-4db0-a207-74c0025fb75c")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f3deb1c-d9f8-44f2-9476-7444c2e4d615")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7e94352-c611-46ff-9f97-3a3e0e322cf8")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60d580a0-6a47-4169-854f-6a0ea6cd097c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6eaac2d-d89c-4998-a360-835f35b65171")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac9db161-d380-4dfc-9dab-606e9fdacd5e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a5f9c08-a6ef-4b44-93a4-0dedddf25e1b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a45b63bf-505b-4c67-87c1-bc68c27887f5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "216b8ea8-6433-4c0e-8cdb-a7260ce814d1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9a67df0-41e3-49a9-ba7b-01b9403fd04c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9af327bf-7b4e-4150-bf7f-7ff79fb61b85")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b715f1c2-3e63-4a43-ab4b-56c196b05580")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 8 "Net-(D_I2-K)")
			(pintype "passive")
			(uuid "7c750f29-440a-412b-bd51-5b39ed89d711")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "5614bbd2-b48f-4fb1-b8bd-9b74811b0247")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "70086b74-abcf-4041-846e-5ebb31418e39")
		(at 153.54 93.925)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I19"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "0e3cdb65-f2af-44a6-b154-4d0db312f404")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "184d71f7-9e5c-4a1e-8b5c-d02ed8128898")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7fe5f8a-8396-4e89-86d3-5a26f16a0ac5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f7a4cdb-5407-4977-a1cf-c086e542c9dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/784e26f5-19d3-42fc-8e87-8b60ee4ab9c1")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba685920-f149-42eb-b3cf-4e878a213866")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ea53343-c3bb-4d4c-85fb-b200d9682066")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c8bc906-8e81-43ca-82de-8543098f6051")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bf924d4-d1b6-4d0c-816d-aac94de2c7b7")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a84929c2-48ea-4134-b875-0959bb0f4f3a")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6b261f6-1e42-4ca6-8ca8-48f752db8a70")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6cbdc04-7786-416c-8730-dd93ae71ea07")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d4ba2aa-ceda-49a6-a6a2-cb8bcf12676e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c20d53f3-36c6-4ec4-82d3-4cbc491ee670")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd41c164-cd53-40ce-8bdd-f1b5ec6c832c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b6c9c809-5d27-46e6-b1ba-a315ef1aa961")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 24 "Net-(D_I11-K)")
			(pintype "passive")
			(uuid "61c0fa35-708b-467a-aa5d-9c2c653cebd9")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "665df5b2-0b95-4cfa-bd0a-fa8ae811caed")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "71fcebd8-d16f-47ec-9621-85975fe8e5d4")
		(at 157.33 59.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I33"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9e504fe4-42ac-458a-92b3-03da95d3373a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "eb5a8d1e-42c8-48d4-b95a-5f4c2797caf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "953e40d3-bd1e-4e9e-a4cd-4bc5b8cb97c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd4ca06d-55c9-4590-a8bf-996c217d83e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/99f007b8-ed34-40e3-a84b-c6cc3f9a3894")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "147fbad6-29e3-4b05-b06f-11592d4d0d15")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7a35434-0d0a-4058-8f57-2f2cf5f79e7a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88f45906-ceb8-4c0f-a77d-7f01b5ec9d08")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f6152e8-19f9-4b05-8cef-577b826db565")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca44af82-8120-4d65-9ddd-60cd596c9c4e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f310db81-d26b-4a64-8f25-9336237a07e3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad90109c-2447-45bf-813a-2c7a7b8efd99")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6770f870-7fde-4ba7-ac1a-5ed8ca081516")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00843b99-9471-486d-b424-3971b7a616be")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7634df7a-fd1a-4cad-9018-b56d31127803")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5fc706dc-88b9-4d8b-b000-fc8e18b03a35")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(D_I7-K)")
			(pintype "passive")
			(uuid "d1788550-81b9-4a78-9ee0-3fe32318d04e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 44 "Net-(D12-A)")
			(pintype "passive")
			(uuid "130ca334-3526-4d22-b2cb-e4c598a03a71")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7275b6d1-099c-4762-b963-caa997ba2a3b")
		(at 152.58 71.275)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I29"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "098212c6-67d3-4943-a4af-b991baf1e83a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "1f487912-777b-4fbb-9d74-5eac1da29108")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e7b5591-5fc8-4d2b-b20a-a654c25c82ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "90e9ee0a-9d25-4d35-a339-8ba172cb2110")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/d809ac8d-1f5c-40ec-929d-629a313cc8e7")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3338196e-acfc-4560-917e-271730de60d5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2ae7708-f9cf-489b-a942-c50b9d9ea72f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6ac6ad5-67e5-4679-85bc-f9dedac6d974")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f789932a-5040-4eb1-b5ef-42ef4dcb1368")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c34d4e6b-b43f-42db-9c3e-9a45122ef45b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "035e24eb-ef55-46ae-807f-eaa264a21cdc")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f76ed98-a200-4013-9bfb-3f653de331c3")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73b9bc5c-2762-4e69-a801-34bbab8f6455")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "529fa8c3-f01f-498f-9cc3-a973f64da753")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bff8f3f-ab1e-43db-ad3a-3e585283608b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "90e4d538-487f-4034-ba97-8c2bd240d8d9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D_I6-K)")
			(pintype "passive")
			(uuid "3d6d0937-a26b-422a-9cd6-c5319e25b318")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(C_I12-Pad1)")
			(pintype "passive")
			(uuid "9455dc29-70c6-4f6a-83aa-cd15ee02ff11")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "751d8e96-40d2-49b2-86d7-4fa8dc726da2")
		(at -11.4625 97.05)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "d1ae2ba0-1fa6-4a88-a485-ba92d94b36ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4u7F"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "f4d055b4-ac0b-434e-ab0c-028651b6a5b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "90950007-a107-44ad-9070-cb2882b80d49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d86e6de5-7d5e-48ed-9dbc-6651cf84cd03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/986fc404-1a2a-4281-b14d-b502df02e93f")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a10ef6e-f51a-4469-a417-5465618efa3d")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4086ce2e-052b-4102-9603-fc0376138f27")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aef09151-14ec-45cb-bd7d-f8a7614729d2")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a43f0549-bf52-4252-908b-67f3898f25bd")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44be1eda-1952-4be7-8de1-75c4c0d67d5b")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a37c7ee-30fe-4346-a486-2ce43c3b08a3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1909cea2-6f06-496c-998c-c10ab81a79d2")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e912de86-b220-49ce-ae45-3ff7291b88fc")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8520d408-67ad-435c-b595-f79d2936716e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7138cc8-1b82-4e35-b834-cc64cd5d132d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "276a1b91-7703-4714-a006-778a7359d537")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "947c45ca-7582-4eb0-b71e-58a6db50e3a8")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "5V")
			(pintype "passive")
			(uuid "9d1d8b76-2acb-4b61-a746-efaea17fbedc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "75dc46b6-c58f-4cdd-bb4b-9a35d1f04fe8")
		(at 141.175 46.31)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I5"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "fc85454d-632f-4044-acfa-d60247c56148")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "8bf63d42-d844-4273-a40d-80b77cefc224")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f227d59-9990-49b5-beb2-2c6c90d7e04c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2668e882-34b2-4517-92e4-4d0eb328b3a5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/ae566f26-73f4-4223-922f-295b03d0e94d")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3335085-356a-494a-b469-ba6084fea65a")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "835fa0c2-f7ff-4c16-9c5e-e400a6df638e")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7c93b24-1a85-4b96-a966-d4b4cb7d707b")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26576d2e-9623-45cf-b1cc-1415010a8ecd")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78a0c1a7-b1a0-4f8a-abfd-ab5c620f1f62")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "656139f9-747d-47a0-b5ad-ab590c166229")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93f9ed4b-1551-4303-93e4-53163c93bfe5")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54a0f240-03c4-4df2-96a8-cfd3bac529c9")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c01ce965-b761-4869-b1bb-b9f47ac275d4")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04a1a81e-81a8-4676-95a0-d26552bd39e2")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90a570de-552f-4d11-b813-2de9a8c33099")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7fe835c-4f2e-4374-a74d-69038f950b01")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "acbc58c3-9987-4e99-a444-80411173d32d")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9c15689-51c9-4614-898e-288e05384bef")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c9d2f41-7393-4b2a-9062-8f53948b030f")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c11cb696-bf8c-483b-a5d4-957094a9896f")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1e8b94b-5490-4640-a936-41d55071e170")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8db146eb-0167-4616-a4d9-9fca0e647d2c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "27457001-b779-4b22-bbeb-50153b61015b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 14 "Net-(D_I5-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "d979128a-fe79-48e8-8dfa-3db49fc32bc8")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "80c1ee5e-754d-4195-ab6f-7998d439da77")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "79ea2888-38ec-4335-a95f-5ed5ac90a62f")
		(at 152.58 120.495)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I67"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2c8c1662-6ed0-4f95-91da-26cf3259eade")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d9b306f1-d6f0-451a-8b3f-9b68594ea216")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aef94f31-5ccc-40e3-b11b-5ea31518a3db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f062dec9-b0c9-4e40-898b-4755784df133")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/5c18a2d4-b508-47a3-9658-454bda1c067c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9866db0-17cf-471a-ba7b-277c55c05a03")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd3ecabf-ae63-4e68-892b-d121e58480e8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb33e74f-10be-4fc5-a382-b3b9c21c0419")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e058315-c3e5-4b3c-9f8c-9e18eefee8b8")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f23cdcc0-6014-436a-8b87-ad4545c2ec21")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0639271-5692-4047-8f28-1cdd3121fa2c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91acb12f-89fb-45c6-83a4-5dd7731c1148")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "249234aa-d797-429e-952b-f3516fa553f3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c08752d7-e2c8-4ec6-90fe-30ca8240c5e3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f43c257e-e4c8-4593-a436-cc6af979b2a2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8fb74c14-69bf-4118-92ec-4fecbb16d59e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(D_I13-K)")
			(pintype "passive")
			(uuid "808b7566-2cd5-487a-906a-8663372f69b4")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 50 "Net-(D18-A)")
			(pintype "passive")
			(uuid "0aaaa704-b398-4c0d-83b4-6c9d405641ec")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7a3575c4-9ef7-488a-8bef-f792dba33450")
		(at 147.83 129.345)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I62"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a2c4720d-f5f7-4790-9871-ad628c4b53f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0e550415-2ef5-4b06-9be9-9276f0df32b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "94d32c0e-2b10-4cbc-b6b9-b50c330909ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "725e1043-7e4b-4774-8d73-0ce3fa162984")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/b818c57d-64a1-4cd7-80c2-25e81c5259b8")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80ed1268-8423-4c89-a4e9-14936b90a31c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62346e29-4458-4ce6-a413-ee317ebfd9ea")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7326425-9fc2-4fb9-ad14-f86a507e83da")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc690bd9-fbbd-4057-9d83-eab9f0ec8641")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "abe3a92a-3dfa-407a-abb7-c50e1c8dea70")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b76cd84-5438-44e4-816a-d542e18e916b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35b2330b-4349-4c9e-a8cf-838b81390c7a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5902687-42a9-4cb9-9a6f-21b82180bb5e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72bd2049-ad50-4f9a-8b1f-13f71d05fcef")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd6c6536-439e-4a3f-9e97-c052cf9aaf6f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "345a4980-4c21-4259-862d-52e87556ef2e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "7d4b0f7d-d13a-4b69-a273-3aaff8cbd0e9")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(D_I13-K)")
			(pintype "passive")
			(uuid "362b6d55-e645-4f3a-bda8-129e89b10c77")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7ae0f7ee-45ea-43d7-9363-23bf3aa14a24")
		(at 153.54 102.955)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I22"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "66f8e775-b48a-4953-ba9b-5f647f48c19e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4f2dec42-e006-4f63-9d5e-67f3a8eabb84")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "92df55c7-0e2f-4683-a262-c003580a75f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "250b0b24-d5d1-4dd4-9ad0-e7bab3cbb6fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/c72ba19b-f220-4ce7-9dd7-55846ce83824")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa94222d-8adc-4a67-8386-f73b52a68265")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8e3767b-25af-4eb1-ab7b-2b655fa56b1d")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b58f21e8-5ef5-43d6-a1ee-a1d436af8d31")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ff98f69-dcd4-47f1-89c7-a203f2bf2535")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd156048-f249-4e10-a3bd-2179d4a9fb77")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c640d76-0338-4258-8fcb-7a96aa9f8203")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19b04f9a-be25-4853-aedb-67b8ffd7fba6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9c2ba2c-1017-4ad7-851c-f7eee6cc08fe")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e1dccb9-65ab-4b27-98a5-c0127083ecfe")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0071b90d-b209-4738-8017-ff4f7e611c38")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1b475717-ebc3-40eb-91e4-3d9f9a1b4465")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 27 "Net-(C_I22-Pad1)")
			(pintype "passive")
			(uuid "ac30e987-e62e-4de1-8a72-83b19014be1e")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "e10ccbfd-91b6-40bc-a39a-6b3c25944c0d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7c638c01-7bb5-4780-9c4a-3884c1e01acd")
		(at 158.35 32.785)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I7"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "696792e4-90e2-40cb-920b-e942b565839f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c908c1da-0f0f-4ad3-8f66-df780b1c2bf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "90ecf414-ae78-4d98-8d5e-22259d3fce04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cfdc9f59-e7bc-423f-922a-96b6d8028466")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/79d7638b-ce07-4a24-a772-470a5a4c7306")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a04554e7-a01d-4a66-9cfc-551197b2132d")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca81af2c-ced6-4ff9-9624-462c310df88c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f9f659e-1b03-4d68-9e6c-43d19c131afc")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4df4869d-e77f-4f64-99d1-37254c68a928")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "762567ab-b2ed-463b-a482-c4d6ecccf84e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38273c3a-5827-4026-b2fe-afb52d07e26b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17655d78-d3de-423d-a002-54b18658f04b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42a8bae7-58b4-4180-964d-c1880aa92b10")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b58c619-b935-451e-8922-3c0ed977f5c8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02fbfb93-0e13-42d3-bba3-408d534f9cc3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "71b5aab9-9551-41f9-aedd-41751c465161")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "Net-(D_I4-K)")
			(pintype "passive")
			(uuid "c5314c73-0a47-43c8-883d-a05aa16b3ce3")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "8e164a50-2471-44a5-9750-35c0a238fb32")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7d8463ef-6a59-4e18-b520-2b96f1087fe7")
		(at 153.54 90.915)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I18"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "e86b7ad1-4762-4e42-9ee1-31e53b50f101")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d2d3ffee-58c9-48d5-b2cc-f6cf560c5775")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27b9fe27-112f-437e-877b-96c69ba7bd2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a6bb6eac-8502-42b9-beb7-beabdad8da37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/c7799b8f-7675-4f80-9da9-30992a18288f")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6da37c15-b2fe-43fa-a566-090769134965")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d7febaa-62b0-47a8-8beb-1ec4437d675b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "450fe17b-e043-4ee9-b793-3a8b9a82658d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "152119e4-f7a5-4db4-9e51-51e576c03538")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3600459c-d52e-433c-b3f6-d37cb38c0e36")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d398a81-8876-48e6-a746-1b2888761ecb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "215f946d-77d9-4729-a5c6-e42ca1b147cc")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd4d78d8-0c9a-4347-b743-ec8b8b5d38ca")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "498bd6a2-7b87-4926-92fa-6a90df7b59ce")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78e0e93f-5a6a-4416-8461-4756cb1d1bcb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d3496cf1-266f-470d-8674-38f5a3f3d875")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 23 "Net-(D_I10-K)")
			(pintype "passive")
			(uuid "61330dea-6c99-4b35-b824-59acf37f79cd")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "cc99cb47-4268-4773-8fca-0ee403611360")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7ec0f305-4648-481e-83db-e40704cb7273")
		(at 163.16 93.925)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I31"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "8018ed14-8cd0-4132-90c2-f53bb78f032e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "26e33024-f0e8-482d-b6c2-2da45800f2da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "81439a47-c946-4295-bf26-a6658b91f3cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b51a293a-21f9-4c11-8803-97dd62aba2c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/fe66ebe3-b951-464b-97ea-0448fa49b634")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eeff4352-fc43-4d71-8f12-73eb3a953af9")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c688b263-63b7-46d3-984f-0e8f5530399f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "02b72c8c-23e5-4523-98f3-cd52af6d4034")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d35c3a8-9e5e-4f3b-a4bc-4157785345a9")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1dcf9d0c-7d53-4040-9dad-4f906815ce79")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c90a77d-0327-47c4-b300-89260eb2f7b1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97840b9f-8645-4ad0-93c7-f400e814a40c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be2d17cb-c3ea-4e60-907b-a5a2bd6714d9")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "909cd9e6-148a-45f8-b323-1329697322fb")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f532549-233a-42ab-9b4a-e1abd492f281")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c24cfb26-650b-47b2-89fc-63d9c3f2b96b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 36 "Net-(C_I31-Pad1)")
			(pintype "passive")
			(uuid "28f0e4be-99df-49d5-ad59-06cece9e0315")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "fac08aa0-7460-4c34-8c35-2bb7954d3bc8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7f9dc49e-3d17-42a6-9aba-68b2abaa96ba")
		(at 157.33 117.545)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I74"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5195df26-cf7e-4599-ae25-6546b5fd70d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "3003968e-3fb2-49fc-83fe-cdb97670283a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f4b473c-381c-422a-81c6-998fa49aa725")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7174872-d8d4-400e-9c89-a26e446ca5e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/bc303157-5aed-4106-869a-34ed21a96270")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18bc38e6-7389-4d2c-b75f-d5215417fdb8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97b45f2b-097f-400f-aea0-03fb311ead7c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "630cb21e-3325-4eb6-8b8c-f741aae59629")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf277457-ecd6-4548-88a8-270311c657ae")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da8af2d3-eed4-42c6-bcd2-29ad2a3a81a2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efdfd506-cd4e-4714-95bf-f01a721d53d4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a29857c-06d7-476c-8381-6095cc7baa04")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ac0d65a-8360-42f1-82ad-d7b46a4f3ae2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f44e2b8-0f11-4145-99a9-74a8a4bee0a2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c5c4b6b-0b9e-498d-b3cc-a84fbcdfd889")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1e088a02-023d-4432-ba6a-430a82829d4a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(D_I16-K)")
			(pintype "passive")
			(uuid "15c30ad4-1936-4c76-85ae-321e06ff56a5")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 53 "Net-(D21-A)")
			(pintype "passive")
			(uuid "fba56276-d26b-4242-b6e4-d753de5c8b88")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "805198a0-6b16-49d4-878d-f16cc7da7909")
		(at 163.16 32.785)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I13"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "6d5de591-2d34-42f1-b9b6-5fc862b0df4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "1b944168-0965-4704-8718-f9a196d8c773")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "75dd4ab2-57e4-43dc-88aa-fc9ab446d12b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e56f60ee-eb5b-4e2e-8ccf-42b0e8f29300")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/bbd8a2ad-879a-4207-8ce0-b1eae1594a75")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51eafe69-cc03-42da-a150-765a2fc1e1dd")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c35039dc-13a9-41c5-be88-45011289e93d")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e12477c0-563b-417e-9b93-58e6227be70b")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9272df77-e499-4607-a1d9-18524df884aa")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f1326b0-31ef-4213-a2e3-30a075d7e9d8")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb3abeec-db31-45d3-8342-a62fbd62818c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7754a4f-022e-4539-8877-e59e903202e5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02d349be-bb69-4def-a0fb-06d95508073b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb2b110d-b674-4cd3-bab3-7c3f0909d13a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e31a7070-53ce-49d8-b303-9a4feee15bcb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b46aecad-75ae-4c79-ad6f-c13871ab0a66")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 18 "Net-(D_I7-K)")
			(pintype "passive")
			(uuid "1e1f7297-faa9-4b36-b326-8b24deb84655")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "b1d94170-c3d7-4b2b-8fc1-eb7190c074a6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "80f414bd-498d-4262-8a6a-0a1c1c901985")
		(at 152.58 80.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I32"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "6a7ba83c-26ea-4847-a210-faa58cd720f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "adb912db-82bf-4179-95e8-de5183b45ea7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a37f992-bd63-45eb-8a93-df017d23c30a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffa01cfd-e0d0-401d-b33d-06bb1aa0c80d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/24237ca2-6fa1-4994-b862-55eb105d875a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22e621ac-b5c4-4162-a8d3-b38d0e874995")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3710ae62-289e-4237-ae8e-1bafafe0b4be")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e419de15-0ce1-4098-8e51-70b784fc8935")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f08b38b-b470-4368-89a0-12a7c8454990")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92bb351b-fb1c-4909-892e-72aaae6dabb9")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13b8fed0-db33-48e7-8be0-9a62651f65da")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7336f62a-6635-44a4-a94e-fdc4df4196bc")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13c9c30d-29d4-49d0-9dcb-969a174dc6aa")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b4157a9-d590-40a0-be0d-78b6252ab9cf")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22d3f452-4b65-482b-a7b3-ad0371806920")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "943aec65-0f44-482f-abc2-66fe7c87b680")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "0fb33fdc-35f8-424b-aa59-70071257b583")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(D_I7-K)")
			(pintype "passive")
			(uuid "75eff093-37ce-4c1c-ac67-0dfcf2caefaf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "820094e2-439a-4023-b15d-188a3364fe19")
		(at 143.08 71.275)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "94c69cc5-683a-4b6e-9bfa-62b800dc9854")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b1bab4b8-4c6f-491c-a1b2-494554d15d2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4a662bdc-acdd-429d-ae54-7d716ca6ddd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "043efd06-513c-4fc8-94e0-46723c15df38")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/957ee8dc-0ca2-4b72-baff-3753846e407a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "178d6759-b77a-4152-9b4c-88eff85cd977")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "916653e0-f904-436e-a713-0a90b9b04dfd")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2151ed1e-bf1f-4c22-8fad-a82309df6d65")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2961595-8fe0-4221-a224-bb902de8ae45")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc208c9b-0d4e-45dd-ab1f-e5f8f5420f35")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "417e20af-a028-496b-8ce4-9339e6b5bbb6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05536a7f-ec57-40fd-86af-9378696f3620")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "341d075d-e9d9-449c-9be4-c87496ccae50")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0c15972-401f-4d69-a87f-cf650e37ea32")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "997b71ce-898f-4c65-8cca-d366eed6edb8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6349fef8-efb6-4efd-ae81-7e16f142d42b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(D_I3-K)")
			(pintype "passive")
			(uuid "3024d90c-eada-4c6e-9819-45e67b7cfca3")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Net-(D4-A)")
			(pintype "passive")
			(uuid "07182374-3d7a-41c7-b396-96ad11f523cf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "82219201-20d1-4e0c-baf9-c18f09466f0f")
		(at 74.7 39.705)
		(property "Reference" "K7"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "23623ff0-b890-44a1-9f26-93f02e6330a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "1cace4d2-a517-48a6-b3d0-6e78e1a806f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4349e4ec-421e-41c6-9b35-3cf819a05e0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "df06b23a-0fea-46db-a4d3-ac27fcc86d35")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "85191371-f13f-4373-a27c-157dabfa585e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/a8e0c662-808a-4eb2-95d9-fa742942e0d5")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7bf0df1-90aa-4898-aa5f-7ecb580366d6")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87c0be58-db67-4c58-adf8-f3f50c6256a2")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3f491ac-4737-42ea-8780-dccc806bd509")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c9218d0f-af7e-453e-a556-73faa0b42f49")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e8f88579-0e0f-4165-9d24-17fb4dfe19f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "4cd42936-7404-44b5-b37e-3710401d26b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "Net-(J11-Pin_2)")
			(pintype "passive")
			(uuid "99f6f780-b0a1-4a78-81aa-1ed785d63a15")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "unconnected-(K7-Pad12)")
			(pintype "passive+no_connect")
			(uuid "0ba90adc-1ff0-4108-b7cd-b1a0b60bce48")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "Net-(J11-Pin_1)")
			(pintype "passive")
			(uuid "e2b290d0-a132-409b-bf74-f35c9eea7592")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "4eb7ced3-1615-476e-8cca-92ab9192f130")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/PLC2 GPO/Relays/Relay6_A2")
			(pintype "passive")
			(uuid "b86746d1-841e-47df-882f-9e52bc83ff6c")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "826335cc-03af-41ee-9602-c9b16c94e482")
		(at 157.33 68.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I36"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "6a56d314-a6de-410f-9e64-35012b81125e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e3483a29-569a-45ff-97e7-b557b9ee9b0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf6239f7-00a9-4ced-9508-7aa0e732d5cf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dfe174f8-a688-4b54-ab16-d59c0dafbb96")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/94213f4f-78eb-4583-b594-2c3b5d6f8261")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8009db38-34b8-423e-92db-282a263cba39")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98485c75-d67a-46db-bf34-a91ed21b57a6")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4aa3d9e9-36a3-4b17-a021-3e33dc6708c6")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34b399cf-c8bf-4e5b-b5a4-d9c283f721fe")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2942d170-e3c8-403c-896f-e59493d374e0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09d5a3f5-8bbd-47a3-b449-471350af2feb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ab9d7b5-4c27-498e-a6fb-f5afdef18afc")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d02b428-8032-48cb-a463-96ed382256b3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f80d093-723b-4be1-859f-ecc26799c718")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce22b7e3-7b2b-4098-85d7-71b1d1a0ea91")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0c1b6662-5340-4de0-967a-b6b6b37e50a6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "9f06dd3e-e141-417e-be9b-cce8ff4d74d5")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(D_I8-K)")
			(pintype "passive")
			(uuid "a614933f-2709-47fe-bb95-8b77a60a2d78")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "835201a6-91e7-4a0e-8bf2-89d5cf368ba4")
		(at 158.35 90.915)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I24"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "c6a95f0a-b763-41a0-bf74-d426d1a56166")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4a2aef9b-b55d-44d5-9734-72c7e675a53a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d707b9f-321b-458c-b8da-df055e92eb2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2483a113-20f7-416e-8287-e2c57fd46ec9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/1da63c80-8980-4afe-bfe8-d6d807fbbdb6")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e0fddfe-8ae3-480c-a6d3-6ab6a5c3a830")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20575a3e-668d-46c7-aef4-4713ea44e0fe")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "197e3dd4-415c-4df6-b3a3-de3c6e9f1ec2")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9afbdcd1-acbe-4f63-a0d4-0c3f04895be8")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6c37bdd-b23f-4793-9bda-220b849cb5f2")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4126881a-3f48-495a-a472-1a591cb42624")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43025766-d5fb-48e6-899f-a0a94a50f07c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b67e6cc-a06f-4f71-8931-52a0ef0dd5d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e6c34e9-0cd1-4859-bb5f-63ac19e88598")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b036641a-39ae-4e70-819d-973e8e96ba8e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c62b25b8-666d-4b3e-95f2-51993918bf7a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 29 "Net-(C_I24-Pad1)")
			(pintype "passive")
			(uuid "689ba61b-f6f8-4291-bbfc-f2f7ef5df12b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "ca705bde-23d2-40fc-9845-10e1767ccd72")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "83676328-cdf5-40d2-87e0-f37790d59f93")
		(at 157.33 129.345)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I78"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e9febf2c-9ce8-400e-91ce-46057e1976b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "72800cf1-fbca-4749-bb56-c8dc2794d04e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0506a3d5-3c55-4d87-a41f-af7d9ba7edfd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab6d8464-9b0a-415e-935d-8cbe02d4c9b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/61940a45-c423-4c7f-8c34-82a6fd005c5d")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5c8266a-deef-4726-a074-cc82902c3034")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa679278-e933-4619-a2be-10b5feb8008d")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9989fd8-31d5-4c44-ba62-4ae683438c0c")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "75d766cc-f26f-40a2-99e1-0cb9289d0a4c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb545d50-66c4-4899-bc80-8e76e46dceb3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "961ad1fb-047f-4cdc-b545-55889ca9660c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a02d830c-cee1-4d6a-84fd-a41d309adb66")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43ccb931-4ef9-4a20-add4-b49f36c7c0ec")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5f79b70-8e86-4c78-9622-b3c66024f191")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2c56c98-9cff-4e71-8dfd-d809f088ab9d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6760cfc9-819c-4504-a7cd-a106b3d9255a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 97 "IN14")
			(pintype "passive")
			(uuid "b757b214-8926-4294-a796-baad261da346")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "c3e229e0-f451-4134-a41b-2c9df3bd692a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "87e58ba3-7e97-437c-9e25-65875c83f3dd")
		(at 138.33 62.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1ffa1624-75f9-4791-a084-f69f061caf8c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "203d513a-cd96-435e-ac45-3849b079f8b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "47d6b545-edc7-435b-a775-60690eb5ea71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f191b6a1-6f9b-4fe9-aa0c-b9ac2202645e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9171c255-2bca-4f7f-a7d6-bf555f121482")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1f6c701-aa87-49b8-9a06-b92a9c0c1bec")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e854cc75-e53f-45fe-81e0-6ab455b2cf60")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67454338-9257-4c35-9e87-dad4445c3a25")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34a34840-4128-41b0-8c5b-67e52e400dd9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a28c3324-f7b2-48e0-9f65-2a3bee3744f6")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b469983-42a2-448f-887b-62511c5aeb21")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "760197ea-da3d-4304-983b-0119cabe7770")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cbe71bf-a445-4283-b052-ed559aa89dab")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ace2775-1616-4278-bd3c-fbbef2c74a64")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dccb29da-1e6a-4bb9-ac4e-513c0aab68d9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "04b25957-6190-440c-a67a-c515b556e2c8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "f177ae87-5336-4200-9b56-a1253197b8f0")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(D_I1-K)")
			(pintype "passive")
			(uuid "9921365e-c89e-4dc9-b966-1ab512224cee")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8844b1dc-dea1-41ee-8bb5-828b989ed4c6")
		(at 138.33 135.245)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I48"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7f5006aa-c6c6-437f-b8de-6c6da7495699")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "1fce5945-84df-46a0-b757-5f14e18ef95a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3009b33-3b3d-425b-917c-7a55f9580928")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc7ea2a9-dc58-4de7-bf7c-1195f8c091e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/7c463f0a-49b7-4fdb-a217-7efd81d04018")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69b0c89a-c5c4-45e9-87e5-498cb38acb9f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92b01a39-0e39-4d4c-95a1-556488fc7062")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72a9cdba-5257-431a-8e99-53c85be822d3")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "732c3dff-58fc-4dc4-91ae-0891e41eb304")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb0fbb6a-b362-4f4f-9ec3-9faa13bbb750")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2328f3c0-5eaa-4e2a-afb4-31496413a204")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de4bf129-33b0-43c7-ba6a-f2e82fa5a266")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e18c640d-72b3-4657-88be-3ef5599ee7d1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8126d4d2-b779-4595-8d40-5efdabdc42b5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9acb95d-3443-4c62-8d27-dab40c4feca6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cb405bb1-362a-40b3-a27a-d02d50c7c832")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "ca8a9426-8d03-4ee0-a7cb-c41a535d0df2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(D_I12-K)")
			(pintype "passive")
			(uuid "ecb10e16-814b-480b-9b9c-a6bd1f88ae6f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "88d4c2be-0346-4f72-955e-04345be04049")
		(at 6.4575 63.46)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7e392786-a070-47c5-b5cf-74b68dd86dd0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1k 10%"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "7b45c575-e7a9-4e82-b344-177be14572d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "55e7a10a-a1de-4723-90a7-ce30607c3aca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6aef9db6-95f1-4e77-a082-d222c62dac47")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/76a367a0-9747-4348-8346-39e6b2fae156")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fb42c36-718a-4bb3-8ef5-02f3aa46e2ce")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68e3e788-5c9b-454a-98bb-6e8082aff4ba")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7afcbbf3-acf1-42f0-9353-b57eb57118b8")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "357b13ef-aa00-4804-9e5b-4729349913ea")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cfae4ce-d1ff-4593-a1c6-c0202df80d2a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f12b4037-b70c-416b-8459-be87d0837097")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20f8f0f3-bcf9-4bc3-a399-60db7acb5e4e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22f3455c-df7a-457e-bd8e-af445e63e103")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dbd150b-595d-4f17-a67d-ebcb107423e2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfa49ac2-74e1-4416-865d-772b24c70a86")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3b74125a-ecbd-4fdb-9250-d0d5f00c52c1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pintype "passive")
			(uuid "0d7e8c1d-713f-4cb6-8cc1-63e565613faf")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 99 "Net-(J1-CC1)")
			(pintype "passive")
			(uuid "11dbbb11-a7ce-4e8a-9611-f3a15ea96caa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "891a3153-4c9d-47ac-9a43-34ace40163ec")
		(at 158.35 44.825)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I11"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "e97548eb-e611-4e3d-af55-b72cb3f4d318")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "9928f55c-6bc6-4d6c-8a50-f04a3587c7b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8235ee80-c302-47f6-bc05-f91d07cc4675")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "22fb62dd-1937-4a04-a277-f2d2c549d74e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/b092855e-62ce-4b60-9063-4c361aa8fbe9")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14dd1aeb-df06-45e7-9ce0-090c71c0e545")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f05ab5da-6658-445d-839c-75c7032f4b92")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b17cfb1-c9b9-45c9-a75e-9349e0d43724")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e02594fa-81a6-42cd-a88f-ac2f079ba44b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42288f43-a4fa-4ca4-a509-aa52a58a7d75")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "679b45a9-61aa-411d-9aec-0c6ffb0773d2")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9db1b1d0-ecf9-4cb7-b2d4-170868b82389")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e085edc3-8387-423c-a417-6610e4f2f4b6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01e8f1db-97e0-400b-9356-8f4c31164da2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd39f885-0d44-4a73-be56-adb0a8e65596")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "665dfb08-c52e-4a87-9b4f-497e63035383")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 16 "Net-(D_I6-K)")
			(pintype "passive")
			(uuid "3881e154-80d0-42ca-bf08-4ad628e29b96")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "9df1ada2-3c4f-428b-9b0b-1c33d0e9193d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "896c48a3-4a08-4bb5-a7ba-5fcc52aa2c10")
		(at 163.16 38.805)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I15"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "b1114b0d-b292-4223-8a88-cabbbd79e345")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "6b17c0b4-9f36-46ae-bc24-435d77802a32")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a2cb3b1-0dc6-43c3-a176-896a096fc0e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ae2663e-0477-4a3e-9369-e76423d4c3cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/48a615e9-4c5d-4bf0-9c67-ab1a87bba1aa")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3bbd5b64-229c-4cb0-a53e-28b20bee024b")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e685b2e-1bf6-445b-8dc4-9e59e101a523")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b0e9850-bd72-4cc2-bada-9bc0d1b04820")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c961cc60-40a5-4b57-83bf-6272cbfa31ed")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bde7ae1-b6ce-4b43-a635-7ab7019be745")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fb922d8-7da5-477a-bea5-ba6a066db92a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37aa6393-de2f-4e37-9bcf-902a8c28fec3")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c6c96a9-b3ca-4021-ac38-6f75aae79801")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df1d3eaf-769c-4f9a-8809-b3a5ca60fb89")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb6fd426-81e4-44ea-85a9-85fbad0412d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d651ffbe-2a24-4dc9-accb-141dded34028")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 20 "Net-(D_I8-K)")
			(pintype "passive")
			(uuid "a9db3671-b8f1-44f8-bf6d-c01482859fa7")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "013bb281-73a2-4110-a937-17d880e02401")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8a791396-f6fa-4c54-b584-8602dfbf4e75")
		(at 153.54 47.835)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "6e6ddb02-9f16-4641-8843-21c14f306ce9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c8b16754-b5d1-4ea6-98e7-af0dc3e10e54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8139ad70-5495-42b3-8dd6-7031efe4e7d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9036ede-917b-4e11-b63e-71166eb37c8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/35a9d180-c2cf-4a19-9000-ed86d8575595")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "852228ea-1818-45db-bcd9-c6d9ac62adbe")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56a34a9f-80be-4111-a9d1-14dc2ee32274")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11d813dd-1c96-4ff6-aa6f-0ec7534cbab9")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df6bd172-9033-43e6-a235-2a53438f9033")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5118cff1-02a6-4b58-b568-f2e548ee0747")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e86e91d-9c3c-444a-aceb-824290793b1b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84549459-a987-4f7d-b5e9-4154404445b4")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c7599cb-2a7d-429d-a6db-a3b40c2f2bb8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d5224b8-c604-482c-8d54-da00512a675e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "946e87cd-4dbf-4ec7-a247-a8ee71d50914")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "21e89d68-9e30-4d6b-8078-a4c0aba99b36")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "Net-(C_I6-Pad1)")
			(pintype "passive")
			(uuid "61f5e3c7-3acc-41d3-a1f6-68d7bdc413d0")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "95bf59ec-25bd-4fcd-be4e-58675c333b70")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8a8406e1-4911-4295-b92d-be134a7bee03")
		(at 152.58 132.295)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I71"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9f290c7d-a3ba-40dd-8518-9107371fa73c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "7c4bb616-a1cc-46a3-97aa-ffc0b0f07be6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "360e360f-009d-4bf8-958e-b6505d015265")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a673215-060c-4405-93d5-24991bee0bcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/5cc7e03c-efee-4ac1-9830-cbe52d23fb6a")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccdd511f-9f1f-4310-85fa-eb3a0fc11aaf")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb013c0b-a692-4878-97b7-d2580cfee6fa")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab7b5504-dc38-4482-b596-43caca9ec5b1")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7c2f38f-766b-44fd-a8a3-977ba3d8bbd7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0897a455-12c8-4139-ae09-6901a86a0c44")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8c03ea6-08cd-4615-b029-bdf17d4278b6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9625f288-d937-459c-aec7-669cb124320b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b19a309-3df8-4a65-8885-ce440c50e136")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1641d763-ff48-4ddf-b215-8697738e9fb8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de8f1588-4e7a-4d1a-87c7-280c57686f08")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1af64ae1-8498-42f4-812d-e64fd3595131")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(D_I14-K)")
			(pintype "passive")
			(uuid "218d712e-bbb5-4ec8-a08e-20d676f20c55")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 51 "Net-(D19-A)")
			(pintype "passive")
			(uuid "5717a2a8-df40-47cd-8bb7-59bbcbd906b0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8bfae0d8-f9b8-4043-b4a5-c26ca7a21f5b")
		(at -11.4625 106.08)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "2d8e1ddd-4609-43b7-8775-59120ed0e61c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "f2191c44-9011-4fe2-aea5-1e07dbb8373a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b897208d-7548-4c39-b096-0665618916b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "53788bc3-9e5e-4e7d-81b7-7cad031f853e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/73abc1c8-c9f3-4549-b911-956d6b08dc3e")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a245cc9a-ee35-4e46-8bf1-7e8c941aae19")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bffaee1f-3ede-4a98-bda1-67c4b943c836")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "daf09c7b-cdc8-4296-8bef-98e4af0c4e0c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "963f7dcc-0bac-4e08-b567-0d658d6502bc")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "035360cf-34d7-4100-80cc-22ebb662b54d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e74cc1d6-9ae4-4477-9e26-adfaa5a9b859")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7bf831e-6de9-4074-b74b-6d1566a16948")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "108748ef-aeb5-4c9d-80d8-be56a78ec575")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdb97ad3-fd6a-4aa3-8a12-07ee169ad153")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8fab328-4d7a-4ddd-aa3d-2cc1212f48d3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "35e71dfa-c787-4181-a4c7-c6cc3ccf7844")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "f4724281-e8bb-4222-9b54-900ecd76cf4d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "37ccf36d-55c4-4f41-ba60-0970216187e9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7051x"
		(layer "F.Cu")
		(uuid "8c6304f1-1c30-4cc7-a069-887440f80ce7")
		(at 3.5775 93.03)
		(descr "USB Type C, vertical, SMT, https://datasheet.lcsc.com/lcsc/2108072030_G-Switch-GT-USB-7051A_C2843970.pdf")
		(tags "USB C Type-C Receptacle SMD GT-USB-7051A GT-USB-7051B")
		(property "Reference" "J1"
			(at -2.5 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "e8aebb3c-ea94-4f43-9dec-65a7f208a6d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 0 4 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "0e4b42e4-f92d-43ba-be06-0e5547d14e17")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54efb645-ae2a-443a-88bb-091d70f8065f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1022f828-7a0a-4748-ae54-f489e3578984")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/1eb5e5a4-bb78-47df-8ead-f22b16b700a8")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.42 -2.17)
			(end -4.42 -1.67)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4732622a-e612-45f8-bf9e-9319b3e41a18")
		)
		(fp_line
			(start -4.42 -2.17)
			(end -3.92 -2.17)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe911e1a-180e-40d4-8ba3-36219f6426b0")
		)
		(fp_line
			(start -4.27 -2.02)
			(end -4.27 -1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92266e84-4aba-4051-9220-d599e1a01ffd")
		)
		(fp_line
			(start -4.27 -2.02)
			(end -3.47 -2.02)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f497796f-0660-4481-9199-98f7d89b4d44")
		)
		(fp_line
			(start -4.27 2.02)
			(end -4.27 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d861876-9f57-413c-958b-56dd2320f81b")
		)
		(fp_line
			(start -4.27 2.02)
			(end -3.47 2.02)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "437efb32-022d-4bc4-aed7-410f14bfe588")
		)
		(fp_line
			(start 4.27 -2.02)
			(end 3.47 -2.02)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30a218c8-e3ec-47e1-8b33-fc8d2705ed57")
		)
		(fp_line
			(start 4.27 -2.02)
			(end 4.27 -1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2e7d363-6a8d-4477-a0a3-8e203b416f82")
		)
		(fp_line
			(start 4.27 2.02)
			(end 3.47 2.02)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af55fd7b-161e-49aa-a5a4-baa7af2be648")
		)
		(fp_line
			(start 4.27 2.02)
			(end 4.27 1.12)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3b6de63-ba01-4ec7-b257-ad3d2c0829de")
		)
		(fp_line
			(start -4.97 -3.2)
			(end -4.97 3.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "199d2a52-04d8-46bd-b839-59b9be2eacb9")
		)
		(fp_line
			(start -4.97 3.2)
			(end 4.97 3.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b8c98cb-75f3-481f-af1f-91f7275eb362")
		)
		(fp_line
			(start 4.97 -3.2)
			(end -4.97 -3.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ae7385b-93a5-4ac0-9f2e-a44d267ebc4b")
		)
		(fp_line
			(start 4.97 3.2)
			(end 4.97 -3.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "654739e4-9f41-472e-b914-6c4543f4152b")
		)
		(fp_line
			(start -4.15 -1.9)
			(end -4.15 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d25949b7-d135-4919-8fb8-159bf115da1e")
		)
		(fp_line
			(start -4.15 -1.9)
			(end -3.35 -1.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "278c2de9-fe59-4a4f-b0b4-97a2f5f73e82")
		)
		(fp_line
			(start -4.15 1.9)
			(end -4.15 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b5c79088-a332-406e-978a-9c9bb0cc8869")
		)
		(fp_line
			(start -4.15 1.9)
			(end -3.35 1.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db436765-bb3a-4a21-9a47-877a233f5ed8")
		)
		(fp_line
			(start -3.35 -1.9)
			(end -3.35 -1.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1ed1285-54da-4a90-afc6-20e25c2a6a6b")
		)
		(fp_line
			(start -3.35 1.9)
			(end -3.35 1.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f0d5fc1-85b4-4bd2-a3d9-0a353020a860")
		)
		(fp_line
			(start -2.89 1.58)
			(end 2.89 1.58)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3880653-b6a2-4e28-842f-1a9a2c3bce45")
		)
		(fp_line
			(start -2.75 -1.26)
			(end -3 -1.58)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac51b68f-6687-498d-b527-adb8d2f4194f")
		)
		(fp_line
			(start -2.7 -2.15)
			(end -1.7 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ceb838e7-c9fc-488a-8651-48659f9869c8")
		)
		(fp_line
			(start -2.7 -1.6)
			(end -2.7 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44e1a91e-5957-40db-8968-e7e22048ea9e")
		)
		(fp_line
			(start -2.7 1.6)
			(end -2.7 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3f19668-7018-4beb-a988-3c37e31f21cf")
		)
		(fp_line
			(start -2.7 2.15)
			(end -1.7 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8069498f-c692-48b1-b205-8e0568e241c2")
		)
		(fp_line
			(start -2.5 -1.58)
			(end -2.75 -1.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5af1dbee-a438-4b71-a61c-6827dc4afbfd")
		)
		(fp_line
			(start -1.7 -2.15)
			(end -1.7 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7db74173-1523-4f22-9edd-4ef9077f447d")
		)
		(fp_line
			(start -1.7 2.15)
			(end -1.7 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71924f62-d732-4b2c-941c-b772487eb342")
		)
		(fp_line
			(start -0.5 -2.15)
			(end 0.5 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e49b13f-9584-4fb5-9441-ee797fa4c6c4")
		)
		(fp_line
			(start -0.5 -1.6)
			(end -0.5 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f75be6af-5172-4961-8d60-72230436f7b9")
		)
		(fp_line
			(start -0.5 2.15)
			(end -0.5 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ae7b157-6c64-4b66-b0eb-ce8c15c62c5f")
		)
		(fp_line
			(start 0.5 -2.15)
			(end 0.5 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "468ece67-6af2-47da-8230-432b1cbdad27")
		)
		(fp_line
			(start 0.5 1.6)
			(end 0.5 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2e8565a-2056-47aa-bc1f-34a30ebcfccc")
		)
		(fp_line
			(start 0.5 2.15)
			(end -0.5 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72ce7f78-2176-4808-a1de-5973f21da94a")
		)
		(fp_line
			(start 1.7 -2.15)
			(end 1.7 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aae0d5b4-2567-4224-886c-b3ba5274ac58")
		)
		(fp_line
			(start 1.7 2.15)
			(end 1.7 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf17a1ea-44b8-485f-8de7-a44581a12cb8")
		)
		(fp_line
			(start 2.7 -2.15)
			(end 1.7 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "954803c1-f8b2-4d55-a5a9-1d2905762dcc")
		)
		(fp_line
			(start 2.7 -1.6)
			(end 2.7 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4de4d892-3c2f-44e5-891b-b7c7a17f4985")
		)
		(fp_line
			(start 2.7 1.6)
			(end 2.7 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d71230de-4b26-46dd-bea7-45adaed9128e")
		)
		(fp_line
			(start 2.7 2.15)
			(end 1.7 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35f414df-2663-4b19-960f-24883e2aaa45")
		)
		(fp_line
			(start 2.89 -1.58)
			(end -2.89 -1.58)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0eb73225-87d2-4fb2-bd98-f0a317191217")
		)
		(fp_line
			(start 3.35 -1.9)
			(end 3.35 -1.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "916f0f7e-bed9-4d66-a896-69093ef8eaf7")
		)
		(fp_line
			(start 3.35 1.9)
			(end 3.35 1.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "704fe271-7838-4e30-8c30-45011eba0bb3")
		)
		(fp_line
			(start 4.15 -1.9)
			(end 3.35 -1.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aff6bccd-d2bc-4325-bd71-c6cc09f09086")
		)
		(fp_line
			(start 4.15 -1.9)
			(end 4.15 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26255a30-3534-4432-96dd-38a8e0f7731b")
		)
		(fp_line
			(start 4.15 1.9)
			(end 3.35 1.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d693795-ca5a-4659-9f62-45ccd34ba453")
		)
		(fp_line
			(start 4.15 1.9)
			(end 4.15 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5653334a-2eb0-4ef7-9499-8bd698939ba8")
		)
		(fp_arc
			(start -2.89 1.58)
			(mid -4.47 0)
			(end -2.89 -1.58)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51471bef-1390-49af-b477-1ca62e58d431")
		)
		(fp_arc
			(start 2.89 -1.58)
			(mid 4.47 0)
			(end 2.89 1.58)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c67a00b-d76b-450d-89fb-6e1c7cc01f75")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "ca379db6-0b1f-4498-a9b8-1c104484062a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -3.75 0)
			(size 0.66 0.66)
			(drill 0.66)
			(layers "*.Cu" "*.Mask")
			(uuid "e1ac0acf-82bd-4a48-a01c-b3b8c40174dc")
		)
		(pad "" np_thru_hole oval
			(at 3.75 0)
			(size 1 0.58)
			(drill oval 1 0.58)
			(layers "*.Cu" "*.Mask")
			(uuid "ef33b2a4-d05e-4768-beb4-23a3541c0b2f")
		)
		(pad "A1" smd roundrect
			(at -2.78 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "76bed270-75f0-4ce3-a870-241721fdf6ba")
		)
		(pad "A4" smd roundrect
			(at -1.99 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "94ab7d21-c8e5-497f-89c8-a3e8506e99ab")
		)
		(pad "A5" smd roundrect
			(at -1.2 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "Net-(J1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(uuid "2d97b0c7-5f70-4d0e-a906-52f7149651ad")
		)
		(pad "A6" smd roundrect
			(at -0.41 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "9dcad9a9-40e9-456a-aaa0-163c699ad103")
		)
		(pad "A7" smd roundrect
			(at 0.38 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "82572da5-1bc6-4fae-a957-735ad22c4c1f")
		)
		(pad "A8" smd roundrect
			(at 1.17 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(uuid "751a1a2c-0cf5-4744-aa37-c378b589c594")
		)
		(pad "A9" smd roundrect
			(at 1.96 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "646d9676-74b3-484a-9dd5-49ccdfb25a5f")
		)
		(pad "A12" smd roundrect
			(at 2.75 -0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "0753f549-3698-4f46-9520-bac0a5a82bdc")
		)
		(pad "B1" smd roundrect
			(at 2.75 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "b1a1df36-c786-4df9-a09c-b99d3b9b0518")
		)
		(pad "B4" smd roundrect
			(at 1.96 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "145c8e23-c4d0-47bb-9cbd-22292391be3d")
		)
		(pad "B5" smd roundrect
			(at 1.17 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "Net-(J1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(uuid "89dd60ee-d01e-44ab-92f9-2e26862b1614")
		)
		(pad "B6" smd roundrect
			(at 0.38 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "ead7c0e0-dd0b-4f3c-9261-7cec64a7dddd")
		)
		(pad "B7" smd roundrect
			(at -0.41 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "2dec9d80-f661-4b34-9373-07a14ecc7a24")
		)
		(pad "B8" smd roundrect
			(at -1.2 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(uuid "b0b154b5-6bc2-4e07-838c-39aa6397da0e")
		)
		(pad "B9" smd roundrect
			(at -1.99 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "b110cbf8-6a89-40a0-8ee9-7ddbf6b4777e")
		)
		(pad "B12" smd roundrect
			(at -2.78 0.76)
			(size 0.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "581d87d1-7ad2-41d3-8143-3d0781b5b7f6")
		)
		(pad "S1" thru_hole circle
			(at -2.4 -2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "3b684876-abea-4446-b99c-87b4abe27bb7")
		)
		(pad "S1" thru_hole circle
			(at -2.4 2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "36a816a3-bde7-4254-af25-d6b99dcdd9c7")
		)
		(pad "S1" thru_hole circle
			(at 2.4 -2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "f6873a9a-27af-48f3-ad80-1512fe68d7fa")
		)
		(pad "S1" thru_hole circle
			(at 2.4 2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "96f8b6c8-3c8f-4bb6-901e-2c61001ee34a")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(uuid "26fcc60c-74c3-46a7-8865-b55e881d7775")
			(name "peg")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 4.3775 91.23) (xy 2.7775 91.23) (xy 2.7775 90.53) (xy 4.3775 90.53)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(uuid "3fc5fa1d-9efd-422f-99ed-1ea4a726679e")
			(name "peg")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 4.3775 95.53) (xy 2.7775 95.53) (xy 2.7775 94.83) (xy 4.3775 94.83)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7051x.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "8d1e1c20-8583-4180-8eb8-673e9e827c4d")
		(at 203.04 140 180)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J8"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "4c166011-c8b4-415b-b99d-cd8d5a94fab3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "a3b24acc-74d5-4a8e-9657-15067d3aca0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d200f4f3-04f3-4154-bb37-054255855fac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac54236e-52ed-45a4-9aab-ba37c2e7ae89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/88392161-d1bb-4f95-822e-059b0fd8b7d4")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee8ec735-9254-4b70-b71a-5ed05a8f4d6d")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df325981-85c7-44e0-97bf-09b744b1ec21")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "791efe85-3d0c-40bd-a035-04195e00482c")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c95df72d-8f53-429d-8f87-b563bfa6b517")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "645cf1ad-0a75-4447-b2c8-5d16eef4630a")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bcb7e3b9-67e2-463c-83b0-49d40d7f8ea6")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "810ba0fb-f891-4abc-b71c-494f77a3cc0e")
		)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ff28650-1984-437e-be54-0c64575763f6")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "441c870c-ff1f-4fd7-9cba-6a98802e1acd")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67ba92a5-775c-44ea-8c60-a7bef2eaacb1")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a6c6323-4fb0-4c97-9778-5f5640cc3557")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8ecaa63-9bed-43de-bb90-cb1e7a259f72")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "199f8a21-9dba-443d-a0d8-1045d9c4c494")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8206ae7-5c23-473a-ace4-65ad082169c2")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bc1c7f4-a93e-45f5-9986-d703f001c131")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82f8f512-6b2c-4705-a382-6c914f54f565")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2851e82b-c059-4712-80ad-fc64c86a113e")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fbbf937-f04f-41ec-af67-8c325e61403e")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad6beb7c-a9b7-4030-942d-ef2970580ef6")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5871c32a-b4c3-4276-9444-8cfae4c6116a")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d06dc462-6ce6-4122-bb13-c91c9fb564ca")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ed6ea0a-f206-4e66-8b02-092eefd886d5")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fe3be33-84e6-424c-887a-948371188f98")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5218d296-2939-489d-84e7-1e1ad48ad3fb")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b639ebd-e545-4372-8549-61bb9dfade14")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "645f6547-9470-43ca-b02e-f7f44724af49")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cffffc9f-b83e-497d-b5b6-1dc0c44946bc")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "45d0944c-af74-408c-a649-223a6f469e2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 119 "Net-(J8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7f441d16-dd82-4183-a7fe-fd284568f453")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(J8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "23c8727c-9d29-4c49-86f9-61e4b5bd975d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8da5c31c-5e58-44e4-9f8a-637373743295")
		(at 157.33 126.395)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I77"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d42e354b-d497-4592-82fb-dc8d39c4c4ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "20b0f4f2-a04d-49e0-b2d9-1c05b5451e93")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "539f8e00-ae15-4314-81ce-5b47a1fdc032")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4ecc66e-0c98-4560-a05a-af5d2bfd6031")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/3dc81a5d-3a62-4d4e-b05b-5cc63ba2802e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5e37cd4-4ea0-49de-89db-06dda41935d1")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed1041dd-4cc8-437a-878f-5578439c7f4f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a9ad398d-4ea5-48ba-9374-24957cdd9972")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "517ecdb5-2b10-49cc-aa29-1754cde902d8")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35b673a4-e8a9-4afa-8938-3a7c014cffb7")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fac5d0f3-2b4b-4840-86ac-3f3dee066f8b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5266f079-372a-44ff-8a3d-e3a6eece6a2e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94cef91e-a918-4a18-8c0a-71555cee2617")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43b76cca-59df-4c2f-8197-d29a93675200")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0727039d-d8de-418d-9e98-2ac2fc91c23e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "74e3c340-31e8-4ed1-a9ab-027c015660aa")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 82 "IN13")
			(pintype "passive")
			(uuid "a7332126-a833-4619-82b6-f7532ba2515c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "e6738427-9333-4416-9184-0a10e78f46a4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8dd23363-3ab7-4837-a796-5c354d18bdf2")
		(at -11.4625 82)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "6307a8d9-49a5-40d6-8000-9c3ff4817104")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4u7"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "3d6f2029-33c4-4948-869a-3d62d3e264b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "def6f336-199e-4839-89d8-7e7fc1564389")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2172c639-bf42-4909-b32f-6fd35716a8d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f591595d-5f0b-4e1c-a559-15ffd1a9d30e")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dab3449d-eb0b-464e-b128-fbda28aa20dd")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fc5acbc-8dac-4de1-821e-072b3140ad42")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb712c8f-44c6-466d-b252-401657b7d4aa")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e622747d-73e1-4a41-80fc-d9e000bad849")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0da487f-553c-4198-83d9-653a7061afb8")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bfa3cc3-16fc-48e1-b97c-7102062fbdf7")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1b933e5-3fd1-4ab9-b5d4-8dd71c1a5157")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57c9e326-a1eb-4200-ba0f-0ac9dcac10d3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fe6644d-2a3d-4063-b741-9b6bc09670e4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "046ebe89-993b-4f03-9e57-76c2556b8a3f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e677005f-674f-4923-bb45-1da8a263a0f7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "5V")
			(pintype "passive")
			(uuid "63aff2a5-ec14-4ed8-92d3-c53668033f3f")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "ebfa8228-2659-423c-878f-04984a3ea07e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8fd9873e-8f3d-433c-a2f4-17344646081b")
		(at 152.58 77.175)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I31"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1be7c35e-6600-4ea8-a165-d4d8f1d24586")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d51440da-26a2-4701-a2b4-cf9792a19f06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f8f2c3a-91c2-4f7d-a9fa-e26951eedbdb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee844879-1f2d-4d45-925b-a23ae739aa0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/68b9bd0f-4918-4619-9bb7-ae1efea23c2d")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "85ce8d5d-54d2-448e-ad13-90543428eaef")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "017e184c-0364-40e1-9a29-6c3d9b024ed1")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52dffc2c-263f-4baa-9037-13d368c88b6a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d4ff4b0-6e93-4d15-8f89-2c20b866846e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "36ca3711-5a04-4f69-920d-f7b0454cc2d3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec2c2df7-7798-4776-9083-444a0bd241cf")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da71d346-08cd-46a5-80dc-1544ddf4d460")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9f8feb7-b718-4e08-865a-33d0204d2011")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b43753a-7e6e-4435-848a-360a93bf949f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b19ba74a-99dd-4459-bc23-b1f1fec22c31")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "257ee20b-81bb-4796-94fd-1ce3498056ae")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "80e3adfc-4114-448c-89c6-a6204b911505")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(D_I7-K)")
			(pintype "passive")
			(uuid "a2b9fd67-e445-46b4-aa6b-401575eaea7f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "91712c7a-959d-4cd4-9f43-37c0c8c57b98")
		(at 138.33 65.375)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "abfa4b41-abff-4233-9a24-889401d80bb1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "8b99b81c-32a2-4f8b-8ece-a3aa959a57f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0a0832a-6503-4aec-b5e6-e57c45f1ab1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "abe41adf-9ebf-4cab-89d6-c6707550ee91")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/0ef67d65-e3a2-45f8-9619-07e5a5be4938")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4c3974a-87a5-4077-8a9c-6310f51c4965")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ba03719-9cce-4ea5-aa1a-4d1c7e40ad35")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "710df66b-ddb1-49e1-8069-daf023944230")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "699476c4-1b08-412b-a2b9-f6b12cb7ed74")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58b5d689-43b9-4630-839b-27be0b7ed0fb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9133f68-5aa3-4b7e-b101-5d58f41affdf")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db9dbd0e-c57b-4392-8dfc-58a99753822e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b433b6f2-4f08-4ce1-9e88-4c038e91eb11")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63137131-091a-4805-b62c-fcc8f762ecd6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81b251d9-b2f9-4647-98e8-61c8df4b37dc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e10d2237-b66b-4092-abfd-c841394f1c49")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(D_I1-K)")
			(pintype "passive")
			(uuid "276049af-c028-4adf-a237-f4af0547a740")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(C_I1-Pad1)")
			(pintype "passive")
			(uuid "236eefd6-adf0-4171-b016-f98bdcdd25cc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "95fe8e14-ce64-4a3d-8481-1417f0f79db1")
		(at 54.15 90.255)
		(property "Reference" "K5"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "f2dadacd-3c6c-4fa0-b751-97f014df4a57")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "ee6be6ff-af4a-4285-a05d-bc53c97a567d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94138da1-3c44-446c-a74b-8cbd82b16426")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "14066f27-66ac-4003-99f6-7036de7cb61f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "581ef464-b1f2-41b8-bc37-cfa2cf233201")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/3a356c72-6ad6-4a41-b1d8-0ea2c5635be8")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a619a50c-30ee-4d75-9064-c268559fbaf3")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c04b6f69-f35e-48c1-9389-7850b40085fc")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c558ed87-c7ac-4d4a-a9e0-b360187ea256")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "47b18876-a526-422e-aba2-822e42bc306c")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "23d29f2d-3fe9-48da-808d-f3687882b277")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "5b91cb86-5894-4063-9ee6-1d2c61e555b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(J9-Pin_2)")
			(pintype "passive")
			(uuid "f33b55a3-7a57-4e04-abc0-ee2337fe4782")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "unconnected-(K5-Pad12)")
			(pintype "passive+no_connect")
			(uuid "32b06313-0b33-4f4b-9ef9-4a3d65314d06")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Net-(J9-Pin_1)")
			(pintype "passive")
			(uuid "0b5960ec-4d19-43f7-8a84-34e0043e05b0")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "49796953-e45e-455b-a9cb-0bdf3f7302c3")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/PLC2 GPO/Relays/Relay4_A2")
			(pintype "passive")
			(uuid "44537281-871a-4f3e-816b-5f699f592dd6")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "98b88ef9-2489-47b8-85bc-b1d1896a9634")
		(at 143.08 77.175)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I15"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c591b346-4c72-4675-92d1-8e33f195d9be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "6437868d-c52e-44e1-9221-1ac21e346a21")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "33a484ec-9ff6-4d2b-8f34-17a12dc888d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "930ecfe8-ee90-4a40-85e6-b472b33d9ca0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/961c8c5b-fcaf-42d1-bb49-85af5050a643")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b9715ad-7bd7-4c70-b46b-68bcccc6e3fc")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92416b64-c9dc-4060-b89c-6a5e42b4d884")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2d08fd2-15f4-48e5-97fd-5fcde80a9909")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89acb072-44ff-4fb4-8f80-d1f24c36b08b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbee5b28-c235-4e2b-88dd-f698ccc2e5ad")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4486f41a-09d3-49f1-aec5-f77b6cb4034d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33e9f6e7-18e1-4eb3-a7b5-d0eddc096c00")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87f685d7-0aa6-4a0e-8b9b-2e318f4142c5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0983e3fb-67de-4852-b945-12e761e418ce")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f97575a-f5d5-4599-bf6e-83174b58aece")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "54a1bb2d-4f38-4552-9af4-3a84bdffd974")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 88 "IN3")
			(pintype "passive")
			(uuid "8ecdfefa-0e2b-4805-9e10-ba5b06cac8d9")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "1170367c-7c5b-474e-b576-0b4e6ea6a45e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9b24be4c-8e22-4466-bb43-cdd2b2730c10")
		(at 143.08 117.545)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I50"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "4e41e16a-f8d4-4157-911b-be3249ba3e9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d6944411-337e-4396-91b7-4571378ce5c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e67e9473-8f02-4938-b40e-c5d0431fd230")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "64dbcaa6-e345-4dbe-a8f3-8bdec25b448d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/70112f8b-ed39-4049-946f-5abbeab12e01")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e955b58f-5473-4395-8e1b-7347f15ba938")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e564ec8-d1fd-452e-b69c-9263614ccb8f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "276fa423-e1ff-4e05-a992-64394912d8e9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af751f8d-7f42-4577-a070-7ae53fe6b87d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbf728d2-950e-44c0-bdf8-123d4aed748c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27227935-c92c-4dc4-837f-95eedd086a64")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04034d0e-3bea-42f1-bdf1-d05e4ef7c47d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2b85100-bb41-4b1b-b6e2-90d5fa05503b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "061b7625-11f9-4794-a31b-393f64b1a075")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35f15cb8-702a-4524-93cd-f20b5611c5f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "48ba1190-2ff7-47f5-b5c7-f7fa687899c2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(D_I10-K)")
			(pintype "passive")
			(uuid "06369d11-07f9-46e6-8000-02eefca47f3e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 47 "Net-(D15-A)")
			(pintype "passive")
			(uuid "58e6fae4-952e-4b4e-ba06-aff663e37a88")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "9d8b3eb4-b6c8-4ac2-a52c-44abe88b0de4")
		(at 141.175 101.43)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I13"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "dff41efb-3ccb-404f-86a2-fb334a0a98ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "24a9bd92-dbed-400a-b9cf-4ba65840b2e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3afbc166-10e9-4bb2-bb58-e77ac6872a02")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4285289e-6a0e-488a-b1e6-5aaa9632a35f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/cd04cbc8-16d1-46ed-a037-735eddfe6370")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c4dcd37-e391-426d-8a8f-bf5fc6f40081")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5160d8b-2abc-44df-805f-897f0153a0a6")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "885d3536-59fb-443f-88de-09cd15ae9608")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "031fc656-021b-47a7-82f1-6b32c610e4e4")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3b6ab0a-65f9-4ff4-910b-49cf58449f77")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bf2c921-b2a7-443c-b856-3b39dbfd2ffb")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf772e27-67e8-4ff2-991e-12e431e57769")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58eb850c-6aaf-4704-af70-6c9d1ccd0379")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fce16b39-ebdf-471f-8f7a-f128ab312e12")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cfad121-a83d-487c-bbae-d06f0cbef20e")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fed3e262-2e52-4693-bfb2-b1d9b2c8cbf9")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04a0eb88-095a-4288-9aa7-bcb4c3ebb5c1")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "838a2909-397f-4e8b-805f-f54a79a712fb")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c125964-3b24-4f53-8032-8f36a53bfc43")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6a97bca-02c8-48b2-8d31-b8298488c611")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b62fab9-0ab0-480c-a107-e0479be35984")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5dafa2d4-9316-4ab1-b186-099fb2c6160d")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eea2adac-f35f-4b10-a35a-023592576d46")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "47e86711-1c8c-47e1-b6a8-924e346cdbf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 30 "Net-(D_I13-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "f87b047b-710b-40d7-b1c3-540ca7df84ed")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1eea6835-6643-4971-a4cf-76bfa5ef1662")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9e3de195-4674-42b1-b04a-f0619ec21604")
		(at 152.58 59.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I25"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "79541231-fdff-40eb-a754-0cad5a2f56f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e9aa1090-1632-419c-93f5-cb8921ca43f7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0844f2e7-cdde-4adc-86c0-4a6df951ec5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4f94759-6b57-430d-a9cd-603b5412937f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3f607dc0-da34-41cc-8c42-df361945c0ec")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad58fc16-175e-4e15-859b-862ea18cf7bb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac23f32f-1ed4-41c2-8a15-51b0051dbdf6")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "524b40e5-05ea-4136-a1fd-50cffa02fd4b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab7a1475-89e1-4ee2-9078-196d4fccc820")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d11373b-6928-4a7e-a016-96baf4d0b163")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f227b6f-e683-4a9e-a44c-71068bb9ecce")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca089758-3ebf-4489-a22c-b214996aa84b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80d05295-b3a7-425d-b9ff-e09d2467b44f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69a0a49d-0bf1-438a-880d-e4764f2743ce")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9984ae09-3a21-4394-a133-2eb8428bbdd3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f9459ab-5262-4eb4-ada8-c71a8cb533be")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 83 "IN5")
			(pintype "passive")
			(uuid "de1cc561-395d-4ddd-be14-61dc6623bd10")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "fdeceec1-6646-4078-bdd6-26ef235b2ecb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "a05bba64-d625-40c9-9205-a3195b3035a3")
		(at 141.175 98.09)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I12"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "ee23fa81-004b-4d97-92e3-6b83018717c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "1cae5c9b-dbd6-4d13-982f-4a3489699255")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65de3b53-4e1f-4cf4-bddb-9d730feac590")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d965fc34-c2af-4a3c-9551-3a29e12aa20d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/70befee9-5279-46b3-8729-9b426fad80ae")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ddc79b96-894c-41f0-a3ca-27a6ffa1e1da")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8983acee-386c-429c-a210-ad2df912d419")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbe0f12c-d193-43ca-8ec4-433dc8fffdec")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acf25b07-6e28-4a17-9860-6a6979bfbbb9")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "110d0e98-a0d8-4cb0-a724-9b1d0d15eb02")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd43dbb1-fa4c-44df-9ae3-4aa3fdee0c5e")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "deba4ca3-4798-4871-bcdc-89cff31d18ff")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52abc267-3819-46d9-b1dd-4133af23ef33")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9f13826-0b07-4d43-85fa-fa4ca8ea96f8")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21e46291-43a1-4673-90c1-cc1d966be842")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2be20b95-fcb1-4a81-8cb1-33c31d1f5059")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cfb67688-4311-4a2c-ba5e-599ed7fc4801")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2688bea-2b5f-4551-b146-c8ae490204f2")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6eff432-b46d-4324-a8af-98b1c7e6771d")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b5faff46-c79f-4844-af55-35980e399fa1")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed5745e5-3198-4c2d-b797-8742d4ac4df5")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9c650cf-0041-49fb-931e-a00858772ccf")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83e48c22-5ebd-4e77-8663-bbcae0396a91")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "87b1ed55-6702-4cc8-9e04-c64097827406")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 25 "Net-(D_I12-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "d97821e5-caf2-4f1b-acfe-236b60677e26")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "d815fc6f-ad7e-49a9-bba0-34032b862528")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a14dce6a-4f2d-4c25-b1a2-17008d0520ea")
		(at 157.33 74.225)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I38"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2f61c4cf-5523-415d-b263-a0f8cdbc9659")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "67a20058-40a9-4b02-ac45-84bffb5e7b91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "abca4b1b-e793-4ab9-9e13-8f3e3405f212")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "231a751d-a578-4bd9-b09d-e84fe5641c0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/02074335-de9e-4439-92e1-4b5ad221a071")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a78d631-d785-440f-afa9-bd201ed871c8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49939944-43a0-4a8e-ae17-6854e51223c2")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "484dde6e-d9ea-451b-b1a1-a385449193e3")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "511c32d2-6f17-4af8-b8a7-01ce62fb0f83")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb82d800-c4fe-471c-9192-85a4aa8e0dbf")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21ab02cc-9b7d-47a4-82b3-e8c3244b5aaa")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22875678-8b0f-4277-a1ad-30401a67b8c6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b8995dd-8bb9-46fd-968a-6eedd0d6b04c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c359e4e2-08e3-46ac-8adb-e05c78169449")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7dbfa64-f767-43c0-88a0-0d76801c6d35")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "85ba6fa2-5c00-41d8-93c3-8188a9f6c474")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(D_I8-K)")
			(pintype "passive")
			(uuid "adca32a7-6754-4c79-96a3-c3f4c220fdcc")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 45 "Net-(D13-A)")
			(pintype "passive")
			(uuid "fd11aa89-ae64-4b47-bb6f-d97295f18015")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a4d1c170-4a00-4078-9202-dac46b32ed53")
		(at 143.08 59.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "399dbe48-e908-4a1e-bf4b-a3ab07dc60c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "600812f2-da4b-403e-bf78-e5208700c15c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d872f508-0e01-4b6d-b77c-869088e69278")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "63dc922b-eaf8-4bb2-bbdb-65dbfc440839")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9303cf0a-8655-49f9-95f8-cef67481286a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8dd6c1f8-a1af-496d-86ac-78404392d491")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "faae28d3-00d6-4155-9bca-a2e42034096a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c470c12-f05c-46a2-90ae-2e46f8d7702d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "446a4ea9-a28a-45c0-8f83-027ee28adce1")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4449a27-3bf2-4def-95ad-c86efc14a42e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d89bd47-2b98-4e9f-a182-321c8f0bda21")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "094532e3-4799-4257-8364-545d70ee1274")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "174cc1b5-a62c-4ef6-954a-954d0858e9e1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7bcdc891-e8cc-4b94-9e28-06856fd562f2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34548427-8e9f-4294-a4ee-03bf2fdf89d5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "695697f1-4544-4838-9f98-905c3f17d3fa")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D_I2-K)")
			(pintype "passive")
			(uuid "ecaf6a4a-2f53-4ffe-aae5-b12969dde09e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 9 "Net-(C_I4-Pad1)")
			(pintype "passive")
			(uuid "689a4af7-9392-423a-b09f-0ae66ced7901")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a51422da-fd06-4018-8706-8f9106ebca3c")
		(at 147.83 132.295)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I63"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "364d78cc-1458-45b9-a10a-aa7eea46f632")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "77345c58-35bc-4257-90ac-75edcc95b8f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7d80d8c-ac8f-4aad-a54b-1bc82054c119")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b02ce25d-1788-45e5-a8a1-37f388924021")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/cbcba419-a81d-4540-b490-c3dc1a681fab")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e77c6ad-6df5-4eda-9bb8-c4c8842b84f0")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d305a5dd-4448-4a14-8b8a-76d7148efa4f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec0feb56-429b-42ae-b019-ca09a0ca185d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "32ebefc9-eec8-4acd-9f29-f50148a0ef63")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "616d72f9-265d-4378-9278-2c1d20e383df")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "509016c4-6ea3-49b6-9d33-12ff1276ba14")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d058a4be-5d06-42fa-bfc8-e8c2a86206f4")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6189f19c-2e2e-4f5d-ada8-ac6b116d3475")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f5b9337-f89f-42ae-80d3-b64490d508b5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e281387f-3d22-4fbd-b5b0-a18b393556ae")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c9bf5dbe-cde8-43ba-a3f6-b9e9012aea72")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "62fd3174-680a-49ab-8dfd-5077addda117")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(D_I14-K)")
			(pintype "passive")
			(uuid "66968bad-49e9-4682-930e-b206b8521a24")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "a6564be5-3b28-4256-9d72-d337e6690657")
		(at 126.76 79.805)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U16"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "34922b39-ea11-444f-a3ca-a647e265c8df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "849af06f-f1ba-4c58-987d-a9c66d4f9c08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d064f96-1d6f-46ca-9fc4-2c8d21339a4f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4bc373df-2cf5-4715-8a51-50c903bffe18")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/943b08bd-68fd-46b5-8c83-a96dc7993f40")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "514ab490-f7c4-4172-bd5e-2614cfc6f68f")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b443b10a-9d56-4324-bc78-ecb50949b907")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2426e1d-a7d1-424a-8c5e-5028d4f3bfbf")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "636bfb7d-9f5f-432a-9d4c-518189e01658")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb9ada93-3201-4a7a-85cf-2ad46621deee")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd347bc3-8156-49a1-8855-2e9bea7233d6")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "95c6de3a-74b5-463e-826c-96c2bad07376")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57dd3bee-416a-40ff-a5d5-834f97307bfb")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fee1afe-03fe-4707-b363-e7edc4ad01b6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d619945c-6d65-4b41-a42e-9fe860a08fb1")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59fcf87e-1b84-4fe4-b1f5-aae7dc92cc63")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8462ac3-be7a-43dc-9d36-eaa46fcb8a34")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "4087df02-bcac-4a42-8d60-778cbbbbb7de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 21 "Net-(C_I16-Pad1)")
			(pintype "passive")
			(uuid "2b112afb-74f8-48cd-8c5b-7da596ef3c24")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "3a287009-4a4f-44ae-89be-d43416205cae")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "943d5a60-72de-44be-946e-3ff58b5656ef")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "/PLC2 GPI/O8")
			(pintype "passive")
			(uuid "9c11be72-faff-427e-a2d9-5b61560b28e0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "a6968588-824c-473e-9741-2273850b175d")
		(at 126.76 95.085)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U18"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "01ab7f18-3d20-4c90-b277-ae28215925d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "f4414a7b-a2be-4ab3-9a2a-c8e86eb2a620")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5970cf75-b3ac-4a9c-9d2e-f9ece343129d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "56f5d5f3-aedc-4d82-b6cc-15063b91189a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/5a6b9b15-1c3c-47de-9706-84f09a604714")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "72a7ea70-f0a0-48f9-8878-dc3c0ba3cc2f")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b36d6c8-ff9a-4c4d-926b-dc48459381bc")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9edd7c84-0130-41b4-aeaa-b4b7ad6ca04d")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a90e02df-4944-4bc5-9955-aa5a349a64b7")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bad0f11-3877-41a1-b0ce-aad00b2429bb")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b68dad4-879d-4c7d-8d82-c3ab21515db5")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "44591f7e-13fc-4ef1-a778-1cbb6fd8ea7e")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51992de6-7906-4512-b3a2-9fafdcb6895b")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8683d7f1-b684-40a7-9984-d62ea080b53e")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a7d8d9c-2f03-4179-83a3-9f077c75146c")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "222d2054-1b48-4eb0-b53c-52fd9196d7bc")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb4b473c-4777-4cd8-9060-1287f41e4010")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "d45ca267-ef59-4553-8145-7afe4cc46946")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 27 "Net-(C_I22-Pad1)")
			(pintype "passive")
			(uuid "25df0187-5067-41cd-8073-ae2207e6eb0b")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "5572d385-6cac-4797-89a5-1c1810acade6")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "7808121f-b6fa-42bc-81cc-a31e42ceab52")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "IN10")
			(pintype "passive")
			(uuid "4c663363-a972-4202-8111-c2f3132a1770")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a75f7f87-0c3d-403a-8551-d6161f510252")
		(at 138.33 77.175)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d71b01e5-a5d0-4bc2-8c15-f112f9e8650c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c4bc11da-7629-472c-926f-b35ecf4d1c38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d139a275-e0c0-45ac-9d42-7cf3f1e7f88b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5873efc5-a0df-475f-b1b1-46e10263064e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/e76da37b-bd37-47d7-b1b2-5bde3ec7c26b")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5240ac8c-0d92-4e58-a8d5-75ca483a89e5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "267b37b5-c623-4a19-9670-10715fbda718")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3bbdc256-9106-476a-a57b-942aeea7587a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "385a7795-4a04-4c80-8e5e-58a832671f4d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11dc8ecf-a414-4c2a-924a-e702ce3dc7bf")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58204c15-063f-4dd2-b1c6-5f07b08855d3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bec93b1-7a90-4048-a7de-9d4cc90e08bb")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cfa49fc-4ab1-42d0-a538-d6ca3c7961f4")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd22451d-2620-4f6d-8dea-fd02f72125d6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cd0ffa5-64ca-4289-895c-c09c138f706b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f06ec6e-89f2-40c8-85e2-2c977ccad4a2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "42332132-c7b3-4fb4-8c89-89c073bcfc13")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D_I2-K)")
			(pintype "passive")
			(uuid "32a4431d-e342-48a3-921b-aa2afca427db")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ab535238-c75c-4c7f-8842-b075dc7dc29a")
		(at 148.765 109.2)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D21"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f5b3ae20-0812-49ae-8067-99ebc7a83a9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "402e3e5e-3f11-4b82-8674-83c7d910762a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba29c222-f37e-4a53-8ff8-93696ebc1468")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "647b9e99-8824-48dc-9699-d7203dec600c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de74a9d0-e5c5-4c7b-b814-ab7c11f5354b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/42eb6ab9-bcf1-4e73-ad02-8bc341261aec")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5a40ade-8337-4dd7-86d6-35bfb33b7b1c")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53bd3f5c-fb07-47f7-8ab1-6d4693086757")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ddaa505d-a70c-4391-8164-f6042056a531")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "039c2383-6ea6-43a1-9575-61cca4e18245")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ed638e3-6eb6-4756-a0e4-f348246d2c49")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e1f0a29-9955-410b-b9d3-eea71bb72494")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e95232d-2189-4e01-993c-0ccae735e017")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ca9dc66-bf85-4576-9802-c98b8ef5e530")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a1885e7-15ee-421b-9b27-a8ae325dd4de")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c3238eb-e7a1-4a67-a906-43ff0d09da40")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a83765ee-cb21-45c2-96d8-832f8a863e8a")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa61c3dc-6817-48d8-9894-b03ac0769f5a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "38354760-32a8-46ae-8dd8-937e7269f826")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "8e517f84-c7d8-4960-b4e1-559da890d0bc")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 53 "Net-(D21-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "516d0e1f-bcd8-4e80-ad27-050548cd9d05")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ad16ec4e-caa1-4073-b3b7-c96c604506fe")
		(at 163.16 41.815)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I16"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "a7e5179d-c1e2-43bb-a46f-f6f8fe950452")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "06f56c52-a6c3-4cba-b79f-a00b60e4c6ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "70c3d3d5-a75d-4c8b-8fce-5dc2918d84de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0cd2fc3c-2dd2-47dc-aa5b-e3b2ae3ffb50")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/33260f71-772a-4a38-b761-f99140df86ae")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd783c54-37e7-4bb6-a3ab-65c04968dbac")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c64f8066-5c2f-4f69-9d8c-befa23e7f2f3")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "153a71f0-b119-45e8-9cba-da45f1329f71")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f61c161-864d-48b9-8087-635c900a4424")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39959da2-ab66-498f-b7a9-49e0f1a7d060")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cce774cd-7d66-451e-a1e0-f929f6001e6b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "93a71126-0059-48ee-bf5d-4eb277a2fe01")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7888e19-2f5a-44c4-b6dc-a96375a887e4")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d085d864-7103-43e5-9ab7-6fc39b09028a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "854eebb6-97df-4872-8eb3-35e467d80422")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ba4fd673-4576-44e1-b0a9-0a177dfff256")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 21 "Net-(C_I16-Pad1)")
			(pintype "passive")
			(uuid "57e74e34-f263-475e-8b86-d6a637c5a9b2")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "6df7e49b-e578-44c2-8738-610a4db45fb4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "ad6bf66e-03ad-4fe3-8a7b-cec6f7bfaaba")
		(at 126.76 121.645)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U22"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "d30289be-656d-4c21-b4df-1b9ab1abc00f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "b14cc151-1a01-4998-af66-1270e1602ec0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "96eaf8a2-bfd2-40cb-86d7-6024b664870b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "189e20e1-6c81-4e51-983d-00c6752fb79b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/78086611-a89a-40a8-986b-f4fcbe1b5f83")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "566bc454-07b0-484e-adbd-23d03375bfa3")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "481359b9-d90d-482a-9ff1-1cd0d6a73a77")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74b49575-30ab-4532-83f5-3904d933b7a6")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1209ad6f-3983-468a-8f80-170dcc7a7ebb")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdd274d4-2c1c-4685-850d-6d378826e423")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f469f90-9bff-453c-960b-33bcf5009f2b")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "3a5f140a-e242-4003-9eb2-0fc141aa5b42")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2a2c3a4-fb60-4130-bea6-6ef210970f16")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d01536ff-d047-4b65-8f81-eeda952151c8")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "813af220-1199-42d5-a2df-ec4164a709bb")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17a7139d-e100-4f4d-a8c3-ecdde7af7c5b")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9f69a58-d1ad-4bcc-bac7-ac896ebd049f")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "3f63f0c2-19a5-423c-b1ee-d7b4831daad5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 35 "Net-(C_I30-Pad1)")
			(pintype "passive")
			(uuid "7ab48158-2258-425d-89ab-67af1f4a1ab0")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "d097321e-15c3-4828-bf3b-ebbd42fd572e")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "ae01e60e-e83d-4553-9df3-97a4ffe1074d")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "IN14")
			(pintype "passive")
			(uuid "df2d69b9-7fec-43a8-9d19-370186319ad1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "aeb4554d-4f24-40bc-957d-8b485c41b95e")
		(at 157.33 71.275)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I37"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a43e9a0e-247d-4572-8a5c-18bd95b0164a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "7a850a4a-007d-4b4f-909e-36970336ac87")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b924692-45a0-42a0-a8f0-7df21bba0331")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f47aeeb-3178-4b95-be1a-a1c1e92d3300")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/7a353c61-65b4-4a58-bc0e-c5a800e6f4ff")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6c33b68-938f-473b-bb5d-26d89da15ff4")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "410fc099-7436-4d69-985b-91340a270baa")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc5850fb-cd80-4000-a16b-925fe84e1411")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33e420dd-a194-44b0-bc36-223ba380117c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8603acc7-49da-4865-b6d9-430b5f2f92a3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f786db1-89e4-409f-a655-88fb6359a5b9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ff853ab-c1d4-43d3-8217-0393d913662d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a0e969b-442b-48cb-8069-bb3235abe3f1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f651e69b-bd1c-42bc-aea3-89e7792ac7ab")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "625c7019-5944-47f6-bc64-7e27014ceec0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "133cc5a8-a082-4f51-9108-46f6fe5e3346")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "c2c122ba-2f54-48b7-8718-24e3ca7d2f6e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(D_I8-K)")
			(pintype "passive")
			(uuid "423f71d0-cfaf-48b9-aff5-0151d02b6788")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "afba0458-f7ae-4e4e-b1ca-64a8c795aa62")
		(at 236.54 140 180)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm, drill diameter 1.2mm, pad diameter 2mm, http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm drill 1.2mm pad 2mm")
		(property "Reference" "J3"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
			(uuid "2b26e34a-b034-48fb-a4b8-de98857a4ec2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NO_Relay Screw Terminal"
			(at 1.27 4.52 0)
			(layer "F.Fab")
			(uuid "5e0033f5-f21d-42b7-b49f-e560d9fe1914")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8525886d-8e31-4ea3-aca3-d9a9a6f0275d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd4bcb23-9e0c-4404-8ccc-4a73f59215bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/77642a50-2076-4588-b483-a3d853093c46")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.18 3.52)
			(end 0.3 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3067c742-e4eb-4649-860c-7388622ecf2e")
		)
		(fp_line
			(start 4.18 -3.22)
			(end 4.18 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c562b8f2-dca9-4952-ac03-2176575cd438")
		)
		(fp_line
			(start -0.3 3.52)
			(end -1.64 3.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9bc7d53-5b00-41b4-9c96-3903e0e98c16")
		)
		(fp_line
			(start -1.64 3.52)
			(end -1.64 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd286fec-d575-44b6-93ed-dd616838b922")
		)
		(fp_line
			(start -1.64 2.6)
			(end 4.18 2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2886ed8d-3562-467d-bbbf-87cade576fd2")
		)
		(fp_line
			(start -1.64 1.6)
			(end 4.18 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25a52d99-11ab-420a-8727-29d7adaa251c")
		)
		(fp_line
			(start -1.64 -1.5)
			(end 4.18 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ade1d709-7f1e-415a-8c01-1b699450f2c5")
		)
		(fp_line
			(start -1.64 -3.22)
			(end 4.18 -3.22)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a32381d-3732-46b6-a116-36b7e1f4d747")
		)
		(fp_poly
			(pts
				(xy 0 3.52) (xy 0.44 4.13) (xy -0.44 4.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "438403dc-3508-47fb-8d96-7e67fcb1abeb")
		)
		(fp_line
			(start 4.57 3.9)
			(end 4.57 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e94e9a7b-a4df-4ebc-8cac-e5b0542e6d9d")
		)
		(fp_line
			(start 4.57 -3.6)
			(end -2.02 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69f03adf-23bf-4a20-bf28-d67f25be226b")
		)
		(fp_line
			(start -2.02 3.9)
			(end 4.57 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1eaae1c7-f0d8-47f5-b5a5-e5a806cde5f8")
		)
		(fp_line
			(start -2.02 -3.6)
			(end -2.02 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c3caab2-2c9f-489c-8ee4-cba500259ccd")
		)
		(fp_line
			(start 4.06 3.4)
			(end -0.72 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "865c31ca-5af9-4a9f-af30-94e558044aa9")
		)
		(fp_line
			(start 4.06 -3.1)
			(end 4.06 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a22709d7-39fe-4061-9a78-d7e056dc2dbf")
		)
		(fp_line
			(start 3.298 -0.636)
			(end 1.904 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e97dee1-7d41-46a0-99b1-ddabfc84b7a7")
		)
		(fp_line
			(start 3.176 -0.758)
			(end 1.782 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c4ea42a-798c-447e-9103-3414c8e39d51")
		)
		(fp_line
			(start 0.758 -0.636)
			(end -0.636 0.758)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9267945c-c826-4034-b77f-3c2e483b3247")
		)
		(fp_line
			(start 0.636 -0.758)
			(end -0.758 0.636)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f27b53f4-c082-48d4-9127-e3acb24a64aa")
		)
		(fp_line
			(start -0.72 3.4)
			(end -1.52 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c9e18f2-5316-4b76-97ba-b1397a7c4f0d")
		)
		(fp_line
			(start -1.52 2.6)
			(end 4.06 2.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b1a27b3-d9cb-481e-adb9-5d93058501dd")
		)
		(fp_line
			(start -1.52 2.6)
			(end -1.52 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e74df79e-4ae4-42bd-8b8c-697279321243")
		)
		(fp_line
			(start -1.52 1.6)
			(end 4.06 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6fe4a122-00c1-4edb-b543-87117de272b0")
		)
		(fp_line
			(start -1.52 -1.5)
			(end 4.06 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fa8daca-2de8-4c6e-be5d-4efc8b98c0d3")
		)
		(fp_line
			(start -1.52 -3.1)
			(end 4.06 -3.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d071a68-17d5-451d-934a-19d5c1bb5f83")
		)
		(fp_circle
			(center 2.54 0)
			(end 3.54 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "aca1ffba-abb9-4b8a-8006-12eb38c8ff13")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "28228a0f-da0a-4d86-bca6-11ca51435282")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
			(uuid "646de988-6270-4d63-ba21-b2f1a004a7c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 106 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ce60797e-a22f-4471-88d3-536cd698991b")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ad988a97-e251-4008-9bfa-e378d8fa0482")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b2f6186c-e46c-4d3e-9d26-feac1e7570b8")
		(at 148.765 51.04)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "dce12a9b-07ba-41a6-a47b-c6bbc67ca2f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4db1cc6c-b63a-44a5-90ec-a18a034ba43f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7f19af5-531d-4a92-a04c-fece154d23fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "de437755-f00e-4e8e-901b-944d96aad204")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "986e7c44-c5a9-489d-b9de-f1fee8042af0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/0ade07f4-ca53-4cea-be6b-24083b4f2c74")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf7454a1-1317-489d-9b24-f038ab70a8c2")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ba78a43-0343-46cf-83d7-3f794f649baa")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22cd52c7-7e3f-4a0f-94fb-89e45aff25c7")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3dd4bea-71f0-4247-bcc1-0d4b9dfa3820")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cab0c262-b9df-4b45-9b44-4a5ee2c4a698")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8e7a6e0-1fb9-4e30-be2c-b6d920ec5889")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b14a761-109f-4542-956d-d09f056a2f94")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25b82e3a-4e0d-47d6-82ab-4259f9efbb2d")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e889aa36-fbf6-43e0-9edb-db39010b5260")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01880dca-0a3e-4dc0-8ee1-3e2a91d04ea8")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eee789bf-acab-48c5-812a-ec0b32f0f286")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a9861af-e280-4d5b-9d03-e4b6d31c3457")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bae3a335-d6a8-4a2a-b5cb-936abad2c720")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e960f386-56e6-40d8-ab10-0a21ee7c302d")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 44 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "c9d9c877-9236-4a49-836c-9fe63e8b8870")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b37bd961-6f1e-4317-92e7-ac7847a98bf3")
		(at 148.765 32.8)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "900a7849-99a7-4169-a20c-cba43663f9fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a4304b0d-bcd3-4e30-b01b-3516651bc891")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b37c15c0-ab5f-4b45-adc7-61e08e9858c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e8d7253-3f10-4545-abfd-9d2d5109db33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd1c5b50-eb9c-4ae1-9890-63722d29202a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/a7bbe722-ef33-4287-a437-35e9c453e020")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94a6f1cb-685f-4f4b-b82d-75210c7ab7ff")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c30e526d-1f59-4c35-be86-4a9f99fae4f3")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1eed2b06-f399-4de5-8ad2-385731a34632")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7135f615-d0da-4db1-8496-499b65e1b2b8")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bfd6b3df-f776-45b0-b2b0-9adbfbbfa58a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6755c89-bc43-4e21-a2ab-9f8f6e20cfd0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f03226ad-2207-4484-8ba0-bccd92b22668")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32b4f436-7691-4cd3-a714-219b5ef66607")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2279acb2-f17b-413d-a381-b0642bd313f9")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49f6704b-bb8b-4d59-a75e-bc4507e9d6fb")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17e61e9c-1749-49c5-8abe-20eb8f29b265")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13ee1dd3-658b-4410-91e1-6b1396271d30")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "585a78bc-476e-4191-9b68-c097fdd50749")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "941a271f-36c9-465d-96d3-f086311186e3")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 38 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "dbd74e87-d02c-404c-9054-9d0ebdf28be8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "b3bc403a-8623-4461-8683-81cc3c42d2b3")
		(at 126.76 53.245)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U7"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "55b59c60-3212-4402-9d18-f676a99a30ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "b15b26bf-3aae-4764-a60a-57e4d410d2c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "80f90508-49e4-4145-8589-5676ae5fd5e4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ae25489-116b-49fc-a779-b30c6625e632")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/4f0def02-9a52-496b-bc7e-746fa2dcc4b6")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8efcea1d-21be-4afb-aea0-706d15a43954")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50bd8f55-1043-483f-8aa6-bb421c166d2b")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c33a2459-8b3f-4442-853a-222177e6d0ae")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff2128fc-7511-4e35-8b33-82794cb43663")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12946775-c6b5-438c-8caa-3a3243dbed31")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "022a0ca8-fed2-4d0c-b3e8-f780adb7f125")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "38112deb-abe6-4c25-8084-79faf6752ada")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e94d77b4-32d6-4add-b7f7-45477f2e697e")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a1a5da8-ae5b-4667-a77c-31d61a549398")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a13e426-1bbf-4270-8734-408b2f95faec")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57ecb84e-7fea-4a56-ab1c-f40888e0cbf7")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4c7d647-8a76-4b00-85cb-513f4517697d")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "f3e79272-31d2-4477-88aa-80234773796e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 15 "Net-(C_I10-Pad1)")
			(pintype "passive")
			(uuid "f5019b63-c311-4632-9892-09765c4ea038")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "dbc92c63-b2d6-4471-b0d0-f3475ed827ff")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "61156622-2e8b-4acc-ad79-1cbe9c674859")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "IN5")
			(pintype "passive")
			(uuid "c28abbc0-2068-4b1d-8f84-5561df79cdaa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b448bab3-b22f-44b0-af73-8aa0e3e20fd2")
		(at 148.765 87.92)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5b6870f5-bfe4-4b21-855a-c13d957ee00e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "633cb8b3-0930-4b17-8afe-50a60da6cc2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2d10e9c-c90c-4e1e-8d49-aa0dfab958f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "18014f36-50f8-4569-97eb-f23df789983f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "27058aa5-021a-4bd0-be07-8a4c367ed206")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/b348de6b-bd55-4fc8-a80c-355cafe4dd5c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cda413aa-2cce-4972-b27a-c178b3a1b03a")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab7ef851-a6cc-4b49-85d3-3b85a3844454")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23d9d941-92e6-408f-a965-3183c618b9f3")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9367a437-c2d0-4a84-9b83-7876a3689fe6")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0891cee1-dc9a-4c4e-9f74-a5bb76c785b6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "817c9d79-0f8c-4548-8477-65632284d6a0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eff861f2-1d84-4d15-aacc-e1c917ffa320")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5597e07c-d923-43ee-ad78-0b75b8f73be2")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6560d8c-d8a0-4237-84b8-c0d1bbb905b2")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61973048-442e-4cc5-b2e9-16d1f2ae9105")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fced4f0b-8970-48da-928b-c5b05c2c026f")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a34b2ed2-df3d-4414-a00c-8105f9c2dc92")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5d90c843-2a2e-461c-8431-13896cb27121")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "765f43ec-d436-47c7-86e2-875d61d88e97")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 46 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "370fcd04-54c6-424b-8603-3bdfcc759511")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b51d48a0-fbae-4975-bb84-c18703f02324")
		(at 152.58 123.445)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I68"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2f463432-2ddb-4b31-80c7-568216e4fd30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "256481c6-0dc3-4a67-a43a-a10c140bd289")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "90d00273-8592-469b-8c43-532a020ec99d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "30ae11b8-f522-468f-add8-62f521c9d23e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/da889322-1a44-417a-8dae-16e99a0ffbdc")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0fcd2f90-f4e9-4d2d-b8d8-47a15393bfe2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6117fda-4f95-4bdd-ad45-8e31dabc702e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b269463c-234c-4a1b-a430-567a4cd1740d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca827226-26b0-4733-bf08-5eb38d0c2331")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "08c9df73-ae5e-4539-a068-99e2775e2e9c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f060d78b-b7b8-4d75-bdcb-c43bf91e577c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b8978bc-7ce1-4ca1-bb53-398a2318c5b0")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4f614d4-3b26-4e18-84b0-8f84d5eddd7d")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8e15ca1-26d4-4de3-8b7d-a1a4be000ba1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0af3155-3898-4965-a764-512981be9ead")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "94fce2bc-a3e2-4ece-a2c6-6472a906cda9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "15da5d39-8a5a-470c-b48c-82cfb659301b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(D_I16-K)")
			(pintype "passive")
			(uuid "e494509d-3b5a-4962-a0d3-62c2d7447e64")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "b5bf6b5a-f535-41ff-9726-ba1d15e8e0f6")
		(at -11.4625 85.01)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "a7a6b177-d7c6-4d41-9f37-3f7c9b66cc8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4u7"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4c2b02a9-7321-4ec9-9f7f-9bc28d1f062b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "18d1f0ab-148a-48c6-9d89-f398bd3f1029")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bea059c-272a-47a8-b2f8-1e7495c65651")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/8a1bc5ad-d1f5-4059-b9bd-6822f5d6bc45")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d14b3a53-6505-4670-9db4-261823c2027c")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96b7040c-4baa-4ed1-957b-a79c5b161288")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39169e3a-0892-4e52-b29b-c7a468093464")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9aae901b-2327-4c31-b74a-44bddc3288bf")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6021ffc7-6666-4435-8a52-45d209231b8f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c9e64b3-1144-48b5-a7a8-02bc944ead95")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d672da27-139e-49ac-b9cc-de7d7f92250c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7d3c79d-e605-4d6a-89fc-7a243304ecde")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1727092-5fb3-42a2-b6eb-c41e225f5292")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd0173da-2f1e-4543-9d3b-066405cda7f2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "62c04d66-e357-49f8-918e-a68727d1acba")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "5V")
			(pintype "passive")
			(uuid "269e9f2a-d468-4d0e-a370-7aa69ecdc517")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "c08dba3f-9c58-42e9-8bb2-4ceb4c88149c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "b6c8a38a-af4a-44f6-ad3c-6d1e3f0e0110")
		(at 126.76 39.965)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "69710034-80cd-498a-bcd2-618fec456ae1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "b88632ef-212b-4cc2-bc69-1694920983a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "22191b37-1cac-4352-b1de-8c7e514a26de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3df12431-e767-4404-a846-0db598eb43c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/41597e1f-d975-4ec1-be4a-9cdd4bee4d92")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "501a45d5-5871-463e-bd73-8a4004b6d559")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa2fc501-8cb0-4a06-a08d-c38eb1b438e6")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "037165a2-781d-499e-984e-5b23cf4550dd")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "181139ce-b484-4e8d-8a91-5d2ff428e3b6")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "307cbc0c-335b-4272-9992-371bfd7a9206")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2adda9ff-eb83-4a81-a544-b1fa9c6ade17")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c9b15ea3-fecf-498f-9dec-8f7ec5f25724")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bbcaca5-ab90-4da4-bd56-cfdeede6d886")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4991d1c9-9b19-4bd2-9f8d-4a1e1b45a0c0")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "595a7528-6c8e-4744-a677-a6a65114a882")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e118243b-83d5-4fd3-8ac8-0a8d74e9bde0")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a5b61b5-5326-4a43-8bcf-4a74d28cb1e9")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "841d5765-062a-4cb4-a86d-8035620e6144")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 11 "Net-(C_I6-Pad1)")
			(pintype "passive")
			(uuid "36ccec98-ef8c-4ba7-ae26-d9306e2c88c5")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "63a3d892-e78d-491a-8e85-4e12781c088e")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "afc2c9cc-cc75-4331-815a-5eded5130aa0")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "IN3")
			(pintype "passive")
			(uuid "89aea43a-afdf-4d9a-a2ce-6bba625571a8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b80e06cb-3dda-4868-ad4f-12b33108fe78")
		(at 148.765 54.08)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "30d0ee31-c53f-453d-a6cd-d8e1c430bbef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2509995f-8a82-40d4-afd6-811beebb04ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b258e99a-4453-4f89-8b3f-43c762e1ba42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "86689a62-1b7d-405e-a7e4-3540340f331b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d36fd227-d7b4-4e6a-966f-02e90312afcc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/394e935e-6362-4bf5-b305-f6f8ecfb3d2a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d698c160-31c4-44a8-8f1b-b722312d5229")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b18c4b1b-a8a8-4e51-9553-effcee22e40f")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b7ba310-6e15-4ef3-91dd-f5df78c1bd03")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "435a9e94-e1e8-408d-ac36-510e515b8429")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa58feb1-18a6-4a34-922b-e4a3d74871ef")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f3e271b-7ba0-473e-80e9-b1d78a2de142")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c109a2c9-e74e-44a2-90d8-8860a0a50f9d")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4139ee96-7438-4f85-91fa-6f19f8f62853")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f52117e5-23fe-4925-9734-d0cc6fc6192c")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "faf5d6b7-c3ec-4bf0-9e54-2256f757d8fe")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ecd7f55a-d72a-4947-a865-548f2294ab9a")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "092460c5-ce64-469d-a43a-721d11a413c8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "86011c83-11d7-4534-8591-4fe1bba7420c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "03a3f528-8858-4531-b283-9ac7a8b9fc84")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 45 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "b0d9f1e0-d059-4e6d-a3af-d792d16c157a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "b8ae8955-34e3-48d2-ad1b-7d91ca19f67f")
		(at -11.4625 103.07)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "bf4963ac-4fca-409e-9e90-41e300f719b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "cf5f9a3b-0f61-458f-8f17-900d32d64766")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f32c419c-00e7-4ff8-ad69-3b79552701f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b081a240-b11d-4242-85b7-58a2318f98bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/acc9c025-94f0-4018-8afa-3810e8659164")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01ff406e-5461-4d9d-82fb-27f2e6ed76c7")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0665e419-1c3c-4d41-8d51-48b5486fb27b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "353793cf-c349-42a2-a2bd-2ddba8b98ba7")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fb0e702-349b-40cd-b436-c91103f03c7b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffe9a09c-185d-4d5c-b3bb-59bfef8dd9d2")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7d0d423-d1c5-42c7-9ca4-7a1d762476b4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "daa3ad75-f723-4641-88b0-79a9ed1e0c4c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48c578f5-a554-407d-8fb0-c2250fdd2d21")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e85150d-aca7-4e79-a1fc-6c25d2cd14fa")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33abc858-5750-4bfd-8ce5-bf73b0d4dbd3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ed6fe622-089b-44f7-bc57-637004e090fe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "178573f8-4c96-45a1-8600-adc4fe5ecfe8")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "af278b8e-7b2d-4b70-b49e-54d4929a9fbc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "b8c26e22-67d5-47ca-bcf4-090a3bfc811b")
		(at 141.175 108.11)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I15"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "1f49ede3-6754-4b19-aa5d-4b61f8be58a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "1ad0bf46-dc22-4dac-91b6-c86319523683")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "30da6ee9-6158-4646-9872-ba4c2e4c34be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3587de9-922d-44dc-b5d9-cc4f3044cef8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/9f85c6a5-2700-4e8d-8da1-a756df7906af")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8eb9ebe9-38d6-4749-897d-f01355527cfb")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb05945e-8226-444d-b007-a6f68ff7f247")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7619d8db-80ec-4db4-84d6-ae090fb044bb")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f57d840-536b-4183-8496-84b56e2b4d01")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ffcf443-6a29-482a-a100-65f5482f7071")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4a07593-e155-4b64-99d6-6245b133f816")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40c0af33-b32f-4211-8383-a145ad1a50de")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fffb1697-9027-48ca-aac7-9b98007dbdbe")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6ffcab0-7818-4683-82dd-f9e2c6693d4d")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e48791bd-e2d1-4ffd-9af1-34c33b69d24e")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac41ca07-ab09-4184-8141-bb5f581bd916")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68257e11-1901-477d-a768-ab32e2114add")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74d0a2b9-ba04-4dff-bc86-4c68d7e5ca29")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44778dc4-8410-4c07-b8be-201609967846")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2b11602-c865-4470-8761-ed1697727135")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23dd9c6b-f5c9-43c3-9604-05a47c1e55e6")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b62eb94-416a-4f42-9888-35c93132c874")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2500217-3b45-4cb6-85a0-548a272bfd84")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "9963a9cc-73c9-43ce-bee8-b1fe3962cad8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 32 "Net-(D_I15-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "461142cd-eceb-4f53-9a3d-120c8ea71377")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "f6cf1213-5f71-41f5-98c7-84f9021a4f2a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "bbb01d4d-6162-465c-a21e-d7a1940945d7")
		(at 163.16 35.795)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I14"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "3e3e7670-ffa3-43c0-b44a-82efc1b99b01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "8d84e861-7243-403d-b3a2-297731be8745")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4f065a6-73d2-4d56-ac4c-a0f9d0e75051")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "408aa67b-5049-4ebd-8579-96cc2e858c36")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/bedb5457-6b1c-4ba2-aded-7bd14a99a128")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe88eaac-f6d2-48c0-ae84-92dd4e726325")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ae2d8a5-c528-40a6-bf67-3c3b59b67ee2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "022048ea-1f20-44a7-b600-9104bb21fa41")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6516ba44-86b7-4e64-8c8c-eecdf8313b15")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e980010b-fd03-421b-b123-dd30daf35cdb")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce9dd0fb-960e-44ff-84b0-c14e62de18fd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0af4511-4e8e-4b62-9137-359dc6f046d1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42bcc91a-cc9b-4f47-94ca-b8482cfed8ad")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dee77eba-e303-4133-a602-ed67bed25180")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bef88289-3939-49ea-8a0f-c76e742465e2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "65d08463-7300-4159-91aa-0030daa9d0fc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 19 "Net-(C_I14-Pad1)")
			(pintype "passive")
			(uuid "99023aa4-0c52-4eec-ba0c-f7c1040eb476")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "761fbf40-83dd-468c-9a41-113aae5b1940")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "bc298c97-7de1-483b-b721-4a72d7145d9d")
		(at 141.175 88.07)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I9"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "1440cafc-f460-4dde-8a9e-d03766f88e5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "66756ddf-771e-4fdd-9535-c7459059f16f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32289151-5dd8-4e4c-8829-06a71b23fd4d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "008d84af-e1cf-4735-8724-a30ac0dc2b40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/bda05778-044d-4f6a-9966-6a69850ca72e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03b1aabe-dae7-4d7f-b80e-af24a1841f80")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d66d528f-7721-41d0-aa1d-2b651aa1c6ab")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1add0b1-42bb-4627-8a49-d317516b31f3")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b8d3b23a-8193-4995-8719-885b3f45c655")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47826187-9d6b-45db-97f8-afc75872262e")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2f0e615-4b80-4007-b84e-9777daebe5a7")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ad92ba3-16bd-47de-a0a2-bf3d83ae5a37")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d001d812-6b0b-4db7-9666-326503fcf004")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc1f4c1e-6904-473b-be73-4ec8047f9c31")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34dd63ca-8d7a-40f3-9375-e508e5b3dfbf")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3091ddff-f151-4e92-832b-9f3c2a6be08d")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88bc0106-795d-4e6e-bec7-c1736da421c3")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cdcbb04-3c3e-4dc3-b153-d7663eed9a70")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e38ee186-73a0-420e-952c-17c06fd98d0c")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1adac604-d6b9-47ed-b88f-f436da3a2aef")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44c48dc1-0953-4587-b4e9-0f9d3dddf400")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9c39bea-6280-47ec-bb0c-b3cf0625a0bd")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2dbea33-8c87-4cf5-a9e8-77eaf87d55f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "57526263-6f80-402f-acc2-a009079dfc08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 22 "Net-(D_I9-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "71eaadb5-a361-460b-9d48-6df9ee25a87d")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "79909e5b-2bbf-46f5-8285-3ccac7ae671b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "bc88722e-dbdd-4b15-867c-ad5efe471116")
		(at 143.08 68.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c295d0b2-b6ce-44ce-a01b-f83ca1dabd63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "143febbb-cdfe-4b1b-a23b-10af0dbf6503")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4961213-cc83-4c05-802d-7183ae738fbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0100c23-6997-46b6-94af-be6d83a89dbd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/57e5751d-c6cd-4d88-a7ba-d5ff63e94b6b")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa878667-8e15-4540-bdd6-42bd0e3fcd1f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed04b4f7-bb3d-4fce-94ed-363ce46fac00")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7caf505-2ba7-4b16-842d-b5a0a79b4840")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b78a029b-a39f-420d-a5ed-24703030da12")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e5be125-0ebd-4e98-b236-f7f84abb5f24")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "024f68bb-8a1a-4e3e-96a9-f809e67cd459")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eee8c58a-bf3d-42ec-8b3f-386f503f695c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e10eef84-b8a7-417e-b4e7-94ea60030788")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f8e7026-0b70-473c-9e54-e4c9048d3543")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a1e9a03-bc2d-4764-8158-34d708a6d139")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "37501467-37c3-464f-85c1-73efcb810d94")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "0e4f8d8d-6f3b-4192-8c27-35ecd601a1ad")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(D_I3-K)")
			(pintype "passive")
			(uuid "a5d2b736-7fb1-459d-8c1c-b9867d9fbf96")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "bd986f6b-a175-49d4-940d-9de48687ff86")
		(at 147.83 74.225)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I22"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cbd744d2-4d5c-4f24-b8c6-721d48c913ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b481304e-a3ee-4095-8980-9a8d4568c8ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d463ed6-27f3-44be-bad8-cbe5f4eb84e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "945af92d-cd55-4de6-adca-c9e83d964132")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/f14ccc6c-0893-4398-aa76-18ac26dca3df")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c90b311-582b-4738-bbfc-df2f0d486c3b")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53e4e285-1e81-486b-8488-27178fd0411a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "612e276b-ffaa-4d26-a314-3dd3b4062c31")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2349bf06-0081-47fc-8fb4-a547ac3bd426")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d67d561d-e3ee-4514-96f5-96f1bfecb9b8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cb19da0-553b-4b68-be54-f644f54c0dc5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ad2f917-02da-40d6-b05e-537f0ac8711a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2eb4ee9c-d897-4cf8-bdfe-f250cbc0f128")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cbca39e-f655-4d7c-84e8-82e395dd39c4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d5252b5-f726-4cfc-b229-a8efac94f18b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "18ebb328-8a29-4bc7-9f5e-30a6e85c14e7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "128f1616-9274-4e8a-a753-c2a3a89ab6e4")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(D_I5-K)")
			(pintype "passive")
			(uuid "a6dc3487-8a3a-4313-a727-12337add75e7")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "bdb52baf-c862-4195-b0e8-fd37d250c632")
		(at 152.58 126.395)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I69"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d63b958d-1525-4988-a312-36089fbd11f4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a29d2dbe-bf9c-4699-9617-d993f48e8478")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "15b1fedf-8795-49e4-987f-49b5528b6622")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "55127f88-ac64-4a93-b384-b6dae72f5e1a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/12831bc2-3ddf-42a8-a8d1-73282f514ce0")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d504d15c-fe42-4b26-8130-c8f2ffe455bc")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14e5bf57-0fd5-448f-b355-87e0bca160cf")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9da269f-875f-47d5-9484-38210064013a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2190fdb-2a56-4d46-ac12-cf6c487db0cb")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eeb209b6-e20b-4816-8ce9-db2d02e0ff55")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4df7013-19d0-4d23-a91e-8cddfcb42f7a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4b59dd4-5dd0-42ba-85b2-60ef09789a0a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9acb2a04-63ca-42c6-abcb-623b8aa81a4f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86e2f439-f891-4e94-9e22-dda9a24b0142")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d954fb86-29ca-46b4-9510-d4402378b846")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4747b021-6258-439f-a2eb-de486c4d1d76")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "c462a778-77e9-48f7-a6e4-8ffddd642951")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(D_I16-K)")
			(pintype "passive")
			(uuid "b993edf0-2ec2-4e46-85d6-b99678945bcf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "c1117dc3-cf9a-42bd-bbd5-fbf25e8b5b8a")
		(at -30.7475 104.965)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D1"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "94e17828-42ed-4e32-8a7f-288b6b4b19b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D_Zener 5.5V"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "46f80ef8-6c85-4557-a01d-6db29c94bb9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a7d2772-15dd-4e91-a499-1d01e2d0685b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "052e30e1-3b0e-42b9-a598-f15ed39faf41")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/da397d7b-52b0-48ca-80c2-a669c9866517")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5b41a81-5df5-464c-9565-075a65ef1688")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0bec3295-e787-464b-85b5-21d729bbdb1c")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d164a7ad-7adc-45c3-b262-3cb9cfc2e7af")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5901b63-a5a3-48f8-b432-988a9d33ee53")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f84de1c0-91ef-44f6-90eb-e02f0005ad42")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be5874ea-f631-41e0-b031-c396ed0b1fd3")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63efeb1d-5245-44f8-a4dc-acf2f2928723")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "145ac456-224d-4c7e-bc5e-be59bbb759ab")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37f9dc80-fb41-489f-9e60-375f9e961fee")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60260a63-5731-464d-9442-8e606a3af93f")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "389ae8b7-b1ec-4c14-8d47-1b882b73e4c3")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2dd582ac-3b31-45ee-9b67-6e3dce06a422")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee9de0c2-830c-4fda-8e23-3f40553e9a01")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "376628f1-87c1-4ec6-945f-6ea83f265f95")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "400c2d5c-ea0c-4b05-b6c0-664606602520")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c20d501-3954-4136-973e-de05f9c6ef42")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "104a9246-22d0-46c5-b50e-a0a6ca18d432")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "950769df-85ad-442e-a892-bd8ded7ddd46")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "fd1a73cb-e772-4be0-92e0-ce79e852dbc5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 1 "5V")
			(pinfunction "K")
			(pintype "passive")
			(uuid "22058bd2-6787-46a4-8869-8a6b1e42e255")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "f53834e4-d746-4de6-ad9f-6a9ef4ba85c2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c2135a77-8c95-4c5f-9c9c-6964e698df76")
		(at 148.765 97.04)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "199ebb04-ffe3-451d-b66e-2d1dc7661b41")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0a2d22c3-e7b0-4684-aef6-98f11e5f2eaa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "06b544d9-a905-44ee-aa37-4e4d5a5c1922")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "217a31f4-999a-4df3-a677-f1ce3bd9dc61")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "273d71f0-e88b-4ee3-89e8-b62fe2457d89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/074bda3c-089b-46fa-81f4-d37cec81ae56")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c5f5adb-8b7d-4137-8b1b-cfc537eeebd1")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fdb3cc0-458a-4285-bb71-acac0d68eed9")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bed86bb-3a90-4149-9b99-c27df14bcbac")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "336f6342-66fb-4499-a95e-c5677aadb000")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ba2515c-4774-4255-a7c7-369883b5bc3c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efeb45ca-f797-40c4-8003-42650c69c602")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2df8c593-d3e1-4b92-9b5c-c6b21bbc6fbd")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3cdc041b-1936-4f57-b061-fc6ad30d2a1b")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17d13dd5-f6c2-45d4-8d43-fcbccb169e14")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7626dc61-722e-4923-9d2b-cb42572c3a9d")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe543b43-93e5-4ab0-829a-3929bfcb1127")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "651d08eb-aa68-4a9c-a66a-3119f39abb81")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "05ca993b-0320-4da6-be84-6af414273ec2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "068c5b3a-0032-4386-8ff8-3546f01fce25")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 49 "Net-(D17-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "bdc8d9dd-970b-4c09-9485-a916d81f13c4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
		(layer "F.Cu")
		(uuid "c46b6314-82fd-460c-b8ea-2d0ad44f9a9b")
		(at -5.7025 103.22)
		(descr "Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)")
		(tags "push horizontal SPST 1P1T")
		(property "Reference" "SW2"
			(at 0 -2.7 180)
			(layer "F.SilkS")
			(uuid "194f62f3-40a6-4bc1-8b7b-c07911e6fa46")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "3f812996-6ae1-41a5-aad0-3d8c162b58ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5bd4517-0a9a-48b0-88fe-1791814c6223")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ace873d-2a92-41f1-879a-ea562795fe78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/f51e380c-7b48-4e77-aecc-181d0c1b1290")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.4 -1.5)
			(end -2.4 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2fbd60b0-2c96-4bc4-8b25-6ad0b979dd54")
		)
		(fp_line
			(start -1.8 -1.5)
			(end -2.4 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f900d8f6-2603-421f-bfaa-031bd6c52d8c")
		)
		(fp_line
			(start -1 1.3)
			(end 1 1.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b70d1336-1024-49bf-a270-c3d2e5b739f4")
		)
		(fp_line
			(start 1.8 -1.5)
			(end 2.4 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a524b0a-7d4f-4ab5-b27c-5699e762c36b")
		)
		(fp_line
			(start 2.4 -1.5)
			(end 2.4 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb997fb4-35b2-4f3e-82a4-383220903b84")
		)
		(fp_line
			(start -1 0.3)
			(end -1 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "0515ecfa-f61a-4b71-bc98-dbd706e22a00")
		)
		(fp_line
			(start -1 1.5)
			(end -0.5 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "b689241a-be16-41ca-897a-58bd289fe6c5")
		)
		(fp_line
			(start -1 1.5)
			(end 1 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "77aa0ac2-6654-4ae6-bc92-81e4d2286dc2")
		)
		(fp_line
			(start -0.5 1.5)
			(end 0 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "411a5c06-4151-45b5-a8dc-eb13b6362c39")
		)
		(fp_line
			(start 0 1.5)
			(end 0.5 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "b319de09-a7ef-4807-9f0d-e9aafc656eca")
		)
		(fp_line
			(start 0.5 1.5)
			(end 1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "580c5e80-1c3d-4297-a500-bdb3ebf2e41a")
		)
		(fp_line
			(start 1 0.3)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "f2d32ea8-3bef-4f93-9ce5-923b375ed990")
		)
		(fp_line
			(start 1 1.5)
			(end 1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a7259b54-f352-43bb-af59-3d16624d0212")
		)
		(fp_line
			(start -2.83 -2.05)
			(end -2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18a971c7-75a7-44b3-a4fb-1d48ebb8182d")
		)
		(fp_line
			(start -2.83 -2.05)
			(end 2.83 -2.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a45a9a1d-cce2-4e6c-a299-daf4e4a88c8b")
		)
		(fp_line
			(start -2.83 2.3)
			(end 2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fcb2546-3c6f-4edb-9694-54cb0edbd270")
		)
		(fp_line
			(start 2.83 -2.05)
			(end 2.83 2.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8203951a-fbf6-4570-94a8-fe6c62e512d1")
		)
		(fp_line
			(start -2.25 -1.35)
			(end -2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f23519b-abcb-416f-9b39-e6f6380c6097")
		)
		(fp_line
			(start -2.25 -1.35)
			(end 2.25 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4af306c1-c938-4ce1-aa1b-937cd22d28c0")
		)
		(fp_line
			(start -2.25 1.21)
			(end 2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4039ca42-1b5d-4a14-b6d9-cd693033b34f")
		)
		(fp_line
			(start -1 2.04)
			(end -1 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "223098ac-cdec-4186-a716-da7c39a014de")
		)
		(fp_line
			(start -1 2.04)
			(end 1 2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "415b4f0f-4a41-467e-8207-80b40f0ada6e")
		)
		(fp_line
			(start 1 2.04)
			(end 1 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0a53852-4fbb-4024-ae91-61c700ab6ea1")
		)
		(fp_line
			(start 2.25 -1.35)
			(end 2.25 1.21)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae214364-5780-4261-bf7f-877cd96cb6b8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1a27e527-5385-4952-a14e-1c98f4cab4b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.125 0)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(uuid "947ee157-b23f-4de2-bd74-374f55f53d6d")
		)
		(pad "" np_thru_hole circle
			(at 2.125 0)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(uuid "841b2a1a-9132-42e6-9645-48535da7c053")
		)
		(pad "1" smd roundrect
			(at -1.225 -0.9)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "4b85711c-8d1c-4f6a-b65c-7d22a6e1de0e")
		)
		(pad "1" smd roundrect
			(at 1.225 -0.9)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "eb97a4e6-3736-422b-9e85-5e52231dc0d1")
		)
		(pad "2" smd roundrect
			(at 0 -0.9)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GPIO0")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8f09e654-e1fb-4ff5-9319-e51c9bd4ae5c")
		)
		(pad "MP" smd roundrect
			(at -1.85 1.05)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "bf6e835c-f4b8-4483-9fc4-48af357047de")
		)
		(pad "MP" smd roundrect
			(at 1.85 1.05)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "9d4e1747-6f1d-4a94-aa3f-07746284f24c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c5fe19fb-5fef-4d33-8427-b24f406dda70")
		(at 158.35 96.935)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I26"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "f38d38dc-d3b2-4430-b9ad-f44e59c85fca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "bd6ed958-5057-406e-8477-05492100c6d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1942c50c-f03a-48b7-a331-2b20e0c01877")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1d940a2-5187-4f6f-b677-7dcc334689ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/8c07b0ca-5c03-4d9d-b073-2b3312c86b12")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb180f44-9e78-41b7-a33f-e9730c362eb1")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "317fb264-f689-4dd9-a329-982333ec35f2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e0c68834-f310-446a-a70d-4c233086b862")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a19a6f35-1301-4c6c-a22d-8a1bd1a32b8f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38f1a195-272d-438c-9884-2d3e8710ed3c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9ef2aae-fc78-4054-b2b0-2b54ed7bd886")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39579366-c0c5-4628-9c1f-b3772c0208cd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bdfd6e3-8e7c-4dba-978a-9824e7519b81")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe23e9a0-995f-4f25-ba82-5a051cfd3088")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9b330ad-6cd3-4022-8860-1fa39a94526c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "13deb7a1-0601-45a3-941b-06d65a1cf5f3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "Net-(D_I14-K)")
			(pintype "passive")
			(uuid "937c0cc3-b0fe-4435-91ff-a1aa0c80ab11")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "be321837-9c1c-48b8-9f46-bd2212a9f369")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c765a5e0-d3c4-4f8c-bf05-f1986d9804cf")
		(at 157.33 135.245)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I80"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "05e1072d-73a3-43c7-b79a-f7b1c973c27b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "88e4bc26-133b-4b22-a54e-9daa94323068")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27463bba-9223-4be2-8728-57759bb6e87b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8aea8637-5bc1-4d7d-bb92-05e111b204a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/1805adf2-09fa-41f1-8271-a6815791b0bc")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22333637-1b45-4c53-835e-308c9959838e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae07db83-5327-4a8d-9929-7ef4b23fe04c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca011849-a546-4ba9-970b-d7018f02d56c")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22a21983-1e35-42a5-b0d3-2143196be5da")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e7ce56c-5124-43ce-8c46-cd38b910be1c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91992fa8-c040-410b-828e-a268e120893f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cd60e70-3681-401b-9896-f238714574f5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2616bde5-72be-44b5-804e-e98ed61094d5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60ba9cd7-04a3-4740-9826-36e83176c0bb")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e75b32a-c32b-4e52-b2e5-975a964de551")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a1c25eb8-59d8-461a-896c-2e2194dc4347")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 81 "IN16")
			(pintype "passive")
			(uuid "52bfcb2d-464f-45be-a28e-2f66e2e298a2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "efc9ecbd-8197-4168-80c3-a1be61e1e8e2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c869e213-e3c5-40ca-93a8-0575a1f699bf")
		(at 147.83 68.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I20"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2df84329-8e6b-4ea5-b73e-61b39b50c158")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a1caf197-577d-41f8-8c21-c4919bacee66")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd4b64e7-848b-4479-a02e-e7646c293e63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba6f284f-7e26-4810-b32c-0321c3b89dd7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3907058e-577f-4ff1-9266-14b0e0571454")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92838397-9939-4fab-8f49-5b3d3a43a601")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1401b06-76f0-4990-ab45-9889207a0441")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98e0221e-2d87-4e49-bde9-5dd97c57669b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1db6278c-1372-433c-9db8-12a00bc6ac87")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59544ca8-e54a-44ad-aaf6-58273c8ce2eb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "487cad40-3450-43a2-888e-a0977cdc28a0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8df098e1-db23-49ce-b586-3d4e97b33c7d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c7b2dd6-73c3-4e0b-9a5f-2a6d8981a3e6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f8bf09a-be8c-429e-9d55-b134887391e9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97b3db7e-9e93-442c-b892-ed38a513d4f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "377d93a8-74f8-4cc9-a698-2f809a9f68be")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 72 "IN4")
			(pintype "passive")
			(uuid "eb41700b-4a07-4d37-99f0-224db9357aa7")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "8548a258-cc40-4e01-a0aa-a83a68262a8a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "cbb2fe01-1b32-487e-b8b4-d09cb09b49ea")
		(at 8.3075 77.145)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "e5586f23-a944-45fb-90d1-8202ddfa9447")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MCP2562-E-SN"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "b68ab64d-b8ea-49d1-8e22-bdd29ee5abf3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "94f718b0-e4de-4f66-848c-f9cd00c1baa3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +125C, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0bc668ab-5c59-4d50-8c8d-34934026a68d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(path "/efe76b5c-b807-437b-becd-55b03d59ee87")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.06 -2.56)
			(end 2.06 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b4bc10f-3aac-47e3-97f6-fb1603302d75")
		)
		(fp_line
			(start -2.06 -2.465)
			(end -2.06 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff9d63e5-7969-4f18-af94-53bd43e4f418")
		)
		(fp_line
			(start -2.06 2.56)
			(end -2.06 2.465)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "925605c9-57ef-436a-98eb-5b5e5853fa0d")
		)
		(fp_line
			(start 2.06 -2.56)
			(end 2.06 -2.465)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f8ab992-7e6d-4911-86d9-5017d440707d")
		)
		(fp_line
			(start 2.06 2.465)
			(end 2.06 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14d82798-e6f9-4683-bb6e-5d7c70f041bc")
		)
		(fp_line
			(start 2.06 2.56)
			(end -2.06 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf93c5b4-de1e-4448-ab29-443c84888f04")
		)
		(fp_poly
			(pts
				(xy -2.6 -2.47) (xy -2.84 -2.8) (xy -2.36 -2.8)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "689b97bc-e2fb-40e1-9627-b5178084366f")
		)
		(fp_line
			(start -3.7 -2.46)
			(end -2.2 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbad27fb-9f47-4571-9f3d-e36b9f364eb8")
		)
		(fp_line
			(start -3.7 2.46)
			(end -3.7 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "888fd1d7-38f5-4efc-8613-47a385b7b182")
		)
		(fp_line
			(start -2.2 -2.7)
			(end 2.2 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff276b8c-474c-4ef9-92b3-c2a052cd9a30")
		)
		(fp_line
			(start -2.2 -2.46)
			(end -2.2 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bf897d4-00a3-4b3d-8746-b23e71571f7b")
		)
		(fp_line
			(start -2.2 2.46)
			(end -3.7 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1165e394-01d4-47bc-a0d1-ada8d7e7f138")
		)
		(fp_line
			(start -2.2 2.7)
			(end -2.2 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61485cb2-f2c8-45a6-8b40-af4a72ab5845")
		)
		(fp_line
			(start 2.2 -2.7)
			(end 2.2 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92833afb-6b0b-42ea-8016-c068fde1c0b1")
		)
		(fp_line
			(start 2.2 -2.46)
			(end 3.7 -2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7352b9bf-e47f-4aab-87f9-cd1f7eb3f211")
		)
		(fp_line
			(start 2.2 2.46)
			(end 2.2 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "753e9680-ac67-487b-82fc-1b165dff61be")
		)
		(fp_line
			(start 2.2 2.7)
			(end -2.2 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "054a05da-3110-4e0a-8dfd-56c293e7ff1f")
		)
		(fp_line
			(start 3.7 -2.46)
			(end 3.7 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71c1c265-594e-4720-8346-9a5c5771b675")
		)
		(fp_line
			(start 3.7 2.46)
			(end 2.2 2.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9d29ef6-e2f6-46cb-8afc-794e8faa7a4d")
		)
		(fp_poly
			(pts
				(xy -1.95 -1.475) (xy -1.95 2.45) (xy 1.95 2.45) (xy 1.95 -2.45) (xy -0.975 -2.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c5702130-0f1f-4cf4-82e8-0abb245d69d4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "82461eb2-341c-4c95-98a7-74e3868a7a9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "CAN Tx")
			(pinfunction "TXD")
			(pintype "input")
			(uuid "d56bf942-a882-4fec-ad43-6612d789926a")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "3ecd5469-8518-4585-bea2-bd1c6431b3a7")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "ba205a68-7e9d-4791-a2d4-8ea1b3c5b4d0")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "CAN Rx")
			(pinfunction "RXD")
			(pintype "output")
			(uuid "f48e412a-21fa-4b7c-8372-a7ff3f0826cc")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "3.3V")
			(pinfunction "Vio")
			(pintype "power_in")
			(uuid "d2845893-fa10-4408-8dc1-96f8fdfbdc45")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "CANH")
			(pinfunction "CANL")
			(pintype "bidirectional")
			(uuid "046b31d5-0753-4bfa-98d1-63d029b42e52")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "CANL")
			(pinfunction "CANH")
			(pintype "bidirectional")
			(uuid "5eaa092c-7751-4e7b-9266-4f36b3661686")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "STBY")
			(pintype "input")
			(uuid "1119f2d3-b229-43b8-889e-fe0a7ec7d90d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "cc0406c5-b886-45d0-8d8e-1e6a0ca98682")
		(at 143.08 123.445)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I52"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "0c479c99-1b7c-4990-ae99-324651c0502b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "843ae3f5-a800-458d-ab49-867b1f32f5b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "befb23fc-9c34-45a7-9a53-a046628a4433")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7cc740e4-3b83-44d6-bc77-e65ccfda6d97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/599f1570-57be-4b6a-abd4-903ed2e5dc96")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4004ca87-2084-48ce-bc2c-3a7ce7bada1e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4101b538-fbaf-4500-958b-219fce008078")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c09c4e2d-658c-45e3-b9e2-8c872cdc549b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23dbf016-3d62-4cbb-8de5-9547bcdba03e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8840c422-d14e-443d-a5b7-0ddca32e769c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "059c6bcd-36ec-4358-8386-4a812fc32684")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55b89882-5015-4729-a6fa-d20b6b30fe8d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08425499-c3a9-473a-bbc0-469ae2cd9117")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "766f6c6a-c4f3-4f8d-ac73-0321fad6157b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4703b6a4-b3f0-4126-9795-68810a866d4b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b2346e9a-bfca-466a-948c-dec0e748f75b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(D_I12-K)")
			(pintype "passive")
			(uuid "c28a0ba8-9127-4d50-a691-4ecdfab30823")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 49 "Net-(D17-A)")
			(pintype "passive")
			(uuid "94efc7a9-16d4-4b5a-b293-6388f2b24310")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "cebb0e37-a314-4756-bc6c-ad7599b6e1e9")
		(at 152.58 62.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I26"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "dd5b6571-8815-4566-95ff-cb1297a8c062")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a26594ee-d9db-4d7d-960f-a0a83556af71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aa6494e4-77f5-45e6-b9d9-8fa41d79cc5b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee10ac2e-ed67-4301-a25b-b80eab0156f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/3dfe342c-86dd-4eb3-80ab-b1ae61416c0a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27dc56d8-dbf1-45cc-8dcd-8942c6c8ba4f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02fb5ec3-0407-4e6b-818a-1676c630c932")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67090a8d-f24c-468a-be6d-35e6292983ae")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf5cd549-9a80-4738-bf2e-9315eda9c193")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcd8eafe-9c19-4bf2-a97a-c95c296e7ffb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e5c8173-f5c4-4af6-b04f-dd144516dc4e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19521ad1-61f7-4489-af01-81054fac2bf1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bb5458c-31f5-4fb6-b6d6-8f1af97d9008")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5976e3d-ba2e-477a-9497-6b3c29743a03")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc2b1001-e740-4dc2-8c57-06c93f0ef2ca")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5eb62f88-e8aa-4a72-a028-bee4ad4f3393")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "5914f399-9f07-4f25-96b8-f5b618a6346c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D_I6-K)")
			(pintype "passive")
			(uuid "3b5ee527-8107-4652-88a6-afc5ef694c8a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d1130ea6-0d8d-410e-8c3d-0ecbf0e006cd")
		(at 138.33 120.495)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I43"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "0b162f06-868f-447b-9bcd-3625b2d4d68d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "9ecd5163-f61c-4139-a63a-94e4375d73cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2aad13ec-8c1f-4a3a-b949-32370d4f2661")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bbdeebc-b3a8-41fc-a98a-ba4b3aca6d84")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/dbdd5dbf-7955-4edb-b805-e434907029e4")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2651be8-0e7f-4122-b442-4e59d2a3a5eb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f392f0ee-48f9-45c2-b547-c3d7fb1919af")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de9969e3-14e1-4621-b591-0e3459489990")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edf0d9ba-46ba-4a0e-bdc7-9d402366c143")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83c84e44-35ba-4ce3-8445-0c59e85978e5")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f9b6bc2-fad1-4262-888b-e9f186798e9c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35864a8e-9483-4920-a2cc-e5b6fcf5fa87")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88d614b0-90fc-4eb4-9f36-0c59f0d58508")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1376279b-69df-472e-806f-b0922e0cc985")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "336d71a4-9df0-4f98-845e-e1951525a8e3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "006fca65-ce08-4d2f-ba6e-9d54fb5b9afc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "a68f1356-15bb-416d-8f95-854be352d1fa")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(D_I10-K)")
			(pintype "passive")
			(uuid "511e5b19-45a4-4f54-bc63-e3f52b4eabe2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d1220383-2259-478a-9914-f4184e3076f2")
		(at 148.765 48)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "60ca765b-c080-402a-980c-710960e15667")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "70eee5e8-2208-4342-85fd-a5153bcd01e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1d11ad6-a005-49d7-a688-addf6d933c2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ffe0eff-2f0b-448b-9238-d4f859b6682a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d52f6e74-1adb-4273-a077-3d6a4684116b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/5efdbce0-5d00-4e60-91d9-06fb64380b70")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70915686-459e-4234-b79e-5103cf9b43d3")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62f4ebf0-1087-4267-8949-ef7ed57099cd")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5bdb5485-cbe3-4bd0-a2db-daa80289c6f8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df60aba0-ad05-4f70-9d45-f0b1dc9f3a57")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f24ab04-7b97-48cf-8cfd-1146233401e1")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c808a77f-f0df-424d-9dd3-a92fa4435ae1")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79f6e248-2fa0-4cd8-ae2c-99dd665c4168")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c24f383-f66c-4144-bc45-884e218b2cfc")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d86c1d8-fd95-4ccf-9e7d-a768a6fe5862")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09f1c939-c11a-4b16-bb6c-945ba529cd25")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "248e20d3-a87b-4ef3-819b-585deba885c7")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76b26bd3-2da5-42b6-9b3d-b12829a79b92")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fe1ea8ca-4f5b-4753-a53a-87c1018953b2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4bdf4afc-cddf-47e0-9b62-01a617acfe15")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 43 "Net-(D11-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "22f6a2fb-4332-405c-ab0e-447db2fbc1c8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d25723d3-5178-4569-aaf9-943bfc639673")
		(at 143.08 62.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b2cfc2e0-6bdc-4cd0-b20a-e860aeff9744")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "1db74981-1c92-4eb5-b3ad-cbfd482189c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2828e4c2-6d8a-4109-9b11-68a9672d83b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d714fee-b18a-448b-bc49-859e86687680")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/63e90c48-b5ee-416a-84bc-3c0a4d3ff7ca")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32b9e49d-e253-44c5-9747-095e1f3553bd")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f542a969-223f-49c5-bb0e-58033eaa9aa7")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "96af6cf5-f730-429f-a2bb-ddaeac15cc17")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ae14637-471a-48b5-87ac-829936ac2489")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7138b393-3cd7-433a-9037-e7df44e6da39")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d610f21-7628-4653-bd48-660be6ceea1d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5cea27b1-095e-47af-9e8a-28fb81769823")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "656bb92b-6443-4a3b-9263-44d6510723fa")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d6df244-c648-4bdf-ab0c-25de791b9bac")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4f31cdd-c1b5-4189-89e6-3bc3ea74dfe5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "50870d66-85e2-434f-9f24-bf864bbd671d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 93 "IN2")
			(pintype "passive")
			(uuid "b3d51c29-de62-4d9e-94ca-90f8b8c66c15")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "043c6886-4af7-4796-bd73-a99122700701")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d2aef483-cd79-4381-9243-499a7298bcdc")
		(at 147.83 62.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7beac1fe-f0c7-46a5-9ef1-643a3c9fc7de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "41954e5b-8342-47dc-af84-f83302f94cad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "13077ae3-7e2f-4f12-8d49-96e6efec6ed9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b834d2a-9dbf-4231-96e4-e04cdcd484fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/74defd07-c820-4ddb-9723-55e4ce862892")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3abd1575-c70f-4222-8234-75479ecfc0fa")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e64a8909-767d-4d63-b61b-828634e87539")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fd2339d-8003-4ac5-a4a0-bba0ab38bf08")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ab9bd6d-85ae-4bce-8565-ffc7837b0c2e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37272aa2-70c2-49fe-b3df-c514c86d9d16")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5358b466-76be-4a8a-abd5-a318ef18078c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0458655-14ef-4fa4-8434-3120f1859008")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f2881c3-3dd8-4d5d-b1c0-a3c177a15b88")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2330865c-7a9d-4e78-9cea-174ce0e6774b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34c19b3a-c0cb-4324-9225-5f7f1cc433be")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b64cd4d8-e6cf-4584-90bc-1bba775d2add")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D_I4-K)")
			(pintype "passive")
			(uuid "466a6107-a42b-4578-903f-b03f10328ed2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 41 "Net-(D5-A)")
			(pintype "passive")
			(uuid "b891f07c-dd49-46f2-89e5-d89591d12831")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d359c755-fb6e-4c2b-82d6-b6e36c57de00")
		(at 143.08 65.375)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5708af12-7ee4-405b-b967-4569a9b53fcc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ada9619d-59be-4caf-9b06-38f2a666d478")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a722c15d-312a-4f9c-ba09-aa8d4cdfecf3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ad7b934-9671-48d4-bc51-cd83c7c45c6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9da59258-a61c-4836-bae2-cd9b63079ff4")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0046a90-0dfd-4b79-8237-b84ffb72ee3e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02172847-869d-47bb-a35f-4954aecc6804")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7edc00a-7d55-4d59-8c84-84018b420e24")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a92f53c5-45be-485a-a382-9f22a926c729")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8564fa81-8263-4081-a730-4b922ba5da97")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53d3b0bf-e0fc-400a-83ef-ea9fb1d0718a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa0633bb-f030-425b-bb14-1366fe9f7acf")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f1030a1-1b22-4709-84f7-928a3fdb48d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dde64973-395e-440d-910e-9e4ee1128400")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68fd9bd1-c3d8-4f02-8ea8-f023bc959573")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "df7b29d7-dabe-43d8-a22e-6560fc7bc8ea")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "a0a5c440-ef87-4f63-942b-bb6b17cfbc3f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(D_I3-K)")
			(pintype "passive")
			(uuid "2f70f83f-dece-4482-a008-b6970155adb8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "d7c1c9e3-d8ab-4288-813e-ff2b0345aff3")
		(at 126.76 73.165)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U15"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "1d7e0365-9254-4a1d-a256-86398323e34c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "1efd63ac-87c4-4f77-96aa-b9f59d253ab8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eba4a43e-88d8-4e77-8f4f-e9d7d034110c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3663138e-9518-4eaa-8ab7-5b73d0c4c3e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/e90e92f8-fd2e-49ba-918d-6b4d7589e55a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efc73b4d-70b6-4673-bb13-2dc31c58d9c3")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03139672-d02a-4c65-a40c-4c9e883dfcf0")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfb38e06-3d6f-43da-bf89-e26b3632994a")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ed61e6e-2d8c-44a3-a444-acd8bd624dd7")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75151422-21b8-4d7b-92de-d9e278bca080")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf47afb2-bb73-4f61-82d8-38259f6f2aff")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8ce3b1c7-2554-4b7b-ad0c-665b213e5711")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59f4ae04-d861-4b88-9565-38d106964764")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b27b5f5-2551-4835-9bae-97fbfc2dfc2c")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83e49e69-b369-4396-9f7f-4ef0faa621dd")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d90d4cf2-24ea-4504-856c-66744326967f")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c76a7ec7-54a6-40b3-b446-f11d67fbd03a")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "93445a55-34cd-420a-8192-876d9efe21bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 19 "Net-(C_I14-Pad1)")
			(pintype "passive")
			(uuid "6e4fd689-5425-4a29-8873-3e32fce85d2d")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "7ff54b1b-77bf-4aaa-bd87-b45242fb8086")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "a1630967-837c-44e2-8e7b-11e48f3ba2a1")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "/PLC2 GPI/O7")
			(pintype "passive")
			(uuid "c1434dc7-e23f-4b20-87d5-29c1694df2ea")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "d875d7c0-3db9-475e-8a90-83dd2c75a7e0")
		(at 126.76 128.285)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U23"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "9af0ec23-d643-4ee0-950d-c9c9b3e3f0a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "fce258fb-4925-4b2a-b106-f78e4e7a6e20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27a9ed3a-543c-4fe1-b6c6-0f3c9d550bdb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c852e1be-2e6b-47af-bef5-d43035d483b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/db5f4b50-6373-4f3c-b88b-5405aa051265")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "079ba257-95f7-47a0-a38f-7046c2c17ba8")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6beaa004-7156-47b2-a538-d9175078ecea")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9edafc5b-36df-4ec2-806d-caea1b514ee8")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c38049bd-f1d6-420a-b61f-4d0e009cd829")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5e9d505-3804-49c5-8743-9c0fb33b5134")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a26719b7-7045-4527-843d-5a9429919998")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "614a7746-ecd2-4944-a5f3-ebcfc02b416d")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a81b8140-4606-4c73-b213-23784efb66ab")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10979843-b68f-4ecc-b136-a1e608f5358f")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9dfe971e-4bc4-453a-899c-4a532efc8fe5")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "156eb5ec-afec-48d4-8133-a1f509c373f6")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03b22bba-3133-43c2-baf9-9c925f582f06")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "5a3bebbf-36e4-402d-8b58-1798fbbebafb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 36 "Net-(C_I31-Pad1)")
			(pintype "passive")
			(uuid "4c87d497-84fe-420f-9bd2-cc673010ed39")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "b754b854-4a11-4a0c-8a13-b5e86cbd2538")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "850373a1-3c6c-4d47-aa25-fca88b739676")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "IN15")
			(pintype "passive")
			(uuid "8d56e4bc-7936-4757-8264-78f299e190bc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "dc320b34-c426-4b07-b83c-11c81a3f34c6")
		(at 141.175 56.33)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I8"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "db037d0c-4740-423e-86d3-fbb065e6f0be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "9eedc5ff-21aa-48bf-a361-322554becacf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5560d7fc-31aa-4781-a0c7-94ebbc2ca79a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1dd0f2e1-dbc6-4df2-b595-7ac8885e19a4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/db329cc8-cae1-4873-ad60-86d45e2f058a")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c8ad7a5-23a5-4dd5-a45a-faf9b3867c0f")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee20fd7b-5b5c-436a-8900-8b0dd78ef1e7")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1637e22f-891c-453d-8f71-b331f0e9203a")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0c2b9d4-dfb8-4be8-a984-9a6d4bd53d61")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "282a0831-5e40-479a-bef0-71da26afb559")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a8e2fcb-7e90-45be-a968-91d4e8cfb4b5")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "536e3321-1e7f-4bb0-a852-de4239b6f827")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bc609d8-d7ae-4cbe-8ee2-a4714a408b61")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ceb66428-da54-4803-a224-96cd00e34c86")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14007f31-2cac-4886-be0b-c93730f3cee8")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdd2aaec-43a1-4580-aec4-0354d0ab90c7")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6e63176-baee-4387-9d51-dfa185c3ab49")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09bd4df6-8335-479b-a6dd-952cead717fa")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "627ab353-76d8-4090-8154-328887268cd0")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6aad880-ffbb-48fd-96e6-e7e26788655e")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63683b70-c9f4-415c-a563-743625ddfbc8")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f7e4316-79e2-4c45-86d7-6d13b86e0c55")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "030575ec-b2ad-4237-9779-8ce74a537e14")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "d6d8ca08-78c1-426a-8a45-59b40cfcb570")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 20 "Net-(D_I8-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "c876ea37-3afc-4235-808b-bf3a00b2849d")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1f6a9c3d-380c-4620-b58e-50a4c3ed8417")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "dcdcf300-2d27-47e0-82f6-41d8a2fc94d3")
		(at 126.76 134.925)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U24"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "ccbab71e-306b-4498-96df-9d585073d37c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "163785e9-c703-4709-8dd9-6adb3e4429e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ece5d54f-9f30-45b0-9b18-cdd01bd2b0b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "32b2a79a-739c-4e40-9d4a-bb143804e58b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/e3135a60-1f1d-4dcc-8e9f-81958e68b977")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73af1a4d-aad5-4a5d-bc30-20977f263357")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a95b610-017b-4f03-8a34-ae6f6fa94ca7")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fed3084a-b9d3-4887-9ab8-f36f7a2223a1")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0663cadb-0445-4d12-8e46-bb40a5f59c25")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dcf18143-6365-4af2-94e4-5dfb383a5237")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a151149-ee72-425b-83cc-33dd1f66e16d")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1b4bc306-d24e-4a02-bbd3-0f62531084a4")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d8ff93d-ee04-41d2-88a6-5ddf621e7609")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f964b07-d6ab-4ea2-82bd-42e4902e60ec")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb703c2b-eacb-45e2-868e-df9cc04d519a")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad469d3b-f7b9-4312-a65b-859fa44b8716")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bd94dd2-6c57-48ed-bc39-426cab7b35b0")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "e43e6de9-ff44-4c80-ae6c-6955dddbbcf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 37 "Net-(C_I32-Pad1)")
			(pintype "passive")
			(uuid "9cc04325-6a7c-4056-95f5-527ba49ce3e9")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "28263044-9567-4e85-82a3-ab4a09c292f6")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "7471756b-534e-4b2c-9670-9ee7d02df424")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "IN16")
			(pintype "passive")
			(uuid "26388028-8e45-4172-9aef-e3aa4c18c5ee")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "dd430106-3cb9-4392-a812-6a487ce3b95d")
		(at 199.16 125.1 90)
		(property "Reference" "K4"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "5d2c615d-3e2c-4cfc-b401-decf66d1b9c0")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "170fe7cd-da1e-433f-b2e0-a014fa0337ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "aaa08a65-3d8a-49ac-878b-ec2fd824d90a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b0cfe9d2-aad9-4b90-b7af-5b60c7a5f2a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "74754c17-90cd-42a5-b59b-ec57c4d06227")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/fdc16f39-9e0f-4976-b47a-930f1e7532fc")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62e69c08-2720-468c-a0c5-76ae95e0714f")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3d23608-c409-40c9-b03d-a69c25468f57")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb938c47-638e-43fb-9f94-eec2cd9800b8")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c8bcb293-0b18-4fa4-9e6d-d4c26e556876")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b0db7298-b49c-4058-920b-2da5ce2748ef")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "060314f6-696c-4ceb-ad1f-3c3c1e72aa01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(J8-Pin_2)")
			(pintype "passive")
			(uuid "df55b715-b073-48d0-bf98-61de901df44d")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "unconnected-(K4-Pad12)")
			(pintype "passive+no_connect")
			(uuid "141b8864-bffe-4b70-a126-b759a5c5da21")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(J8-Pin_1)")
			(pintype "passive")
			(uuid "f1f9bd3f-3a3b-40c4-a7dc-5d9d2bbd253e")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16 90)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "03c68b66-f8fd-4624-8b32-8a25488a1f52")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PLC2 GPO/Relays/Relay3_A2")
			(pintype "passive")
			(uuid "38c11e63-400a-4a4d-9dd4-305d22de10b6")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "df55342a-106d-4009-9706-63c1920e8a38")
		(at 143.08 135.245)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I56"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "99dfc04e-365e-4964-a6ac-3b98cdb357da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a74ae90a-0d83-4ef9-b9db-3a5e88640967")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "150373ee-057c-452e-a2d0-483e74c99893")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f76e2c32-ca97-4657-a0a4-872d065a8343")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/d232b959-d1b2-4628-a908-ef7a7e139156")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "261ab3a4-b6c1-4a7f-b621-941af4447a05")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "026e011c-3f42-4bfb-9ec4-c3852d49f455")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edb2aea8-f652-49a4-842d-510b86cbdf04")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6af452e9-5aa5-48a5-9fb2-fd85a4736ac6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7cd33dae-d56c-4652-a3ad-7d83af56ed76")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e2c93de-b4db-4dcd-83c7-42c92dda895e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00733e6d-1d1b-40ed-9db9-1d8437815f57")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cd3c33a-4363-4f77-a961-5c0c1a56b496")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b61b1201-d8b5-4ffa-a97e-6cb170ea5b0a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b6ed4ba-dea0-4540-b5aa-f67c17c15187")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f680e157-9454-4daf-884e-9394bd6d6f55")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(D_I12-K)")
			(pintype "passive")
			(uuid "b4e82d6b-4ecc-4d0d-a652-d79ad8113d9b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(C_I24-Pad1)")
			(pintype "passive")
			(uuid "029f9c27-1086-4e84-865a-b789654ca7dd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "e1048091-63fd-4080-8e50-9af2f6589f6d")
		(at -0.7625 73.95)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
			(uuid "195f5da6-0d18-43f5-8485-df9288ff191e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Jumper_2_Open"
			(at 0 4.92 0)
			(layer "F.Fab")
			(uuid "ab06ddad-0e9f-43a1-88bd-3a0be641828e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7477310-741a-4262-943d-84557e368a04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "74c88fc5-d227-495d-8201-27b468fe9884")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(path "/05ee22a6-6cf3-4840-a122-8ce256ee2357")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.38 -1.38)
			(end 0 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3e91e7e-a3f8-4478-a0b0-3271e5a0c437")
		)
		(fp_line
			(start -1.38 0)
			(end -1.38 -1.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b67afaee-ff91-4b22-b533-0e7c97a6ab51")
		)
		(fp_line
			(start -1.38 1.27)
			(end -1.38 3.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc62b738-c1f8-43c8-9c95-72803a65a8e2")
		)
		(fp_line
			(start -1.38 1.27)
			(end 1.38 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "449fc29d-a74a-472f-b539-a5b61413424b")
		)
		(fp_line
			(start -1.38 3.92)
			(end 1.38 3.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cfccad2-84af-4979-828d-48f548c80838")
		)
		(fp_line
			(start 1.38 1.27)
			(end 1.38 3.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce5a7c46-db94-46d5-9627-6ad3f727357c")
		)
		(fp_line
			(start -1.77 -1.77)
			(end -1.77 4.32)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e7e5abe-afe8-4ef7-bb39-65f475b2e8fa")
		)
		(fp_line
			(start -1.77 4.32)
			(end 1.77 4.32)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "852844b5-af2a-4648-99a2-32f0664a1368")
		)
		(fp_line
			(start 1.77 -1.77)
			(end -1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a736834b-4aa6-4c83-84df-5121c72dda8a")
		)
		(fp_line
			(start 1.77 4.32)
			(end 1.77 -1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04c7ca5c-b0ae-4f42-ae39-be1aeefc3271")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a664b160-e539-4642-a6cd-5412e531fe82")
		)
		(fp_line
			(start -1.27 3.81)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09248d5a-5c3c-428d-adfd-3335891a119a")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9ebb46e-825f-4302-8e40-3efee5f52ccb")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "740ca435-ed6b-462a-9603-c462dbd169a4")
		)
		(fp_line
			(start 1.27 3.81)
			(end -1.27 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1d121e1-6389-464d-b85e-dbebf58df7a8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
			(uuid "f584d30c-cc04-47a6-9d89-b06d96d0f93a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "0a70d512-96d0-48eb-b131-9580989740f4")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "CANH")
			(pinfunction "B")
			(pintype "passive")
			(uuid "3a859837-e0ab-4eec-a962-becc6922fe78")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e1edab27-fae2-4242-95ec-d73ae236ee3f")
		(at 148.765 41.92)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "560ff227-22f5-4c0e-95f4-d8ad7cb29251")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "cc3bd8db-1a80-4a70-84f5-caae5001f46c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf90bccb-144b-4027-af14-d9e45860fd9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd584f64-c4dc-433c-a340-b66a146a1dfd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0251e32-9333-4783-bb98-46651d3fa995")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/1a0fa150-2a5e-4eca-9f0b-319d4aa39b79")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "297a3b96-f8e6-4c4c-a22a-e72354595a36")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1790e084-75d4-4596-b934-941ada809239")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60b709ff-7b15-4469-acea-6d00460b9c4e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "300c9901-99a5-4d14-98a7-593da31fe187")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5a4fa29-015f-4e51-94ad-ca9621ef709d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a39237e9-b71e-48aa-b56f-cdde6959111b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fe5b17a-3a5c-4179-b315-f04dd36e3cf5")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaa30ef9-76de-4a2c-9b06-fe2960de4e41")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e790a125-8664-4290-bbe3-c2a918312eb3")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b109b28a-4b83-4d2f-b582-6653586722da")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db267799-0ef3-4759-9808-583cb5a14401")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "597fc854-5aeb-462e-b7cd-9f74ad20c16b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "40d29582-f977-42ee-a1c0-01bf47c0fedd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "64d17ad7-64ff-4fc8-b9f3-22ce8f650889")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 41 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "7e5397cc-1152-4708-8707-5bb2f6ebafca")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e2f506d6-ed65-4d3a-af94-c76070528504")
		(at 153.54 87.905)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I17"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "a15cc415-08b4-4b5c-8d92-6f74770f1b48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "25197e2e-b95a-4f0f-9d07-7a327c5d46e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3302eeb-7cf4-430f-8131-3a542e30a0ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f06c7cc-199b-46ac-aa7c-90a4d3906a41")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/dde057d5-1115-4704-ae90-fbe688b65ebb")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e4edc2c3-9ea7-4f4b-badc-9e147c72196b")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3b666e9-55b9-47eb-88bf-f8c8ff0d61a4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3019f453-b404-42dd-bbc4-b6fa31b3270c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7802e6a0-2700-4d25-8bbf-d52af69328ff")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa4933d7-d23b-488e-8bf2-ef5c7b8beb6f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6a19371-21b2-4816-abe4-dfb0cf1fe70d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6d368c8-10c5-4d39-8635-02581e475567")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd8c0edc-21a4-4264-8987-cad10a0521b7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ec6c5af-0d6f-4d11-894e-9f1376032067")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aac6a8a4-df2e-4694-9bc4-8aa4b2cf3882")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "02b0e0c9-47ff-451d-aa06-482f9c775460")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 22 "Net-(D_I9-K)")
			(pintype "passive")
			(uuid "53a92c6b-df91-4b12-9961-f8c93a99a4dc")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "cb7c116c-0d34-4e87-ab1d-e21653d67bd7")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e31d40cb-de6a-4441-b15b-8b1a3a1f3fd1")
		(at 158.35 47.835)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I12"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "ed5ba04c-23af-46de-b21b-94b36b86ee14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "a307e4bd-ed27-496b-9a0d-5c63b01143ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97388afa-b6fe-45ac-8413-156f496beff3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b60d58eb-7864-42e7-a787-1997f5775b2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/70077f4a-70d0-4799-bb55-cd6711f99355")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d5f2bf1-b3d2-4900-9c8b-70d57c348167")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a090001e-65c9-402a-9ec9-c71793668648")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7563fed-d6e2-4b9e-b81a-9fc71779c325")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65ca924a-c4d1-4eb8-8654-d4f49b150a63")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15b7cea8-487d-4dd7-8282-e065741d9344")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07e23cc4-b04f-46ae-9ae7-fab6a9c4c2f3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a98b89dd-7dbe-445a-8aa5-1f7e410aae8c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d66e9c9b-2d93-4d93-9e87-2e96885ee4e1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33d1da5d-6b5a-4719-822d-354e0803a6b4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87e9f74a-8ed3-44ca-9aca-a2393cfec92e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "92ad55ad-fe5a-4dd1-9d19-f117fb98cd9f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 17 "Net-(C_I12-Pad1)")
			(pintype "passive")
			(uuid "94dd3533-a34d-43ad-9a98-760f4ab95595")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "206c954a-7723-46b7-9e0f-633af7f69cf4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "e445c6e2-08f8-4294-b2bd-a8c3abaa62f4")
		(at 74.7 73.405)
		(property "Reference" "K9"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "339b0e3b-7752-4dcb-82d0-562bc1f3a4fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e5fdd1dd-96e3-49af-ab81-4f63c3b13e5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e3a2165-655b-4045-86ea-b48163811844")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45cf2140-b486-48dd-b554-1bb2706bdeb9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54552c0c-0496-4128-8c95-e5dbb0530514")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/9f67a5df-bfd2-471b-a3bd-7c6804afc7fb")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7731b283-5aa8-4052-bad2-0df269b28984")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a37f50fb-fc61-4a60-8315-797a9fcf7e8c")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "620a1298-31d8-4b24-aec9-e20783147b12")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "51659584-a357-4b38-be85-31ddfc045def")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b0b2461d-c526-4b38-a9c8-c72f21b624d8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "1c0d8870-1442-46e2-b0da-f9aaf9bee3d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "Net-(J13-Pin_2)")
			(pintype "passive")
			(uuid "e4c67ef2-cec1-4d7c-9289-fbbfbb59c2ba")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "unconnected-(K9-Pad12)")
			(pintype "passive+no_connect")
			(uuid "9a01d521-61e3-4af6-839a-515d78738898")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(J13-Pin_1)")
			(pintype "passive")
			(uuid "7090a79d-3dfe-4ae4-8ff0-a46999332af4")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "14c4ef90-f914-4e30-a7c9-63649885c7fe")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/PLC2 GPO/Relays/Relay8_A2")
			(pintype "passive")
			(uuid "edfbfdac-5c38-4753-899e-6e9c7ea97eb3")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e61f8d4c-8237-47ba-b02e-54b132b4aeba")
		(at 157.33 65.375)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I35"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "4b010fa0-01f3-4665-9fe6-9f3f39f52601")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "dc3f91ff-f962-4897-a911-fbc8994a5bcf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "41abe24e-0b8f-4762-88bf-94c5516de65e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7918fbc-79c3-4cab-b2a9-2f709f3c4ce7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/d9e36152-482e-4d07-afc0-6c4e88c3e68e")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44935556-ff4b-44f6-b063-1b368e7a9b38")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8339e31f-8ceb-4174-a354-fa9e7dbc21ca")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ac517b2-e562-4691-9ee6-8af133f9ea08")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ea7e92b-708e-4512-a45e-0b7c67b5dbb1")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fec2033-ae83-45a0-921e-3ac5ee015548")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d79592a0-f386-4155-83b1-b7248cde25e4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a92a5299-c594-43b0-9a54-7a43ad2da883")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71b19a25-cd4f-4983-87b7-bafffe7818bb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6528c383-dbd0-4369-a8e0-2d4e6bee52e1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32140d4e-1d65-427e-a292-f28a6bc32edd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "68aeaa9e-901f-4f2b-b168-362270826cf8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 139 "/PLC2 GPI/O7")
			(pintype "passive")
			(uuid "095e7b50-94ec-4557-bcfd-1b1baf31b282")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "1c9a16d3-0014-46e4-bc93-5c8e1ed0779e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e748d859-2084-43f2-8e60-b05baf817544")
		(at 158.35 87.905)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I23"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "30c83daa-f271-427d-84bb-2d57bc9449b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "2f4c12f6-1529-4462-89e4-d738d0df778e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e422c81-d2d1-4fee-93c5-c8147c914009")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "801049cb-57ba-45c5-98a8-76e32c64ecbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/288adaae-76db-4880-97e3-6cadfda21653")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d61fb3d2-2eeb-48fd-87a5-ce47691062a0")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96ed7e19-e395-489a-b86b-06c4e6ee0be2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ad5da1b-ef6b-4c8e-b3eb-736c7bcb3f02")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c02ef27b-5fbb-469d-ad7a-af9ea4269931")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fde13d71-3f5a-4e42-8398-dcd405f783d3")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2925302f-51e8-4d2b-90d5-ee06e46028c4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e653891e-4896-4e0f-87fc-2a9b2b9cdaaf")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4921427-3723-4600-9e4f-58c3385545d3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c47b557-e452-4174-89a4-a9021c553b84")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "377e7e6d-2017-4904-a799-c94f486a5cf1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8c0abfa6-1f81-4d0e-b250-2d3984dd1463")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 28 "Net-(C_I23-Pad1)")
			(pintype "passive")
			(uuid "dcd7f535-606d-448e-8d46-2c907db8f9de")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "4dd53b53-ffbb-4551-9fb2-1fa6e318afa4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e89f19a6-0cd3-47f7-8627-ca9789d7a71b")
		(at 157.33 80.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I40"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "dc4abf5d-166f-4378-acf1-d5de23fbb4e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5c5676fd-eb89-4a49-ac36-22cb96a3e0da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a1b59c6-7827-4ad8-a24a-cda74f7328f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bd44758-3423-47e6-9c44-69a5ba45b616")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/766154ed-a8cf-4ca8-940d-a9714bb137d6")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6015fae7-4801-42f0-a231-999b36089683")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b41404f-10d2-44a0-840c-eab315a77296")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "201efc99-fcd9-43c2-b040-f5fdbd54bb95")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7575fcbc-d644-4d86-93cf-ab59b1eee166")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a310d808-bc1e-4bb7-8bf3-5fd2fcfc8e59")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f358b491-a8b9-4b76-b8e6-e4613745fed5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d426f7bd-ca3b-465a-baca-d7acabf56aa6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ec7ca73-b9de-4e4f-954e-1b5e125f7507")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f23ce4f-2050-48cf-a377-62832ed323ed")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7173232-fddb-4466-a465-b0ea92dcce0a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0675bdc5-b8bc-4592-b0af-73199a5b3f7f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 140 "/PLC2 GPI/O8")
			(pintype "passive")
			(uuid "b1da1234-1366-4b48-b4c2-b1132e0b12c4")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "1c3b0c06-a165-4b0e-afe6-6950697b6080")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "ea3fb6d4-89c8-4120-add9-7601c60a3b93")
		(at 141.175 36.29)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I2"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "5e08c5b0-060f-42aa-b91f-ba279a2bc415")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "e71e320c-efa6-4ee2-8193-15401ac8f8df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68920f2a-70b7-49c4-93cd-ffb60eeac5be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc158e40-55e3-483b-a7c8-90e5dc2ee18d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/9e777189-fa26-49a7-ae34-cf40cc7fc247")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7c015fa-e1f0-4801-9119-f0a104d8c11e")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "818fb8da-67e3-4337-a90f-6e4810d9daba")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea53ab9a-eb91-4cb8-95f2-54dff0b31ed4")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0e2dc15-7005-4a01-8220-53b8a89d043b")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90225871-5b1c-4bc9-b963-6d2dba7a9bc0")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c1c92ef-bc7f-47e3-aaa7-05ac822a7a94")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9331f5ca-78bd-4598-a3b5-c7c4a67465ad")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44c59ba4-a318-4b09-8f2a-f8b1951a7807")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f534ce84-8ec2-45a2-90fc-ac89691f2191")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc88fae7-5f9f-4e20-a95e-eb3ee8617edc")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1128c278-2bd3-46f1-ab72-8cba09f6eef5")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "626347c7-efc0-4661-bc17-df70e4a03918")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88be3588-c2fb-462e-a71d-a130c25e8023")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "364cdb6e-3f76-41ed-bca2-fb2e2c8f5f8d")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a01ee51-ad90-4e7f-b30d-64893cdb2369")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "799e4da2-c7ca-41d6-a262-e4a6dc23fd26")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2507202-d295-43d7-b296-722f5bba9217")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17828aa9-25a2-4603-a77b-2eb8c10c6b87")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "cfcefb07-8970-4ea3-9207-e94681d3411f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 8 "Net-(D_I2-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "c5eb7440-1498-4f19-9153-c80ec61a4c91")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "494df3c6-a571-4f15-9341-5c0c40882fc0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ea503557-796e-4bc5-a3da-d1f96f3b9b40")
		(at 163.16 90.915)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I30"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "63c82d7e-c745-4c53-85f4-2c3afa04debc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "3871c366-c100-499b-8986-2224c344afd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef084f19-9f5a-4a7f-9e17-419b4d587e5e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed0cba28-ecf2-4ce2-b94b-ac7cb150b8dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/f4695d1e-c00e-4906-8310-1c7cf0974b29")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42e0933c-8d78-4101-953b-660adbca2273")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6eb868c6-d047-4895-a595-994554c0b51c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16ac7ba5-294b-457b-8a6c-48fc4c776770")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04c32b2c-2381-4dfc-9fe7-fdda81040144")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35a26420-15f1-4ea6-97eb-23f5a1c24957")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89670364-59d7-4dc9-b705-d70277bd27a3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58853c49-5cbf-4e16-95ae-00b1e1e0dd60")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9275e9f9-8b5d-4bac-b293-e6f00887e219")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0778e6ee-68fb-4541-aef7-0b4877762071")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "546c8205-2774-4751-904f-623eab8f339e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d5490349-dbd0-4681-a1c5-69fa58ceae6c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "Net-(C_I30-Pad1)")
			(pintype "passive")
			(uuid "0a584236-6ae1-4926-8885-5f9da2f55bbd")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "c7491277-fdda-4540-ac1b-ff2adde4edcc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ea984e1e-d229-4969-8a02-e70f6dccef02")
		(at 157.33 123.445)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I76"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "89ff675a-d52b-4735-a52c-3661026650a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d7c03cbf-3015-48a1-b490-54d6e870d010")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d184f739-3685-4259-8d30-ffab904678a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b2c09eae-dc25-4e18-9530-6bb9ac347ccc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/b877cb5d-e9fe-4202-8052-4b0823f96d2e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc0ce15f-14d5-4389-b8e7-8de1044864c5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7ab55d1-0b16-4333-bb85-42a4ae151068")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fcf0e9c-5e4e-4720-b580-a75a713656a2")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fdaca2a5-5b41-474d-bec2-7a7fcaf6193c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "893f5396-3100-4a46-a9c5-ed9aba359ede")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13191362-a3e7-4a7a-bccf-b0634de50086")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "449fad6b-f001-449d-9099-2686c61791d6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d98bf3bc-251b-4fb9-b266-360259e47ff2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e0f4465-cefe-4bf0-a313-eab49fbe009a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4bdd367-b521-4f7c-b682-8f094dec95a1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ebe14fac-e1f6-4745-8ed5-26bb72bef577")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(D_I16-K)")
			(pintype "passive")
			(uuid "878ca868-87af-4092-9576-bd4c339d451f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Net-(C_I32-Pad1)")
			(pintype "passive")
			(uuid "cbe448a6-681b-4c54-860b-e6dbc6c5385c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "eb069fc8-005d-48d4-95c8-e733d5253d8c")
		(at 141.175 49.65)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I6"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "075f1b5a-1b6a-4b40-a219-317a321acaab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "700eb26a-4373-43d9-8cb3-b3d5b3f16bb5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "541d357d-7dff-4898-a726-379fe675f48a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54030e34-5790-4411-b8c8-07369179b8e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/981655fc-fdb0-427c-b5d3-0f7aa9b0fcfb")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4dffe8e-c7c4-4152-8d44-e88e0cb9a4e5")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1b5480d-ad9c-4f39-86d1-8e5f2d957ebe")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db90613c-dc63-4257-bb5d-a51e352682b5")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05376ea4-881c-413e-8fe3-a04b3721dbf2")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f41f686-7729-4551-8bf0-f04057de9ab6")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5530d5f0-7050-4a60-b022-4f2e63558a0f")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fa1e7cd-8e73-4413-bc35-d13a2f5fe483")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7e8ac9a-2159-4217-8c3a-e2ea11e02c7d")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb226fd8-64fe-409c-8acb-1681dab14bb3")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e613960-6e0c-4561-b1e2-557b7193fe8e")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7f6e2e9-8d80-404b-8361-c36a3a66063c")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c875d9b-fa22-4e36-8e58-facaa71fddaf")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89836701-0459-4062-8e38-c37281427f93")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5b2c5e8-2f03-44ab-9837-fc11408e4bb5")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab036fac-8553-4eb2-bdc1-9016c327186f")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a238cad9-5572-4529-a473-72f9e22f66c2")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70879dfc-1d30-4d6a-888e-11bfc78a65d4")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53f318dc-7c75-4e3f-b898-4bb173d0e80d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "52d0b2e4-7a4f-4880-bad9-514d845bcb50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 16 "Net-(D_I6-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "94dbd1c9-c9ba-4312-b550-36f8e1e3c9f1")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "60a262d4-b759-44bd-b92e-b7f4706f26b5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "eb4c664e-a77d-4dfb-ae38-d69e188f6974")
		(at 143.08 132.295)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I55"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a645c8c8-45d5-4c9e-846c-f4f52958d287")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "9c005409-00bc-4cde-a3a3-477199c6eb84")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c254398-07e6-43fb-bd7a-c3135be17d64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9540786-82ae-4ddd-aae4-f5ec468186bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/51caca55-4cf9-4d4e-b1e1-8713297f856c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cccada7-e635-45b5-a31a-dabd34e84cf2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce3f0624-aa39-43d0-940f-8ebbd4658a56")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcf78e8e-db83-4d3b-9624-db1d01365272")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef47867b-1365-49bc-8c38-b7c91b727faa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "360c16fb-87e4-46b3-a457-63967c91baec")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cb6483e-ca58-479b-9ff2-7a7ea631a9ff")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84da55d6-bc2f-4d2e-a63a-91d5c6d84f4d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53d6f318-3be9-4720-89b0-2319262c4749")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7f5332c-d5d6-4af5-976c-daa4e156f307")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ded38c1-5aa9-41ec-9c25-4889df543c75")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "14bcfca1-63e2-4a90-adc2-22ffe9057764")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(D_I11-K)")
			(pintype "passive")
			(uuid "547170a6-580c-4f88-bdeb-e14319a29bec")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 28 "Net-(C_I23-Pad1)")
			(pintype "passive")
			(uuid "296a72fa-8025-4fae-b083-f5ea02a1da7a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ebe3b5f3-fadb-4af4-9fb4-e4ad5c8df4f1")
		(at 147.83 114.595)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I57"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c8792a57-0f0b-4289-8f55-b4988adef5e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "aafe72c7-1f79-4cef-bfc4-81886c545e14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2100341-6264-464f-ac95-401d9718b58f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6f7ff2b-0bad-4960-9d13-96919072b3f1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/d4bc3b26-6660-47fe-9650-603c1dabedf5")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d44fe33f-4d9d-4588-9988-e665ad730710")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b21874c-24d7-443f-bf1c-bb6e1c5d341f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c29e526a-9824-454d-ad28-d56f2867a5bd")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2bfdf1b-549c-4880-9ea2-cf5629570c24")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f654f07-5f52-411b-b97a-3cbb09da979f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b137ed0-9332-4cdd-8b34-a00a61e22e81")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2df51062-a3cb-4be9-aa0c-b29ed7b0f5ec")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbf5983a-5b6b-4cee-ba18-1979b94ce097")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35779c59-36d6-4783-8299-f95b94d80b54")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25bfd3ea-d22d-4c63-8e9a-fa74f82cfee5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a773fb58-e304-4560-940b-f87ee9b16f97")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 89 "IN9")
			(pintype "passive")
			(uuid "9e51c03d-424c-40cf-9617-67c49a544b98")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "3.3V")
			(pintype "passive")
			(uuid "b8b64e86-5183-436c-85af-1f66dc78fb3b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ed0da2a4-cc10-4f9b-ad08-fa61de1b61ac")
		(at 152.58 117.545)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I66"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1b39134d-8cbe-4614-88cb-2002a5a6cb5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0b325485-211c-44d8-8524-6ef585aebd8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5edb5a5a-9f95-460d-a866-e83168ba571e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "99fed5e9-07bf-43cd-bd22-c74cafd15e8e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/481c4d7d-3bb1-4bba-91d1-67324bb5ae3e")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "740816dc-91be-462e-a4aa-1a91ebbe966a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b98083b-323d-4bf2-9d1e-38d8b2a886ce")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b893c3e-e729-4074-870c-ab793c8a78a9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f635453e-123a-446f-ae54-4c257ecfc58b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6083379-27f5-4e03-b71c-16ff72a986f6")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16e901bc-a999-4c82-9f63-143869e4f2a3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "deb0c87b-aced-4d8a-bf6b-956fc065f58a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca214578-93e0-4507-a60a-c74c7ffed67f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15150bf2-9423-4c81-9d03-b4d20057e082")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0547d81-ba9c-45ad-b5ad-f5c98197ca47")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "71bbece1-7599-4a00-9abc-f3801be67f83")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "1109210a-aba9-4b2b-a6d1-ea2fc1716f51")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(D_I15-K)")
			(pintype "passive")
			(uuid "5f1a6240-a0a1-4ae3-86ef-be032f0c7e8d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "edd091e0-fa94-41a5-ac3e-39bc64ec84d5")
		(at 143.08 80.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f4f5b284-a490-490c-8334-f160cb65bac4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "bf02083c-2738-49de-9ab7-80176851b775")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f889bec3-6f87-46a3-9623-aa5f119b6ca2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a096dcf2-3e60-416e-a00c-9e061123b9cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/04c392b7-842c-4cc7-82a6-dec9d0989d21")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9ca0608-981a-45f7-af36-044bbb703b70")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bc081ff-83d0-4ad8-bd81-c19d2fbaa9c7")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbc63024-2dd3-44c3-b699-285650a25ef4")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbc0f385-cedd-407b-9a2f-a506919bd96b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "959912ba-4be4-4233-857d-4e9961f61e1e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e75fef4-b19c-456b-9fa1-d3ce2b68b936")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "176d1773-2a76-4edd-8b23-12b5baee509f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e02effd3-e894-4f55-9a95-35cb7940c1ac")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b816343-13c7-4d6b-8499-178a02e55342")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b811aac6-883d-4959-98ed-48237c4300bb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a0c786e6-ef9f-435f-992b-ba881a876b9c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "a0a35d36-7464-43ed-92b3-97184b61c2dd")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D_I4-K)")
			(pintype "passive")
			(uuid "dd20feba-32b6-4885-8c44-b7f7401a0f03")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT_custom:Relay_AmericanZettler_AZ943-1CH"
		(layer "F.Cu")
		(uuid "eee26f96-bec1-4155-b47f-4de264c0543b")
		(at 215.66 125.1 90)
		(property "Reference" "K3"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "ba639ce7-90f8-4ec2-a3a8-3658038eeb4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Relay_SPDT"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "9b855cf8-c884-41a3-b1ed-cf8a53419f43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "758bd85a-6d51-4f39-86da-a95c885136ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Relay SPDT, monostable, EN50005"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "065a2002-95f7-4d08-8bb3-b3ff7ded4614")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field5" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6aa04e1a-0a80-4b67-ad98-ae78d7f1e8d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay?SPDT*")
		(path "/5b67250f-355a-4c65-ba9d-a43c60854ac8/2f0daa86-7bed-42d8-ac89-2ed7b6947d4f/f7eb5d09-992f-4bdd-800e-ca4d8e77b130")
		(sheetname "/PLC2 GPO/Relays/")
		(sheetfile "Relays.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -7.4)
			(end 3.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa56acd2-96eb-4b66-80e8-02b443d1250d")
		)
		(fp_line
			(start 9.2 -3.5)
			(end 9.2 3.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba6a1a11-05af-4f8f-b5d5-d8433305142e")
		)
		(fp_line
			(start -3.5 7.4)
			(end 3.5 7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5a8cc07-a78a-418a-9051-24c94a290140")
		)
		(fp_rect
			(start -9.75 -7.9)
			(end 9.75 7.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "5424369b-66d7-4d7e-8f4d-3f7399daa002")
		)
		(fp_rect
			(start -9.5 -7.65)
			(end 9.5 7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "bfa4801d-ff85-43fd-9a8f-23243216a483")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "75f50729-b697-4c48-ae72-f94788dde122")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "11" thru_hole circle
			(at -8.1 -0.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(J6-Pin_2)")
			(pintype "passive")
			(uuid "84cc3834-4be0-4479-b530-bbec9cf5e671")
		)
		(pad "12" thru_hole circle
			(at -6.1 -6.16 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "unconnected-(K3-Pad12)")
			(pintype "passive+no_connect")
			(uuid "8d89998b-a8b0-4844-be2d-37ed78d8d357")
		)
		(pad "14" thru_hole circle
			(at -6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(J6-Pin_1)")
			(pintype "passive")
			(uuid "032c6919-d112-497f-9c8c-a2319e1cb9c7")
		)
		(pad "A1" thru_hole rect
			(at 6.1 -6.16 90)
			(size 2.7 2.4)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "469c6e8f-655d-4530-9d1f-b5475e4c2731")
		)
		(pad "A2" thru_hole circle
			(at 6.1 5.84 90)
			(size 2.7 2.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/PLC2 GPO/Relays/Relay2_A2")
			(pintype "passive")
			(uuid "4f24aa7d-e1b0-4b9a-ba9d-20f17c26b544")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f23f506d-ad1e-4b4f-a4f2-489845975712")
		(at 147.83 71.275)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I21"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "3907a850-bb4c-4371-8e8d-4a5919fa9d2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "adc34fc4-5f2d-44ce-b668-22eaab596c4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "77fd8983-e138-489e-ad8e-ea463adf11b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "14ced0b7-c22f-452d-b3b1-65a0cf955786")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/17d32de2-6bee-4861-ac0f-269a6d83e026")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "891112ea-8b6e-48d9-88e2-f39fdc47e73d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad215a46-9deb-4c8a-b664-2134bb0ccf12")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a69030ba-b986-483e-b81d-a577fae6b33c")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94231c04-abe1-4e7e-9000-94648f37cef7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "820c6554-ef6e-45ec-ab38-158052cd0c4d")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e404f95c-0612-4255-8983-7515cd268e42")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0750621d-2742-4b42-8579-061e7b79b364")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c2b984f-0d80-4bcf-9240-a4da130af753")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "230f6b0e-8e62-410f-8ed6-2c4837194cc4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff337569-dd70-46af-9aed-0ba60aefcd38")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8754fa70-61fa-4ca3-8b49-096a32635c38")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "61cd2c71-6994-4ec0-b65c-6c476a924f05")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(D_I5-K)")
			(pintype "passive")
			(uuid "09d78acc-2acf-4b13-9557-b1dc3b7582da")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f3991591-6f40-4261-8ac5-682dc7115f57")
		(at 148.765 35.84)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "392acc2e-d134-4d0d-8b85-4956d80aa19e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "03698296-46b1-440a-b716-0a0d66eb0eed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "278f69fc-f7c4-4f06-8b17-acbd1a8f9914")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffca7ac4-6ff4-438c-8107-e2db0c80e106")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67c43f00-f462-4576-a01d-262d2f73f247")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/88248441-019d-4696-8372-a67a1fafc52f")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f1bff21-c3c2-4e54-ae9c-7304001582dd")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2845908c-c56c-446d-ba25-e20023066f48")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "816d1fc3-b707-4403-94a6-e4f1c443966b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bc79ba6-daad-47ac-b8b7-8ef23eff9a41")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b385215f-76e2-4741-83b9-6ed6a5fda0b3")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92046e04-7e98-4dcd-ad33-893f8e69afc8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d419e43-43a7-4516-ad20-aa9b2d80dc9d")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d75b0ec0-3d0a-440a-8005-ecf11ad821f3")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fb63758-ef92-4854-8685-55c81284bdce")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4a131c4-958e-499c-b5e0-804a453e7142")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e2bb271-53b6-48f7-9873-886ebeab8c6f")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8f6a42b-9987-465b-8001-c9c9e4e7e924")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "64222c23-4abb-4704-a530-79aca7afc6fa")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "0085aeff-c150-4529-bb6c-25bab257c689")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 39 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "38797534-08fd-4ce8-86b6-fe37e2a6aa31")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_MiniMELF_Handsoldering"
		(layer "F.Cu")
		(uuid "f44fe8b7-7166-4a19-b122-194d85744473")
		(at 141.175 52.99)
		(descr "Diode Mini-MELF (SOD-80) Handsoldering")
		(tags "Diode Mini-MELF (SOD-80) Handsoldering")
		(property "Reference" "D_I7"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "5f05c7bf-9462-43a2-b424-fe1f66f52c58")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1V Z"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "a6f5ed2c-ae37-44f0-b083-b96c5e5ba513")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0f38e40-2a30-47dc-bfbe-9447e6eb1143")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d75e8021-f9f0-47f7-8353-b32918344fd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/dcda6f06-bb91-43ea-aedb-d0a85695f642")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.66 -1.11)
			(end -4.66 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71c5d075-6bcb-432f-a1ea-98d48b9ca3c0")
		)
		(fp_line
			(start -4.66 1.11)
			(end 2.75 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d174e770-e80b-4005-914f-79b611bcc5e7")
		)
		(fp_line
			(start 2.75 -1.11)
			(end -4.66 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "653bf6e3-979d-43b1-8039-51b19e54d677")
		)
		(fp_line
			(start -4.65 -1.1)
			(end 4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c0fe963-1f42-4aa0-94f0-70ff84931635")
		)
		(fp_line
			(start -4.65 1.1)
			(end -4.65 -1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34a8be71-4e6a-4111-a35a-ea10ea51d645")
		)
		(fp_line
			(start 4.65 -1.1)
			(end 4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9397f7d-d427-44b5-abbf-376831139680")
		)
		(fp_line
			(start 4.65 1.1)
			(end -4.65 1.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f26fa670-dcc5-4bf0-9b1e-41eb2830bbd1")
		)
		(fp_line
			(start -1.65 -0.8)
			(end 1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54840080-189e-4091-86bc-ddc518cc06c6")
		)
		(fp_line
			(start -1.65 0.8)
			(end -1.65 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff9fd853-328f-4a39-9ca0-6d7ddf43db35")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20d48c13-4021-4960-80d9-b99bcc404528")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b7dfa41-6668-4696-9340-eee4adbbbf14")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffe472d6-4ad2-464a-be35-236b35e579ce")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d72a7050-2c04-4e38-bd33-e7884d49eab8")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f656c28-daa9-42a3-9df8-c9bae8df9a57")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9939a2b2-1764-43bb-a24f-a4649923f188")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1eb1f02-2352-4a61-a6e8-0314ab13a8d9")
		)
		(fp_line
			(start 1.65 -0.8)
			(end 1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d069b627-2f12-475f-8ec6-60781273dcac")
		)
		(fp_line
			(start 1.65 0.8)
			(end -1.65 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4d15744-5f05-4734-b599-c47265756e48")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "c3d3bb9b-e0b3-480e-aa91-bf3168c6364f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 18 "Net-(D_I7-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e12a2958-1472-47e3-b01d-e44116d08adb")
		)
		(pad "2" smd roundrect
			(at 2.75 0)
			(size 3.3 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1470588235)
			(net 5 "24V GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "3abf4e7b-471b-4f06-926d-3034af782c86")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(uuid "f74b394f-f355-46d7-8e16-98b07270d1c7")
		(at 126.76 46.605)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "bdb30030-4ff7-4f6e-b3f2-9a50dfbe5eac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PC817"
			(at 3.81 4.87 0)
			(layer "F.Fab")
			(uuid "1141dc3c-1122-4d9b-bbf9-52733a988dbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "af71cbdc-1196-4592-8c85-508e07ea27fd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bcf1ee6f-6a80-40d7-89d9-d11051377897")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/cfaad72d-c380-4263-ad8e-47d5dc899252")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e269693-fd39-4807-9a9a-9682da18669c")
		)
		(fp_line
			(start 1.16 3.87)
			(end 6.46 3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3c87740-3dff-4ab2-bf5d-2a24f05dacaf")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e42eaff6-d87a-4869-a622-2be55cda144d")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9f5cdbb-93bc-4d57-b11a-832029ad1e8b")
		)
		(fp_line
			(start 6.46 3.87)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5dbf14d2-8e49-4323-b986-b2df857c2737")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5770c071-f2b2-41e1-af1e-20542110e796")
		)
		(fp_rect
			(start -1.06 -1.52)
			(end 8.67 4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "d0d0da5e-aa58-48f9-8b02-237f35804eb5")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73dea864-062e-4dad-a1b7-0fef19a68cc3")
		)
		(fp_line
			(start 0.635 3.81)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef367da4-cecd-4950-bf55-b2ec19014eee")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f49df7e-f0a9-441a-88ff-d92fc8c1ebcc")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3e4ed42-59be-47e4-9b55-635629c8b4dd")
		)
		(fp_line
			(start 6.985 3.81)
			(end 0.635 3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b08e7079-3a3f-44f9-a519-8868454328eb")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 0)
			(layer "F.Fab")
			(uuid "d6fc4d98-16a4-4385-8408-0352745ec2f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 13 "Net-(C_I8-Pad1)")
			(pintype "passive")
			(uuid "a3708d41-9589-4c9a-a2ae-3c7f99a041c2")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "1d4cf93e-3278-4fec-8e33-ac313c045227")
		)
		(pad "3" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(uuid "9304d663-89bf-4cd9-8767-6831ef30c325")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "IN4")
			(pintype "passive")
			(uuid "cf34c0d4-90aa-43cc-aedb-78f2ed52b567")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f8aa24bd-8417-4fc9-918d-af7b2e9a7e24")
		(at 138.33 117.545)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I42"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "38fc5699-aec0-49d7-b933-f6a0249d7699")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "16k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5de93961-6759-4da3-8ecc-15d574032835")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "df49e5df-0a71-4b67-8ff9-4749871a2112")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3a2618b-bfc7-4159-8f69-957c746e6ddf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/dc44654b-909c-468c-9b62-e2ee7c41bd70")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7b063c4-61f7-4c0b-9969-eea7b5f5cc95")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42ece729-92de-4e47-a11c-559978d7cd38")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7988d8ad-5348-4625-a38b-f23ba4c32f7e")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fdc194f8-b707-4fe8-ad06-a8b023c201d5")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fd4cff5-1e3b-47ea-aa4c-7b705fb788c2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ca0a8d1-5791-43e1-ae2a-e8dec4eec984")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee0d1b58-5b3a-4341-bc93-123227baa038")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24f681dd-25a8-48c3-88bb-d5b68635077a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c4b25f4-bc87-4d36-b0f5-34ee833531f3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d62c6be-c0b6-4f1d-8b6e-a0cc3d6a29ca")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2d190034-44a1-49ad-bf1a-eca473b78a43")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "24 IN")
			(pintype "passive")
			(uuid "b33e31d9-0285-483d-bbad-7db729f002f8")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(D_I9-K)")
			(pintype "passive")
			(uuid "0bfeefaa-2eed-4333-82fe-c4ecbf727e03")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "fb2664ec-06b8-48a6-a0ba-e72b1720ea48")
		(at 147.83 80.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R_I24"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "92e118f3-b93c-4eab-9d62-3c5c064ced06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "749f6138-4ac4-4eee-a92e-32da1ef6d245")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f13ad1a0-9676-4bba-8a6e-5f61f92c8d6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9cd15a4a-2c19-404a-ba50-6106b8698cbd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/114a0c5b-b79e-4a9a-ba31-888f2d71abad/97aae1ac-6eb3-48b7-b400-81d3d7548039")
		(sheetname "/PLC2 GPI/")
		(sheetfile "PLC2 GPI.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e16115ba-0ca8-4c33-beff-68b5ff94349d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0204abc1-64d0-41a1-ba6c-9d96b244d719")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "269ba1c6-6adf-4b08-b2f8-c806fdd78286")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c4596f0-191c-4ee0-a427-d9156ec5f10c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2e30077-5604-4d0b-bc29-404033d3b59a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d1b50a5-7535-4026-ac69-be759c83f1b8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c778fe5-4510-402f-bdca-334e0f30d21b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb3a343e-6384-4e8a-a3db-b0419905d012")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8f16000-151c-411c-aa90-dc5610f8cce0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbffdf83-9dad-402b-b7e5-dfa55bd4b5aa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "12efc271-244b-4326-9c86-00b4db9da415")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(D_I5-K)")
			(pintype "passive")
			(uuid "2488dec4-725b-4feb-99d2-06273e919e6b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 15 "Net-(C_I10-Pad1)")
			(pintype "passive")
			(uuid "ea92594a-84a7-479c-9283-6cd9be5c5cd0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ESP32-S3-WROOM-1U-N16R8:ESP32S3WROOM1UN16R8"
		(layer "F.Cu")
		(uuid "fe1ea130-963e-43bb-a90e-4d0c96eca236")
		(at 189.75 78.91)
		(descr "ESP32-S3-WROOM-1U-N16R8")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at 0 0.25 0)
			(layer "F.SilkS")
			(uuid "351d3980-b2e6-41d5-bf9e-da5cd6cf45db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "ESP32-S3-WROOM-1U-N16R8"
			(at 0 0.25 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7c3a6e52-47ee-46e9-9b4c-fc13c60eb6a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-1_wroom-1u_datasheet_en.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e9701ce-7ab8-48df-8a45-36ffc88547db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "WiFi Modules - 802.11 [Engineering Samples] SMD Module, ESP32-S3R8, 8 MB Octal PSRAM Die, 16 MB Quad SPI Flash, IPEX Antenna Connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6dad9c5-2a11-433d-8c92-b558235cf7ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "3.35"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ade0983e-e2d0-4027-8f70-e230f96bf918")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "356-ESP32S3WM1UN16R8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3d89470-3293-4d95-8e4c-0fb094cb1285")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Espressif-Systems/ESP32-S3-WROOM-1U-N16R8?qs=Li%252BoUPsLEns6V0Pr5KRJtw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5bdcd7f-ffcf-4388-bff1-e3ec92cfb63b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Espressif Systems"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "63a7c1d6-ff93-454a-8872-1a6feb2c97ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "ESP32-S3-WROOM-1U-N16R8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbf58b5c-5e0c-465f-8307-71f33e465da2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d2155090-dc7d-4632-af7a-79cf0b9d5dc2")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -10 -8.4)
			(end -10 -8.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd2019cf-c743-4400-bcd4-e3294b310519")
		)
		(fp_line
			(start -9.9 -8.4)
			(end -9.9 -8.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea31b5fd-ac3c-4d25-9957-02be950e9803")
		)
		(fp_line
			(start -9 -9.6)
			(end 9 -9.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36ee1283-05c9-48d0-8650-d7dcd9082341")
		)
		(fp_arc
			(start -10 -8.4)
			(mid -9.95 -8.45)
			(end -9.9 -8.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd960065-796e-4688-afc8-e1655089ef51")
		)
		(fp_arc
			(start -9.9 -8.4)
			(mid -9.95 -8.35)
			(end -10 -8.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5183e0f-741e-43ac-80dc-30f08e071eea")
		)
		(fp_line
			(start -10.5 -10.6)
			(end 10.5 -10.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b32c94d9-db09-45e9-a70d-ffb0402500c4")
		)
		(fp_line
			(start -10.5 11.1)
			(end -10.5 -10.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0739525d-356e-40e4-8323-a9bd6f67a2b7")
		)
		(fp_line
			(start 10.5 -10.6)
			(end 10.5 11.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03f80997-0840-447b-ac24-d87943233b4f")
		)
		(fp_line
			(start 10.5 11.1)
			(end -10.5 11.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b3964c5-0b28-4ffd-b5d7-51aae4de651c")
		)
		(fp_line
			(start -9 -9.6)
			(end 9 -9.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1aecccae-0800-47a7-82b6-d782bc5b3f66")
		)
		(fp_line
			(start -9 9.6)
			(end -9 -9.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df8885d2-4a91-4768-bbc0-d01250373337")
		)
		(fp_line
			(start 9 -9.6)
			(end 9 9.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "105b7d44-ef14-41b2-b883-ebc917eefa56")
		)
		(fp_line
			(start 9 9.6)
			(end -9 9.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6f84bd0-d0d4-423e-ac93-8e8ad4aa07fe")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0.25 0)
			(layer "F.Fab")
			(uuid "adce6b63-906d-4892-ab84-313c25af83c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -8.75 -8.41 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "b193af16-6611-4022-ada6-d90741cc8f8b")
		)
		(pad "2" smd rect
			(at -8.75 -7.14 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "3.3V")
			(pinfunction "3V3")
			(pintype "passive")
			(uuid "793a9294-7b3d-4394-97ad-dd2cc1f4ca3f")
		)
		(pad "3" smd rect
			(at -8.75 -5.87 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "EN")
			(pinfunction "EN")
			(pintype "passive")
			(uuid "7ce0cb09-1b13-4d1a-bdde-643cb7172902")
		)
		(pad "4" smd rect
			(at -8.75 -4.6 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "OUT4")
			(pinfunction "IO4")
			(pintype "passive")
			(uuid "4950ad13-513f-4ee5-915a-c62b8546b443")
		)
		(pad "5" smd rect
			(at -8.75 -3.33 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "OUT5")
			(pinfunction "IO5")
			(pintype "passive")
			(uuid "5ec9ae19-5f7d-4750-a0c0-18411fff4c38")
		)
		(pad "6" smd rect
			(at -8.75 -2.06 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "OUT6")
			(pinfunction "IO6")
			(pintype "passive")
			(uuid "d40e8c3d-ee11-4577-8dcd-9298371cb8d5")
		)
		(pad "7" smd rect
			(at -8.75 -0.79 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "OUT7")
			(pinfunction "IO7")
			(pintype "passive")
			(uuid "ff866e68-c10b-48f9-85ba-f819b3148ad7")
		)
		(pad "8" smd rect
			(at -8.75 0.48 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "IN15")
			(pinfunction "IO15")
			(pintype "passive")
			(uuid "fe3cb873-4674-4bb4-aec3-9e6d32651bee")
		)
		(pad "9" smd rect
			(at -8.75 1.75 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "IN16")
			(pinfunction "IO16")
			(pintype "passive")
			(uuid "7404ae10-d7b9-431d-86f0-d82f978958a1")
		)
		(pad "10" smd rect
			(at -8.75 3.02 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "CAN Tx")
			(pinfunction "IO17")
			(pintype "passive")
			(uuid "6ebcfa81-2617-4ad7-bef0-eb81315d99f6")
		)
		(pad "11" smd rect
			(at -8.75 4.29 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "CAN Rx")
			(pinfunction "IO18")
			(pintype "passive")
			(uuid "2c2676dd-46a0-4f25-a917-e55567b4a6aa")
		)
		(pad "12" smd rect
			(at -8.75 5.56 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "OUT8")
			(pinfunction "IO8")
			(pintype "passive")
			(uuid "afce9f6c-d741-48d5-a7ff-a0510cf821e2")
		)
		(pad "13" smd rect
			(at -8.75 6.83 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "D-")
			(pinfunction "IO19")
			(pintype "passive")
			(uuid "2005b381-e169-42b4-bc8b-b8f33c7fdce8")
		)
		(pad "14" smd rect
			(at -8.75 8.1 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "D+")
			(pinfunction "IO20")
			(pintype "passive")
			(uuid "e0968aeb-e127-4ff9-ab36-c79e69a16e7c")
		)
		(pad "15" smd rect
			(at -6.985 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "OUT3")
			(pinfunction "IO3")
			(pintype "passive")
			(uuid "07561ed3-0999-42bb-bda9-2c0f74a5cfda")
		)
		(pad "16" smd rect
			(at -5.715 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "IN3")
			(pinfunction "IO46")
			(pintype "passive")
			(uuid "92741c95-f4e2-486b-93f5-1aa220bfd540")
		)
		(pad "17" smd rect
			(at -4.445 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "IN9")
			(pinfunction "IO9")
			(pintype "passive")
			(uuid "a233e7ad-129e-4287-b9d9-c2d1b5412fb3")
		)
		(pad "18" smd rect
			(at -3.175 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "IN10")
			(pinfunction "IO10")
			(pintype "passive")
			(uuid "28f21bdb-a3ad-4148-8e96-1b17f1e284a0")
		)
		(pad "19" smd rect
			(at -1.905 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "IN11")
			(pinfunction "IO11")
			(pintype "passive")
			(uuid "8a1874d7-1351-4c01-822a-60b87268e98a")
		)
		(pad "20" smd rect
			(at -0.635 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "IN12")
			(pinfunction "IO12")
			(pintype "passive")
			(uuid "a85241cd-af15-40bb-a9b0-9d43cf1f8040")
		)
		(pad "21" smd rect
			(at 0.635 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "IN13")
			(pinfunction "IO13")
			(pintype "passive")
			(uuid "7c6f2a2d-91d5-4007-a165-f77fbe612961")
		)
		(pad "22" smd rect
			(at 1.905 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "IN14")
			(pinfunction "IO14")
			(pintype "passive")
			(uuid "fa205cb9-af80-4032-9233-453356b9657a")
		)
		(pad "23" smd rect
			(at 3.175 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "IN6")
			(pinfunction "IO21")
			(pintype "passive")
			(uuid "8cfcd88c-0df5-4de1-a6e7-b593c37c443c")
		)
		(pad "24" smd rect
			(at 4.445 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "IN2")
			(pinfunction "IO47")
			(pintype "passive")
			(uuid "c383c275-d5b6-401b-96b1-0ba302d2bd0d")
		)
		(pad "25" smd rect
			(at 5.715 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "IN1")
			(pinfunction "IO48")
			(pintype "passive")
			(uuid "cbbae90f-ee80-474d-a69e-69f596fbd148")
		)
		(pad "26" smd rect
			(at 6.985 9.35)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "IN4")
			(pinfunction "IO45")
			(pintype "passive")
			(uuid "09c2c99a-86a4-4630-8a75-eb6e4c1e3b5c")
		)
		(pad "27" smd rect
			(at 8.75 8.1 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "GPIO0")
			(pinfunction "IO0")
			(pintype "passive")
			(uuid "b8b93c0d-568f-4978-af7e-9c11713a8648")
		)
		(pad "28" smd rect
			(at 8.75 6.83 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(IC3-IO35-Pad28)")
			(pinfunction "IO35")
			(pintype "passive+no_connect")
			(uuid "127e9dfa-64e1-4167-b1eb-0b3fbbc760ff")
		)
		(pad "29" smd rect
			(at 8.75 5.56 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(IC3-IO36-Pad29)")
			(pinfunction "IO36")
			(pintype "passive+no_connect")
			(uuid "8c3da133-1028-42d0-ba0d-70111d25aec2")
		)
		(pad "30" smd rect
			(at 8.75 4.29 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "/PSRAM")
			(pinfunction "IO37")
			(pintype "passive+no_connect")
			(uuid "8dff2114-1cc1-4775-9904-3ef5b218de19")
		)
		(pad "31" smd rect
			(at 8.75 3.02 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "IN5")
			(pinfunction "IO38")
			(pintype "passive")
			(uuid "89330d65-005f-44ce-9830-7c2eea7d6196")
		)
		(pad "32" smd rect
			(at 8.75 1.75 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "TCK")
			(pinfunction "IO39")
			(pintype "passive")
			(uuid "0969f64d-3de2-4d43-b07f-f8f057cc29a6")
		)
		(pad "33" smd rect
			(at 8.75 0.48 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "TDO")
			(pinfunction "IO40")
			(pintype "passive")
			(uuid "180fad00-0e3b-4296-b2b0-11e44f37aa33")
		)
		(pad "34" smd rect
			(at 8.75 -0.79 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "TDI")
			(pinfunction "IO41")
			(pintype "passive")
			(uuid "bede1fee-4fce-470b-ab83-798c52100ccb")
		)
		(pad "35" smd rect
			(at 8.75 -2.06 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "TMS")
			(pinfunction "IO42")
			(pintype "passive")
			(uuid "d3b906ae-9aba-4845-bc4c-aa319746ffac")
		)
		(pad "36" smd rect
			(at 8.75 -3.33 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "RXD0")
			(pinfunction "RXD0")
			(pintype "passive")
			(uuid "2948ffe8-9918-48f2-9032-ebf3925d7795")
		)
		(pad "37" smd rect
			(at 8.75 -4.6 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "TXD0")
			(pinfunction "TXD0")
			(pintype "passive")
			(uuid "1c57626f-3a22-46d1-a198-bbd0bd3ef51e")
		)
		(pad "38" smd rect
			(at 8.75 -5.87 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "OUT2")
			(pinfunction "IO2")
			(pintype "passive")
			(uuid "9edf9823-e6c9-4fc6-bc70-19e5564183a3")
		)
		(pad "39" smd rect
			(at 8.75 -7.14 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "OUT1")
			(pinfunction "IO1")
			(pintype "passive")
			(uuid "81fd308b-5bce-457e-895b-19f8d1f2ada1")
		)
		(pad "40" smd rect
			(at 8.75 -8.41 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
			(uuid "29332397-a11f-4df0-a15b-f2dc82eb77e1")
		)
		(pad "41" smd rect
			(at -1.5 -0.69)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
			(uuid "d4c5c3df-5bc7-418b-b2a6-a8547ac2dfd0")
		)
		(pad "42" smd rect
			(at -1.5 -2.09)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
			(uuid "cf5eb543-e876-47b7-a38b-3cf49d89ba7d")
		)
		(pad "43" smd rect
			(at -2.9 -2.09)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
			(uuid "afbfe0da-b4e5-4451-9fac-be0be787c73d")
		)
		(pad "44" smd rect
			(at -2.9 -0.69)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_6")
			(pintype "passive")
			(uuid "4eff160a-7bf3-481e-9d03-60d6e7682aa3")
		)
		(pad "45" smd rect
			(at -2.9 0.71)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_7")
			(pintype "passive")
			(uuid "bb73a18a-52c3-4f16-8832-4100d3b92ae8")
		)
		(pad "46" smd rect
			(at -1.5 0.71)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_8")
			(pintype "passive")
			(uuid "cfff04d6-31dd-4e79-83ab-88b861e0a29b")
		)
		(pad "47" smd rect
			(at -0.1 0.71)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_9")
			(pintype "passive")
			(uuid "4b4eed35-cb83-4d16-b2e8-e2266cfc9940")
		)
		(pad "48" smd rect
			(at -0.1 -0.69)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_10")
			(pintype "passive")
			(uuid "5ee551fc-bacf-49a0-80b5-462cfcf32cc2")
		)
		(pad "49" smd rect
			(at -0.1 -2.09)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND_11")
			(pintype "passive")
			(uuid "aaa435a1-dea7-4b45-8be6-54a296b13b71")
		)
		(embedded_fonts no)
		(model "ESP32-S3-WROOM-1U-N16R8.stp"
			(offset
				(xyz 0 -0.2499999962 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "feb7e2dd-be73-4f93-b179-c7340947cc3c")
		(at 148.765 94)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "44db6830-ac8e-4c7d-a227-c9cf913f66df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "77a8530f-9dd9-493d-a2b8-f0e2ff6f63e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc52b24f-be3d-4910-8a4f-4d640e43f243")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ca97d4f-301c-479b-bd82-59e1812911ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "10fc919f-797a-434e-9110-5092502882be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/813dbf6b-055d-45b2-9b63-46ec956bef0c")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fef5cc3c-0a1e-4c69-b16a-db790e9d64cd")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea02f9f5-cfee-49fe-8390-cda1215cc52d")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9dee8fe-5aed-4a8e-a750-8b5a0ebb07d0")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "571e59c7-783f-4799-8792-c8cbc7233fa2")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7bd9ac3-2985-46ed-8d29-da35a8d62eda")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ef3a8f8-8e2a-4e25-bcdf-7c6c6cca1daa")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4574d410-4048-480c-a044-5507ce43a60c")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f7d8b32-4650-4dc0-9f81-4722c010c651")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ac15373-b62d-4f3a-8e8b-9e61f42ce636")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09fde127-2cb9-44e0-b8da-76a7f1b29273")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "772b72e3-89aa-4a94-9f95-dfa4a232d440")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f833b1cf-6f28-4930-857e-606d794867a1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f3d14df-a78b-4f83-9372-28354c0805a7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "24V GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "9fa8b540-4b0e-4b59-a836-fc1017063e2e")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 48 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8f32733a-c32c-493b-82f5-6155a2c431ec")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ffeb9ebb-43ae-4a5e-acea-24fa852c3a03")
		(at 153.54 96.935)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C_I20"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "4dd61d29-3059-46e1-a8d3-4ebf60331468")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "8d037ab9-552d-43bd-9d76-413907607e91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "51ab9ba2-21e8-4efa-b31b-1a1bf9f6a596")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "704807e0-8290-425d-af90-5f55df6d6d89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/481e6807-80be-4c05-a2e3-e1d4fc932b8d/eaa17ae1-2d85-49e9-adc3-def370e08eb5")
		(sheetname "/PLC2 GPI2/")
		(sheetfile "PLC2 GPI2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09de5f4f-e7f4-4e3d-afe8-5041f2d347b9")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c71f33b-8858-4d0c-b286-d2a4a485bd89")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3fb2cd6-7148-486c-95f2-734940bcdfd8")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "31f08ffe-f50a-45b1-895d-1ffaa82b1676")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d51de5d4-7cac-4f5a-8e0c-9d397b35f9bd")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fccabf1-b4af-470f-81a8-407a1f1220eb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "545afca6-76dc-4fc2-91aa-62680dea0364")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d64c2ba5-a57e-4f7f-aa8d-8ce0e0c4df8b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e7e769a-f77a-4007-b35f-60fc8998439d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e66a33fc-1fbf-407a-b0e8-1cdb75e31acc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9e0295dc-63c7-4376-b9c3-083567dbcf65")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 25 "Net-(D_I12-K)")
			(pintype "passive")
			(uuid "1df7e008-fcfc-4352-94a4-dbeb0dfff017")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "24V GND")
			(pintype "passive")
			(uuid "dc75a39e-8c9c-44de-8c31-77dab7037c52")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ffed3353-81fe-4d6b-8b24-353e29cc5d1d")
		(at -11.4625 100.06)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "19d8bc01-082e-4b04-8f21-125a07fc4b0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "909d32f0-7ecc-4c7e-be34-32d01cc7e74f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "76efc6da-ab21-455b-87b1-f8c6096a88a5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3dc4d33c-6796-4aa0-bc3d-b8ff08fe90fd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7bc4f572-5bfd-4ab8-8c9f-319c0c83b405")
		(sheetname "/")
		(sheetfile "projekt2.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c4919f6-e7fa-49d1-a29b-eccd37287113")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33cb36c1-05cd-4bae-90d6-5abccd525191")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "62bb4da7-a24c-4f77-a734-867d2f7ca551")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c9ed2be-5848-471d-afb7-2497ca45e5ae")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "614c0040-8716-4daf-8ae5-518537a56a1d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3c727f4-ecbd-4c6d-b0e8-7e6017fd32dc")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8928f05c-3c84-44a6-9b1f-cf90c0bc3f74")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58b9f996-3955-42a7-8839-d2f1a018d2c8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbc1bea1-26f3-42ad-bdbc-db9b72074211")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a209625-9ffe-41f4-bfac-61e45a262d0e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9fdab40d-cd01-4b33-9b09-90bba879dbb4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "89ea8e76-b8b6-4391-94f8-3aa81778f91a")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "EN")
			(pintype "passive")
			(uuid "89594108-2d61-4b56-97cb-3b1358d074ad")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.stpZ"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 142.5 53.5)
		(end 252.5 143.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "10ce2022-93bd-4cd6-85e1-47a10679bbca")
	)
	(embedded_fonts no)
)
