FILE_TYPE = MULTI_PHYS_TABLE;

PART 'ESP32_WROOM_32E_N8'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Espressif Systems", "ESP32-WROOM-32E-N8" (!) = "", "ESP32WROOM32EN8", "Other", "356-ESP32WRM32E164PH", "https://www.mouser.co.uk/ProductDetail/Espressif-Systems/ESP32-WROOM-32E-N8?qs=Li%252BoUPsLEnsLnZW%252BGLgUhw%3D%3D", "WiFi Modules - 802.11 SMD Module ESP32-WROOM-32E, ESP32-D0WD-V3, 8 MB SPI flash, PCB antenna", "https://www.google.com/url?sa=t&rct=j&q=&esrc=s&source=web&cd=&ved=2ahUKEwjLw4ysybv2AhXFzIUKHZUbB64QFnoECCwQAQ&url=https%3A%2F%2Fwww.espressif.com%2Fsites%2Fdefault%2Ffiles%2Fdocumentation%2Fesp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf&usg=AOvVaw1xSL", "3.25 mm"
END_PART

END.
