(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(uuid "bbf1e387-9542-4fed-9089-3295a4f03dd5")
	(paper "A4")
	(title_block
		(title "esp32d0wd_v3")
		(date "2026-02-23")
	)
	(lib_symbols
		(symbol "ESP32-WROOM-32E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -12.7 34.29 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "ESP32-WROOM-32E"
				(at 1.27 34.29 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "RF_Module:ESP32-WROOM-32D"
				(at 16.51 -34.29 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "RF Module, ESP32-D0WD-V3 SoC, without PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "ESP32?WROOM?32D*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "ESP32-WROOM-32E_0_1"
				(rectangle
					(start -12.7 33.02)
					(end 12.7 -33.02)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "ESP32-WROOM-32E_1_1"
				(pin input line
					(at -15.24 30.48 0)
					(length 2.54)
					(name "EN"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -15.24 25.4 0)
					(length 2.54)
					(name "SENSOR_VP"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -15.24 22.86 0)
					(length 2.54)
					(name "SENSOR_VN"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 0 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "21"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "22"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "17"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "18"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "20"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "19"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect line
					(at -12.7 -27.94 0)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "32"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 35.56 270)
					(length 2.54)
					(name "VDD"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -35.56 90)
					(length 2.54)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -35.56 90)
					(length 2.54)
					(hide yes)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -35.56 90)
					(length 2.54)
					(hide yes)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "38"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -35.56 90)
					(length 2.54)
					(hide yes)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "39"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 30.48 180)
					(length 2.54)
					(name "IO0"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "25"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 27.94 180)
					(length 2.54)
					(name "TXD0/IO1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "35"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 25.4 180)
					(length 2.54)
					(name "IO2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "24"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 22.86 180)
					(length 2.54)
					(name "RXD0/IO3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "34"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 20.32 180)
					(length 2.54)
					(name "IO4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "26"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 17.78 180)
					(length 2.54)
					(name "IO5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "29"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 15.24 180)
					(length 2.54)
					(name "IO12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 12.7 180)
					(length 2.54)
					(name "IO13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "16"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 10.16 180)
					(length 2.54)
					(name "IO14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 2.54)
					(name "IO15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "23"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 5.08 180)
					(length 2.54)
					(name "IO16"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "27"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 2.54)
					(name "IO17"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "28"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 2.54)
					(name "IO18"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "30"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "IO19"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "31"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "IO21"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "33"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "IO22"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "36"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "IO23"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "37"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -12.7 180)
					(length 2.54)
					(name "IO25"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "IO26"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -17.78 180)
					(length 2.54)
					(name "IO27"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -20.32 180)
					(length 2.54)
					(name "IO32"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 15.24 -22.86 180)
					(length 2.54)
					(name "IO33"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at 15.24 -25.4 180)
					(length 2.54)
					(name "IO34"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at 15.24 -27.94 180)
					(length 2.54)
					(name "IO35"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
	)
	(symbol
		(lib_id "ESP32-WROOM-32E")
		(at 143.51 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "2a1fd477-6dd2-4809-819b-0ec8e1ff776d")
		(property "Reference" "U1"
			(at 143.51 91.44 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "ESP32-WROOM-32E"
			(at 143.51 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "RF_Module:ESP32-WROOM-32D"
			(at 143.51 91.44 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 143.51 91.44 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "ESP32-D0WD-V3 module"
			(at 143.51 91.44 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "3"
			(uuid "1baf1be8-95f1-41ba-90be-c5e2f27dc94e")
		)
		(pin "4"
			(uuid "4ae14719-60b1-47e8-96a3-08f2c8ef6e88")
		)
		(pin "5"
			(uuid "d0d20612-5671-4f6e-8ee2-76bb852b4d9f")
		)
		(pin "21"
			(uuid "96989053-a6b8-4d08-9d42-10c5ad057ae9")
		)
		(pin "22"
			(uuid "410ee7f4-642e-4afa-af83-a936e3518a9d")
		)
		(pin "17"
			(uuid "512f2b5a-d332-478f-baef-0d5ac524f959")
		)
		(pin "18"
			(uuid "883c4881-c9a5-4c04-93d6-3515cd16dba0")
		)
		(pin "20"
			(uuid "7531c6c4-e661-440a-85e6-f19616b80655")
		)
		(pin "19"
			(uuid "31296b1c-ed8d-4b02-b745-c0766a46db51")
		)
		(pin "32"
			(uuid "07cd8385-1038-45ea-8c33-36f9a8f3e95a")
		)
		(pin "2"
			(uuid "cd016e59-5e1c-4988-8660-565fc1f6bfd8")
		)
		(pin "1"
			(uuid "d5909793-55a2-45f2-a7b4-419fbbea7a20")
		)
		(pin "15"
			(uuid "468e37d7-bae3-4335-b8fd-cbd630f89226")
		)
		(pin "38"
			(uuid "a46c25d2-930f-4871-bc64-ff208da40fcd")
		)
		(pin "39"
			(uuid "7b7cc753-c98c-4d42-9d91-3c7ecd3c94c0")
		)
		(pin "25"
			(uuid "7c65781b-684f-4d72-a783-c958dd560851")
		)
		(pin "35"
			(uuid "1aa973ce-3a67-4a4f-882e-7a06533f9df8")
		)
		(pin "24"
			(uuid "9f4068be-ca71-4b5c-9ffa-2600555cd636")
		)
		(pin "34"
			(uuid "8a979c64-172b-41b0-8f55-c450764b34f7")
		)
		(pin "26"
			(uuid "19002913-8212-4c4d-bca1-b45f055efba1")
		)
		(pin "29"
			(uuid "9df730a6-8b69-4626-8f1f-066d252d9a49")
		)
		(pin "14"
			(uuid "edeb56d9-c3e2-4840-8bff-12e00c44ac09")
		)
		(pin "16"
			(uuid "c1fb754a-7b4f-4b70-891c-f64898dbc0c8")
		)
		(pin "13"
			(uuid "bd914d6a-7dd1-40cd-80aa-ec8851ec4bc5")
		)
		(pin "23"
			(uuid "31cc8bce-d3a1-48db-b097-9e8da2abcfa8")
		)
		(pin "27"
			(uuid "1b1e2545-1929-4003-81aa-ff52d6cd5475")
		)
		(pin "28"
			(uuid "2385d6fc-4a7e-444a-aece-4c5a6fa262d6")
		)
		(pin "30"
			(uuid "bf0bf5b3-62e9-49de-820d-82256681db83")
		)
		(pin "31"
			(uuid "22f47a9f-9a6f-436e-b42b-9bc640491a5a")
		)
		(pin "33"
			(uuid "3ba8f336-f59c-484b-805a-c625f2bc3fcd")
		)
		(pin "36"
			(uuid "945e9a16-db02-4974-8213-c35614809d2d")
		)
		(pin "37"
			(uuid "1dfa280f-16af-4054-8235-936ef72d6b26")
		)
		(pin "10"
			(uuid "2c8e008b-6729-4f29-8489-64972f8df21c")
		)
		(pin "11"
			(uuid "97fa69e9-4d42-4a31-99e3-4c83e4e981a6")
		)
		(pin "12"
			(uuid "9216c946-0da2-4b3a-a2ac-18b2130ccab5")
		)
		(pin "8"
			(uuid "c6d0dd6d-cfff-465f-8796-0211063c5c1b")
		)
		(pin "9"
			(uuid "d7bc8b76-0356-472d-8de1-5f16a32a95ba")
		)
		(pin "6"
			(uuid "72f07658-1d2b-4d92-91f1-6b540eca99d6")
		)
		(pin "7"
			(uuid "ed8aed9f-8c89-4003-b6f7-a3696dc16f1e")
		)
		(instances
			(project "esp32d0wd_v3"
				(path "/bbf1e387-9542-4fed-9089-3295a4f03dd5"
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path "/"
			(page "1")
		)
	)
	(embedded_fonts no)
)
