(footprint "Relay_AmericanZettler_AZ943-1CH"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5a781128-1672-488a-9fa6-2bd3533b7c66")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Relay_AmericanZettler_AZ943-1CH"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cbee3265-8b63-4342-b158-7b9571e1c36a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "481b8cf4-834b-43b6-9a5d-14352fbd30ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f4a78de9-1ddd-40ff-812c-71a9dccb9538")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.5 -7.4)
		(end 3.5 -7.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a9b72ecc-9534-4cd1-97d2-01a39bf4de59")
	)
	(fp_line
		(start -3.5 7.4)
		(end 3.5 7.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4ebe22b3-45bc-4fdb-9a4f-0461f3a3eb50")
	)
	(fp_line
		(start 9.2 -3.5)
		(end 9.2 3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "80c4e933-f8e1-4416-a4d4-4e0a94b869ff")
	)
	(fp_rect
		(start -9.75 -7.9)
		(end 9.75 7.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "32a1cd56-1748-4e40-8d53-3fe80b757050")
	)
	(fp_rect
		(start -9.5 -7.65)
		(end 9.5 7.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "e6aad73a-0ce7-4cef-a4b0-640c81b02c47")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "75eab95d-b5e5-42ad-8ae1-ec64dcc6b2bd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "11" thru_hole circle
		(at -8.1 -0.16)
		(size 2.7 2.7)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c2227ba8-6a5b-462c-b514-6a88c223cb7a")
	)
	(pad "12" thru_hole circle
		(at -6.1 -6.16)
		(size 2.7 2.7)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "872cefb0-cdda-46e7-84a0-f7a7684aecf6")
	)
	(pad "14" thru_hole circle
		(at -6.1 5.84)
		(size 2.7 2.7)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d46e7ac-0e96-4475-96cb-e80572fa7aea")
	)
	(pad "A1" thru_hole rect
		(at 6.1 -6.16)
		(size 2.7 2.4)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5bcb0cd7-94f3-4a87-b5ea-48e82c7ef4c1")
	)
	(pad "A2" thru_hole circle
		(at 6.1 5.84)
		(size 2.7 2.7)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4e359a84-af6a-4d32-b085-49f0ba8d1f80")
	)
	(embedded_fonts no)
)
