(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "TBD62083AFWG,EL" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 26.67 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "TBD62083AFWG,EL" (at 26.67 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOIC127P1032X285-18N" (at 26.67 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "" (at 26.67 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Gate Drivers DMOS Transistor Array 8-CH, 50V/0.5A" (at 26.67 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "2.85" (at 26.67 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "757-TBD62083AFWGEL" (at 26.67 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TBD62083AFWGEL?qs=fSnNYG2PaKJPpDBB6xK1QA%3D%3D" (at 26.67 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Toshiba" (at 26.67 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "TBD62083AFWG,EL" (at 26.67 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 25.4 -22.86)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "I1" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "I2" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "I3" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "I4" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "I5" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "I6" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "I7" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "I8" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -20.32 0) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 0 180) (length 5.08)
      (name "O1" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -2.54 180) (length 5.08)
      (name "O2" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -5.08 180) (length 5.08)
      (name "O3" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -7.62 180) (length 5.08)
      (name "O4" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -10.16 180) (length 5.08)
      (name "O5" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -12.7 180) (length 5.08)
      (name "O6" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -15.24 180) (length 5.08)
      (name "O7" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -17.78 180) (length 5.08)
      (name "O8" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -20.32 180) (length 5.08)
      (name "COMMON" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
  )
)
